From 051ca74ff3462463e5e49a509cbf42552f8c3d41 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Fri, 20 Sep 2024 16:16:02 +0100
Subject: [PATCH] Input: sensehat-joystick : Revert to downstream keymap

Upstream chose to use BTN_DPAD_* and BTN_SELECT, whilst downstream
had used KEY_*.

Revert to the downstream map to avoid any regressions.
(Ideally this would be read from DT)

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/input/joystick/sensehat-joystick.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/input/joystick/sensehat-joystick.c
+++ b/drivers/input/joystick/sensehat-joystick.c
@@ -28,7 +28,7 @@ struct sensehat_joystick {
 };
 
 static const unsigned int keymap[] = {
-	BTN_DPAD_DOWN, BTN_DPAD_RIGHT, BTN_DPAD_UP, BTN_SELECT, BTN_DPAD_LEFT,
+	KEY_DOWN, KEY_RIGHT, KEY_UP, KEY_ENTER, KEY_LEFT
 };
 
 static irqreturn_t sensehat_joystick_report(int irq, void *cookie)
