From 5de52f2adb6518a146cc87c41786e7bb726429d7 Mon Sep 17 00:00:00 2001
From: Nicolai Buchwitz <nb@tipi-net.de>
Date: Thu, 19 Feb 2026 16:18:22 +0100
Subject: [PATCH] overlays: README: add Pi4 and CM4 to eee dtparam description

The eee dtparam is also available on Pi4 and CM4 via the
__overrides__ in bcm2711-rpi-ds.dtsi. Update the description
accordingly.

Signed-off-by: Nicolai Buchwitz <nb@tipi-net.de>
---
 arch/arm/boot/dts/overlays/README | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -234,7 +234,7 @@ Params:
 
         eee                     Enable Energy Efficient Ethernet support for
                                 compatible devices (default "on"). See also
-                                "tx_lpi_timer". Pi3B+ only.
+                                "tx_lpi_timer". Pi3B+, Pi4 and CM4 only.
 
         enable_eeprom           Set to "on" to enable the onboard bootloader
                                 EEPROM by driving GPIO 57 low
