From 6751906070b6708ede20d896be7d62e19be6ef63 Mon Sep 17 00:00:00 2001
From: Robert Marko <robert.marko@sartura.hr>
Date: Thu, 25 Sep 2025 22:26:58 +0200
Subject: [PATCH 123/124] arm64: dts: microchip: lan969x: add SDMMC nodes

Add nodes for both SDMMC controllers.

Signed-off-by: Robert Marko <robert.marko@sartura.hr>
---
 arch/arm64/boot/dts/microchip/lan9691.dtsi | 22 ++++++++++++++++++++++
 1 file changed, 22 insertions(+)

--- a/arch/arm64/boot/dts/microchip/lan9691.dtsi
+++ b/arch/arm64/boot/dts/microchip/lan9691.dtsi
@@ -411,6 +411,28 @@
 			status = "disabled";
 		};
 
+		sdmmc0: mmc@e0830000 {
+			compatible = "microchip,lan9691-sdhci";
+			reg = <0xe0830000 0x00000300>;
+			interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clks GCK_ID_SDMMC0>, <&clks GCK_ID_SDMMC0>;
+			clock-names = "hclock", "multclk";
+			assigned-clocks = <&clks GCK_ID_SDMMC0>;
+			assigned-clock-rates = <100000000>;
+			status = "disabled";
+		};
+
+		sdmmc1: mmc@e0838000 {
+			compatible = "microchip,lan9691-sdhci";
+			reg = <0xe0838000 0x00000300>;
+			interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clks GCK_ID_SDMMC1>, <&clks GCK_ID_SDMMC1>;
+			clock-names = "hclock", "multclk";
+			assigned-clocks = <&clks GCK_ID_SDMMC1>;
+			assigned-clock-rates = <45000000>;
+			status = "disabled";
+		};
+
 		qspi2: spi@e0834000 {
 			compatible = "microchip,lan9691-qspi";
 			reg = <0xe0834000 0x00000100>,
