From 20959cefc27e7e2e506b4e789b728e5702c77f95 Mon Sep 17 00:00:00 2001
From: George Moussalem <george.moussalem@outlook.com>
Date: Mon, 8 Jun 2026 09:09:18 +0400
Subject: arm64: qcom: ipq5018: Add GEPHY RX and TX clocks

Add RX and TX clocks for the IPQ5018 GEPHY to enable the datapath.

Fixes: f5f2b835e316 ("arm64: dts: qcom: ipq5018: Add GE PHY to internal mdio bus")
Reviewed-by: Dmitry Baryshkov <dmitry.baryshkov@oss.qualcomm.com>
Signed-off-by: George Moussalem <george.moussalem@outlook.com>
Link: https://lore.kernel.org/r/20260608-ipq5018-gephy-clocks-v4-3-fb2ccd56894b@outlook.com
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
---
 arch/arm64/boot/dts/qcom/ipq5018.dtsi | 3 +++
 1 file changed, 3 insertions(+)

(limited to 'arch/arm64/boot/dts/qcom/ipq5018.dtsi')

--- a/arch/arm64/boot/dts/qcom/ipq5018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq5018.dtsi
@@ -229,6 +229,9 @@
 				compatible = "ethernet-phy-id004d.d0c0";
 				reg = <7>;
 
+				clocks = <&gcc GCC_GEPHY_RX_CLK>,
+					 <&gcc GCC_GEPHY_TX_CLK>;
+				clock-names = "rx", "tx";
 				resets = <&gcc GCC_GEPHY_MISC_ARES>;
 			};
 		};
