From 8da57800caa33f42690cc1c7f3dbf2e580289348 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Thu, 12 Nov 2020 17:01:52 +0000
Subject: [PATCH] dt-bindings: Add compatible for BCM2711 DSI1

DSI1 on BCM2711 doesn't require the DMA workaround that is used
on BCM2835/6/7, therefore it needs a new compatible string.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 Documentation/devicetree/bindings/display/brcm,bcm2835-dsi0.yaml | 1 +
 1 file changed, 1 insertion(+)

--- a/Documentation/devicetree/bindings/display/brcm,bcm2835-dsi0.yaml
+++ b/Documentation/devicetree/bindings/display/brcm,bcm2835-dsi0.yaml
@@ -21,6 +21,7 @@ properties:
       - brcm,bcm2711-dsi1
       - brcm,bcm2835-dsi0
       - brcm,bcm2835-dsi1
+      - brcm,bcm2711-dsi1
 
   reg:
     maxItems: 1
