From 3b4329230db8750bea7a56ef07f07cbbf5fc6c5a Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Tue, 4 Jul 2023 22:50:12 +0200
Subject: [PATCH 19/20] net: dsa: qca8k: implement lag_fdb_add/del ops

Implement lag_fdb_add/del ops to correctly support using LAG interface.
Qca8k switch supports declaring fdb entry for link aggregation by simply
setting the DES_PORT bits to all the LAG member.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/net/dsa/qca/qca8k-8xxx.c   |  2 ++
 drivers/net/dsa/qca/qca8k-common.c | 48 ++++++++++++++++++++++++++++++
 drivers/net/dsa/qca/qca8k.h        |  6 ++++
 3 files changed, 56 insertions(+)

--- a/drivers/net/dsa/qca/qca8k-8xxx.c
+++ b/drivers/net/dsa/qca/qca8k-8xxx.c
@@ -2040,6 +2040,8 @@ static const struct dsa_switch_ops qca8k
 	.port_fdb_add		= qca8k_port_fdb_add,
 	.port_fdb_del		= qca8k_port_fdb_del,
 	.port_fdb_dump		= qca8k_port_fdb_dump,
+	.lag_fdb_add		= qca8k_lag_fdb_add,
+	.lag_fdb_del		= qca8k_lag_fdb_del,
 	.port_mdb_add		= qca8k_port_mdb_add,
 	.port_mdb_del		= qca8k_port_mdb_del,
 	.port_mirror_add	= qca8k_port_mirror_add,
--- a/drivers/net/dsa/qca/qca8k-common.c
+++ b/drivers/net/dsa/qca/qca8k-common.c
@@ -1227,6 +1227,42 @@ int qca8k_port_lag_leave(struct dsa_swit
 	return qca8k_lag_refresh_portmap(ds, port, lag, true);
 }
 
+int qca8k_lag_fdb_add(struct dsa_switch *ds, struct dsa_lag lag,
+		      const unsigned char *addr, u16 vid,
+		      struct dsa_db db)
+{
+	struct qca8k_priv *priv = (struct qca8k_priv *)ds->priv;
+	struct dsa_port *dp;
+	u16 port_mask = 0;
+
+	/* Set the vid to the port vlan id if no vid is set */
+	if (!vid)
+		vid = QCA8K_PORT_VID_DEF;
+
+	dsa_lag_foreach_port(dp, ds->dst, &lag)
+		port_mask |= BIT(dp->index);
+
+	return qca8k_port_fdb_insert(priv, addr, port_mask, vid);
+}
+
+int qca8k_lag_fdb_del(struct dsa_switch *ds, struct dsa_lag lag,
+		      const unsigned char *addr, u16 vid,
+		      struct dsa_db db)
+{
+	struct qca8k_priv *priv = (struct qca8k_priv *)ds->priv;
+	struct dsa_port *dp;
+	u16 port_mask = 0;
+
+	/* Set the vid to the port vlan id if no vid is set */
+	if (!vid)
+		vid = QCA8K_PORT_VID_DEF;
+
+	dsa_lag_foreach_port(dp, ds->dst, &lag)
+	port_mask |= BIT(dp->index);
+
+	return qca8k_fdb_del(priv, addr, port_mask, vid);
+}
+
 int qca8k_read_switch_id(struct qca8k_priv *priv)
 {
 	u32 val;
--- a/drivers/net/dsa/qca/qca8k.h
+++ b/drivers/net/dsa/qca/qca8k.h
@@ -592,5 +592,11 @@ int qca8k_port_lag_join(struct dsa_switc
 			struct netlink_ext_ack *extack);
 int qca8k_port_lag_leave(struct dsa_switch *ds, int port,
 			 struct dsa_lag lag);
+int qca8k_lag_fdb_add(struct dsa_switch *ds, struct dsa_lag lag,
+		      const unsigned char *addr, u16 vid,
+		      struct dsa_db db);
+int qca8k_lag_fdb_del(struct dsa_switch *ds, struct dsa_lag lag,
+		      const unsigned char *addr, u16 vid,
+		      struct dsa_db db);
 
 #endif /* __QCA8K_H */
