From c5d151dccce7deb62620a7b16418c0d6d6a59720 Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Mon, 17 Mar 2025 23:07:45 +0100
Subject: [PATCH 6/7] dt-bindings: net: ethernet-controller: permit to define
 multiple PCS

Drop the limitation of a single PCS in pcs-handle property. Multiple PCS
can be defined for an ethrnet-controller node to support various PHY
interface mode type.

It's very common for SoCs to have a dedicated PCS for SGMII mode and one
for USXGMII mode.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 Documentation/devicetree/bindings/net/ethernet-controller.yaml | 2 --
 1 file changed, 2 deletions(-)

--- a/Documentation/devicetree/bindings/net/ethernet-controller.yaml
+++ b/Documentation/devicetree/bindings/net/ethernet-controller.yaml
@@ -110,8 +110,6 @@ properties:
 
   pcs-handle:
     $ref: /schemas/types.yaml#/definitions/phandle-array
-    items:
-      maxItems: 1
     description:
       Specifies a reference to a node representing a PCS PHY device on a MDIO
       bus to link with an external PHY (phy-handle) if exists.
