From bbfb1983944f2eaa8ee192e0f7b59ecc0fda9981 Mon Sep 17 00:00:00 2001
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Wed, 13 May 2026 17:03:59 +0200
Subject: [PATCH] net: airoha: Reserve RX headroom to avoid skb reallocation

Reserve NET_SKB_PAD + NET_IP_ALIGN bytes of headroom for received packets
to avoid skb head reallocation when pushing protocol headers into the skb.

Tested-by: Xuegang Lu <xuegang.lu@airoha.com>
Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Link: https://patch.msgid.link/20260513-airoha-rx-headroom-v1-1-bd87798e422d@kernel.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/airoha/airoha_eth.c | 14 ++++++++------
 drivers/net/ethernet/airoha/airoha_eth.h |  2 ++
 2 files changed, 10 insertions(+), 6 deletions(-)

--- a/drivers/net/ethernet/airoha/airoha_eth.c
+++ b/drivers/net/ethernet/airoha/airoha_eth.c
@@ -543,9 +543,10 @@ static int airoha_qdma_fill_rx_queue(str
 		q->queued++;
 		nframes++;
 
+		offset += AIROHA_RX_HEADROOM;
 		e->buf = page_address(page) + offset;
 		e->dma_addr = page_pool_get_dma_addr(page) + offset;
-		e->dma_len = SKB_WITH_OVERHEAD(q->buf_size);
+		e->dma_len = SKB_WITH_OVERHEAD(AIROHA_RX_LEN(q->buf_size));
 
 		val = FIELD_PREP(QDMA_DESC_LEN_MASK, e->dma_len);
 		WRITE_ONCE(desc->ctrl, cpu_to_le32(val));
@@ -611,13 +612,12 @@ static int airoha_qdma_rx_process(struct
 		q->tail = (q->tail + 1) % q->ndesc;
 		q->queued--;
 
-		dma_sync_single_for_cpu(eth->dev, e->dma_addr,
-					SKB_WITH_OVERHEAD(q->buf_size), dir);
+		dma_sync_single_for_cpu(eth->dev, e->dma_addr, e->dma_len,
+					dir);
 
 		page = virt_to_head_page(e->buf);
 		len = FIELD_GET(QDMA_DESC_LEN_MASK, desc_ctrl);
-		data_len = q->skb ? q->buf_size
-				  : SKB_WITH_OVERHEAD(q->buf_size);
+		data_len = q->skb ? AIROHA_RX_LEN(q->buf_size) : e->dma_len;
 		if (!len || data_len < len)
 			goto free_frag;
 
@@ -627,10 +627,12 @@ static int airoha_qdma_rx_process(struct
 
 		port = eth->ports[p];
 		if (!q->skb) { /* first buffer */
-			q->skb = napi_build_skb(e->buf, q->buf_size);
+			q->skb = napi_build_skb(e->buf - AIROHA_RX_HEADROOM,
+						q->buf_size);
 			if (!q->skb)
 				goto free_frag;
 
+			skb_reserve(q->skb, AIROHA_RX_HEADROOM);
 			__skb_put(q->skb, len);
 			skb_mark_for_recycle(q->skb);
 			q->skb->dev = port->dev;
--- a/drivers/net/ethernet/airoha/airoha_eth.h
+++ b/drivers/net/ethernet/airoha/airoha_eth.h
@@ -32,6 +32,8 @@
 #define AIROHA_FE_MC_MAX_VLAN_TABLE	64
 #define AIROHA_FE_MC_MAX_VLAN_PORT	16
 #define AIROHA_NUM_TX_IRQ		2
+#define AIROHA_RX_HEADROOM		(NET_SKB_PAD + NET_IP_ALIGN)
+#define AIROHA_RX_LEN(_n)		((_n) - AIROHA_RX_HEADROOM)
 #define HW_DSCP_NUM			2048
 #define IRQ_QUEUE_LEN(_n)		((_n) ? 1024 : 2048)
 #define TX_DSCP_NUM			1024
