From 0eaf04ef4963db173428da176f52320754b0574c Mon Sep 17 00:00:00 2001
From: Hal Feng <hal.feng@starfivetech.com>
Date: Thu, 10 Oct 2024 11:05:20 +0800
Subject: [PATCH 19/55] net: stmmac: Extend waiting time of dma reset

Fix dma reset failure happening when disabling network.

Signed-off-by: Hal Feng <hal.feng@starfivetech.com>
---
 drivers/net/ethernet/stmicro/stmmac/dwmac4_lib.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/stmicro/stmmac/dwmac4_lib.c
+++ b/drivers/net/ethernet/stmicro/stmmac/dwmac4_lib.c
@@ -23,7 +23,7 @@ int dwmac4_dma_reset(void __iomem *ioadd
 
 	return readl_poll_timeout(ioaddr + DMA_BUS_MODE, value,
 				 !(value & DMA_BUS_MODE_SFT_RESET),
-				 10000, 1000000);
+				 10000, 3000000);
 }
 
 void dwmac4_set_rx_tail_ptr(struct stmmac_priv *priv, void __iomem *ioaddr,
