--- a/arch/arm64/boot/dts/rockchip/rk3566-radxa-zero-3.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3566-radxa-zero-3.dtsi
@@ -6,6 +6,13 @@
 #include "rk3566t.dtsi"
 
 / {
+	aliases {
+		led-boot = &led_green;
+		led-failsafe = &led_green;
+		led-running = &led_green;
+		led-upgrade = &led_green;
+	};
+
 	chosen {
 		stdout-path = "serial2:1500000n8";
 	};
@@ -26,12 +33,11 @@
 		pinctrl-names = "default";
 		pinctrl-0 = <&user_led2>;
 
-		led-green {
+		led_green: led-green {
 			color = <LED_COLOR_ID_GREEN>;
 			default-state = "on";
 			function = LED_FUNCTION_HEARTBEAT;
 			gpios = <&gpio0 RK_PA0 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "heartbeat";
 		};
 	};
 
