From 28a23b2437f9d6ef4ebe4c8da6e420004beca938 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Tue, 14 Apr 2026 00:47:00 +0100
Subject: [PATCH] ARM: dts: mediatek: mt7623n: remove mali reset

The mali reset on the MT7623N is very destructive and prevents
subsequent resumes after the GPU has been suspended.
Turns out the easiest fix is to just not use it.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 arch/arm/boot/dts/mediatek/mt7623n.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/mediatek/mt7623n.dtsi
+++ b/arch/arm/boot/dts/mediatek/mt7623n.dtsi
@@ -45,7 +45,7 @@
 			 <&g3dsys CLK_G3DSYS_CORE>;
 		clock-names = "bus", "core";
 		power-domains = <&scpsys MT2701_POWER_DOMAIN_MFG>;
-		resets = <&g3dsys MT2701_G3DSYS_CORE_RST>;
+		/* resets = <&g3dsys MT2701_G3DSYS_CORE_RST>; */
 	};
 
 	mmsys: syscon@14000000 {
