// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7242.dtsi"
#include "ar724x_senao_loader-4k.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "engenius,eap350-v1", "qca,ar7242";
	model = "EnGenius EAP350 v1";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};
	};
};

&mdio0 {
	status = "okay";

	phy4: ethernet-phy@4 {
		reg = <4>;
		eee-broken-100tx;
		eee-broken-1000t;
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0 0>;
	nvmem-cell-names = "mac-address";

	phy-handle = <&phy4>;
	phy-mode = "rgmii-id";

	pll-data = <0x02000000 0x00000101 0x00001313>;
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "pci168c,002a";
		reg = <0x0 0 0 0 0>;
		nvmem-cells = <&cal_art_1000>, <&macaddr_art_0 1>;
		nvmem-cell-names = "calibration", "mac-address";
	};
};

&art {
	nvmem-layout {
		compatible = "fixed-layout";
		#address-cells = <1>;
		#size-cells = <1>;

		macaddr_art_0: macaddr@0 {
			compatible = "mac-base";
			reg = <0x0 0x6>;
			#nvmem-cell-cells = <1>;
		};

		cal_art_1000: calibration@1000 {
			reg = <0x1000 0xeb8>;
		};
	};
};
