From 947643509279a605a09959a06d332bf027e8be57 Mon Sep 17 00:00:00 2001
From: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
Date: Mon, 10 Nov 2025 06:56:43 +0300
Subject: [PATCH] dt-bindings: clock: airoha: Add reset support to EN7523 clock
 binding

Introduce reset capability to EN7523 device-tree clock binding
documentation.

Signed-off-by: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
Reviewed-by: Rob Herring (Arm) <robh@kernel.org>
Signed-off-by: Stephen Boyd <sboyd@kernel.org>
---
 .../dt-bindings/reset/airoha,en7523-reset.h   | 61 +++++++++++++++++++
 1 file changed, 61 insertions(+)
 create mode 100644 include/dt-bindings/reset/airoha,en7523-reset.h

--- /dev/null
+++ b/include/dt-bindings/reset/airoha,en7523-reset.h
@@ -0,0 +1,61 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+/*
+ * Copyright (C) 2024 iopsys Software Solutions AB.
+ * Copyright (C) 2025 Genexis AB.
+ *
+ * Author: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
+ *
+ * based on
+ *   include/dt-bindings/reset/airoha,en7581-reset.h
+ * by Lorenzo Bianconi <lorenzo@kernel.org>
+ */
+
+#ifndef __DT_BINDINGS_RESET_CONTROLLER_AIROHA_EN7523_H_
+#define __DT_BINDINGS_RESET_CONTROLLER_AIROHA_EN7523_H_
+
+/* RST_CTRL2 */
+#define EN7523_XPON_PHY_RST		 0
+#define EN7523_XSI_MAC_RST		 1
+#define EN7523_XSI_PHY_RST		 2
+#define EN7523_NPU_RST			 3
+#define EN7523_I2S_RST			 4
+#define EN7523_TRNG_RST			 5
+#define EN7523_TRNG_MSTART_RST		 6
+#define EN7523_DUAL_HSI0_RST		 7
+#define EN7523_DUAL_HSI1_RST		 8
+#define EN7523_HSI_RST			 9
+#define EN7523_DUAL_HSI0_MAC_RST	10
+#define EN7523_DUAL_HSI1_MAC_RST	11
+#define EN7523_HSI_MAC_RST		12
+#define EN7523_WDMA_RST			13
+#define EN7523_WOE0_RST			14
+#define EN7523_WOE1_RST			15
+#define EN7523_HSDMA_RST		16
+#define EN7523_I2C2RBUS_RST		17
+#define EN7523_TDMA_RST			18
+/* RST_CTRL1 */
+#define EN7523_PCM1_ZSI_ISI_RST		19
+#define EN7523_FE_PDMA_RST		20
+#define EN7523_FE_QDMA_RST		21
+#define EN7523_PCM_SPIWP_RST		22
+#define EN7523_CRYPTO_RST		23
+#define EN7523_TIMER_RST		24
+#define EN7523_PCM1_RST			25
+#define EN7523_UART_RST			26
+#define EN7523_GPIO_RST			27
+#define EN7523_GDMA_RST			28
+#define EN7523_I2C_MASTER_RST		29
+#define EN7523_PCM2_ZSI_ISI_RST		30
+#define EN7523_SFC_RST			31
+#define EN7523_UART2_RST		32
+#define EN7523_GDMP_RST			33
+#define EN7523_FE_RST			34
+#define EN7523_USB_HOST_P0_RST		35
+#define EN7523_GSW_RST			36
+#define EN7523_SFC2_PCM_RST		37
+#define EN7523_PCIE0_RST		38
+#define EN7523_PCIE1_RST		39
+#define EN7523_PCIE_HB_RST		40
+#define EN7523_XPON_MAC_RST		41
+
+#endif /* __DT_BINDINGS_RESET_CONTROLLER_AIROHA_EN7523_H_ */
