From 9b695bfdb8b61bfb8766d5b8ce9552460a18a848 Mon Sep 17 00:00:00 2001
From: Stephen Gordon <gordoste@iinet.net.au>
Date: Mon, 23 Dec 2024 10:06:10 +1100
Subject: [PATCH] docs: pcm3168a: Add DT bindings to force clock consumer mode

Document the new force-adc-cons/force-dac-cons DT bindings.

Signed-off-by: Stephen Gordon <gordoste@iinet.net.au>
---
 Documentation/devicetree/bindings/sound/ti,pcm3168a.yaml | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/Documentation/devicetree/bindings/sound/ti,pcm3168a.yaml
+++ b/Documentation/devicetree/bindings/sound/ti,pcm3168a.yaml
@@ -58,6 +58,14 @@ properties:
   VCCDA2-supply:
     description: DAC power supply regulator 2 (+5V)
 
+  adc-force-cons:
+    description: Force ADC to operate in consumer mode. Useful if ADC and DAC
+      clock pins are tied together with DAC as producer.
+
+  dac-force-cons:
+    description: Force DAC to operate in consumer mode. Useful if ADC and DAC
+      clock pins are tied together with ADC as producer.
+
   ports:
     $ref: audio-graph-port.yaml#/definitions/port-base
     unevaluatedProperties: false
