From 174c73330839bad688b9fb2e9b6b9a2e5d74021f Mon Sep 17 00:00:00 2001
From: Emil Renner Berthing <kernel@esmil.dk>
Date: Thu, 14 Oct 2021 20:35:43 +0200
Subject: [PATCH 1009/1021] clk: starfive: jh7100: Keep more clocks alive

Signed-off-by: Emil Renner Berthing <kernel@esmil.dk>
---
 drivers/clk/starfive/clk-starfive-jh7100.c | 19 ++++++++++---------
 1 file changed, 10 insertions(+), 9 deletions(-)

--- a/drivers/clk/starfive/clk-starfive-jh7100.c
+++ b/drivers/clk/starfive/clk-starfive-jh7100.c
@@ -94,9 +94,9 @@ static const struct jh71x0_clk_data jh71
 	JH71X0_GATE(JH7100_CLK_DMA2PNOC_AXI, "dma2pnoc_axi", 0, JH7100_CLK_CPU_AXI),
 	JH71X0_GATE(JH7100_CLK_SGDMA2P_AHB, "sgdma2p_ahb", 0, JH7100_CLK_AHB_BUS),
 	JH71X0__DIV(JH7100_CLK_DLA_BUS, "dla_bus", 4, JH7100_CLK_DLA_ROOT),
-	JH71X0_GATE(JH7100_CLK_DLA_AXI, "dla_axi", 0, JH7100_CLK_DLA_BUS),
-	JH71X0_GATE(JH7100_CLK_DLANOC_AXI, "dlanoc_axi", 0, JH7100_CLK_DLA_BUS),
-	JH71X0_GATE(JH7100_CLK_DLA_APB, "dla_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GATE(JH7100_CLK_DLA_AXI, "dla_axi", CLK_IGNORE_UNUSED, JH7100_CLK_DLA_BUS),
+	JH71X0_GATE(JH7100_CLK_DLANOC_AXI, "dlanoc_axi", CLK_IGNORE_UNUSED, JH7100_CLK_DLA_BUS),
+	JH71X0_GATE(JH7100_CLK_DLA_APB, "dla_apb", CLK_IGNORE_UNUSED, JH7100_CLK_APB1_BUS),
 	JH71X0_GDIV(JH7100_CLK_VP6_CORE, "vp6_core", 0, 4, JH7100_CLK_DSP_ROOT_DIV),
 	JH71X0__DIV(JH7100_CLK_VP6BUS_SRC, "vp6bus_src", 4, JH7100_CLK_DSP_ROOT),
 	JH71X0_GDIV(JH7100_CLK_VP6_AXI, "vp6_axi", 0, 4, JH7100_CLK_VP6BUS_SRC),
@@ -163,8 +163,9 @@ static const struct jh71x0_clk_data jh71
 	JH71X0_GATE(JH7100_CLK_USB_AXI, "usb_axi", 0, JH7100_CLK_USB_BUS),
 	JH71X0_GATE(JH7100_CLK_USBNOC_AXI, "usbnoc_axi", 0, JH7100_CLK_USB_BUS),
 	JH71X0__DIV(JH7100_CLK_USBPHY_ROOTDIV, "usbphy_rootdiv", 4, JH7100_CLK_GMACUSB_ROOT),
-	JH71X0_GDIV(JH7100_CLK_USBPHY_125M, "usbphy_125m", 0, 8, JH7100_CLK_USBPHY_ROOTDIV),
-	JH71X0_GDIV(JH7100_CLK_USBPHY_PLLDIV25M, "usbphy_plldiv25m", 0, 32,
+	JH71X0_GDIV(JH7100_CLK_USBPHY_125M, "usbphy_125m", CLK_IGNORE_UNUSED, 8,
+		    JH7100_CLK_USBPHY_ROOTDIV),
+	JH71X0_GDIV(JH7100_CLK_USBPHY_PLLDIV25M, "usbphy_plldiv25m", CLK_IGNORE_UNUSED, 32,
 		    JH7100_CLK_USBPHY_ROOTDIV),
 	JH71X0__MUX(JH7100_CLK_USBPHY_25M, "usbphy_25m", 0, 2,
 		    JH7100_CLK_OSC_SYS,
@@ -183,11 +184,11 @@ static const struct jh71x0_clk_data jh71
 	JH71X0__DIV(JH7100_CLK_VIN_BUS, "vin_bus", 8, JH7100_CLK_VIN_SRC),
 	JH71X0_GATE(JH7100_CLK_VIN_AXI, "vin_axi", 0, JH7100_CLK_VIN_BUS),
 	JH71X0_GATE(JH7100_CLK_VINNOC_AXI, "vinnoc_axi", 0, JH7100_CLK_VIN_BUS),
-	JH71X0_GDIV(JH7100_CLK_VOUT_SRC, "vout_src", 0, 4, JH7100_CLK_VOUT_ROOT),
+	JH71X0_GDIV(JH7100_CLK_VOUT_SRC, "vout_src", CLK_IGNORE_UNUSED, 4, JH7100_CLK_VOUT_ROOT),
 	JH71X0__DIV(JH7100_CLK_DISPBUS_SRC, "dispbus_src", 4, JH7100_CLK_VOUTBUS_ROOT),
 	JH71X0__DIV(JH7100_CLK_DISP_BUS, "disp_bus", 4, JH7100_CLK_DISPBUS_SRC),
-	JH71X0_GATE(JH7100_CLK_DISP_AXI, "disp_axi", 0, JH7100_CLK_DISP_BUS),
-	JH71X0_GATE(JH7100_CLK_DISPNOC_AXI, "dispnoc_axi", 0, JH7100_CLK_DISP_BUS),
+	JH71X0_GATE(JH7100_CLK_DISP_AXI, "disp_axi", CLK_IGNORE_UNUSED, JH7100_CLK_DISP_BUS),
+	JH71X0_GATE(JH7100_CLK_DISPNOC_AXI, "dispnoc_axi", CLK_IGNORE_UNUSED, JH7100_CLK_DISP_BUS),
 	JH71X0_GATE(JH7100_CLK_SDIO0_AHB, "sdio0_ahb", 0, JH7100_CLK_AHB_BUS),
 	JH71X0_GDIV(JH7100_CLK_SDIO0_CCLKINT, "sdio0_cclkint", 0, 24, JH7100_CLK_PERH0_SRC),
 	JH71X0__INV(JH7100_CLK_SDIO0_CCLKINT_INV, "sdio0_cclkint_inv", JH7100_CLK_SDIO0_CCLKINT),
@@ -223,7 +224,7 @@ static const struct jh71x0_clk_data jh71
 	JH71X0_GATE(JH7100_CLK_AES, "aes_clk", 0, JH7100_CLK_SEC_AHB),
 	JH71X0_GATE(JH7100_CLK_SHA, "sha_clk", 0, JH7100_CLK_SEC_AHB),
 	JH71X0_GATE(JH7100_CLK_PKA, "pka_clk", 0, JH7100_CLK_SEC_AHB),
-	JH71X0_GATE(JH7100_CLK_TRNG_APB, "trng_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GATE(JH7100_CLK_TRNG_APB, "trng_apb", CLK_IGNORE_UNUSED, JH7100_CLK_APB1_BUS),
 	JH71X0_GATE(JH7100_CLK_OTP_APB, "otp_apb", 0, JH7100_CLK_APB1_BUS),
 	JH71X0_GATE(JH7100_CLK_UART0_APB, "uart0_apb", 0, JH7100_CLK_APB1_BUS),
 	JH71X0_GDIV(JH7100_CLK_UART0_CORE, "uart0_core", 0, 63, JH7100_CLK_PERH1_SRC),
