From 01561065af5bf1d2a4244896d897e3a1eafbcd46 Mon Sep 17 00:00:00 2001
Message-Id: <01561065af5bf1d2a4244896d897e3a1eafbcd46.1678717704.git.lorenzo@kernel.org>
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Mon, 13 Mar 2023 15:10:56 +0100
Subject: [PATCH net-next] arm64: dts: mt7986: move ilm in a dedicated node

Since the ilm memory region is not part of the RAM SoC, move ilm in a
deidicated syscon node.
This patch helps to keep backward-compatibility with older version of
uboot codebase where we have a limit of 8 reserved-memory dts child
nodes.

Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
---
 arch/arm64/boot/dts/mediatek/mt7986a.dtsi | 34 +++++++++++------------
 1 file changed, 16 insertions(+), 18 deletions(-)

--- a/arch/arm64/boot/dts/mediatek/mt7986a.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt7986a.dtsi
@@ -97,16 +97,6 @@
 			no-map;
 		};
 
-		wo_ilm0: wo-ilm@151e0000 {
-			reg = <0 0x151e0000 0 0x8000>;
-			no-map;
-		};
-
-		wo_ilm1: wo-ilm@151f0000 {
-			reg = <0 0x151f0000 0 0x8000>;
-			no-map;
-		};
-
 		wo_data: wo-data@4fd80000 {
 			reg = <0 0x4fd80000 0 0x240000>;
 			no-map;
@@ -526,11 +516,10 @@
 			reg = <0 0x15010000 0 0x1000>;
 			interrupt-parent = <&gic>;
 			interrupts = <GIC_SPI 205 IRQ_TYPE_LEVEL_HIGH>;
-			memory-region = <&wo_emi0>, <&wo_ilm0>, <&wo_dlm0>,
-					<&wo_data>;
-			memory-region-names = "wo-emi", "wo-ilm", "wo-dlm",
-					      "wo-data";
+			memory-region = <&wo_emi0>, <&wo_dlm0>, <&wo_data>;
+			memory-region-names = "wo-emi", "wo-dlm", "wo-data";
 			mediatek,wo-ccif = <&wo_ccif0>;
+			mediatek,wo-ilm = <&wo_ilm0>;
 			mediatek,wo-cpuboot = <&wo_cpuboot>;
 		};
 
@@ -540,11 +529,10 @@
 			reg = <0 0x15011000 0 0x1000>;
 			interrupt-parent = <&gic>;
 			interrupts = <GIC_SPI 206 IRQ_TYPE_LEVEL_HIGH>;
-			memory-region = <&wo_emi1>, <&wo_ilm1>, <&wo_dlm1>,
-					<&wo_data>;
-			memory-region-names = "wo-emi", "wo-ilm", "wo-dlm",
-					      "wo-data";
+			memory-region = <&wo_emi1>, <&wo_dlm1>, <&wo_data>;
+			memory-region-names = "wo-emi", "wo-dlm", "wo-data";
 			mediatek,wo-ccif = <&wo_ccif1>;
+			mediatek,wo-ilm = <&wo_ilm1>;
 			mediatek,wo-cpuboot = <&wo_cpuboot>;
 		};
 
@@ -619,6 +607,16 @@
 			interrupts = <GIC_SPI 212 IRQ_TYPE_LEVEL_HIGH>;
 		};
 
+		wo_ilm0: syscon@151e0000 {
+			compatible = "mediatek,mt7986-wo-ilm", "syscon";
+			reg = <0 0x151e0000 0 0x8000>;
+		};
+
+		wo_ilm1: syscon@151f0000 {
+			compatible = "mediatek,mt7986-wo-ilm", "syscon";
+			reg = <0 0x151f0000 0 0x8000>;
+		};
+
 		wo_cpuboot: syscon@15194000 {
 			compatible = "mediatek,mt7986-wo-cpuboot", "syscon";
 			reg = <0 0x15194000 0 0x1000>;
