From 2728124b7d4e32c32ffdc3f9091ccf8c97179f93 Mon Sep 17 00:00:00 2001
From: Devi Priya <quic_devipriy@quicinc.com>
Date: Wed, 4 Feb 2026 15:25:08 +0400
Subject: [PATCH] pwm: driver for qualcomm ipq6018 pwm block

Driver for the PWM block in Qualcomm IPQ6018 line of SoCs. Based on
driver from downstream Codeaurora kernel tree. Removed support for older
(V1) variants because I have no access to that hardware.

Tested on IPQ5018 and IPQ6010 based hardware.

Co-developed-by: Baruch Siach <baruch.siach@siklu.com>
Signed-off-by: Baruch Siach <baruch.siach@siklu.com>
Signed-off-by: Devi Priya <quic_devipriy@quicinc.com>
Reviewed-by: Bjorn Andersson <andersson@kernel.org>
Signed-off-by: George Moussalem <george.moussalem@outlook.com>
---
 drivers/pwm/Kconfig   |  12 +++
 drivers/pwm/Makefile  |   1 +
 drivers/pwm/pwm-ipq.c | 239 ++++++++++++++++++++++++++++++++++++++++++
 3 files changed, 252 insertions(+)
 create mode 100644 drivers/pwm/pwm-ipq.c

--- a/drivers/pwm/Kconfig
+++ b/drivers/pwm/Kconfig
@@ -337,6 +337,18 @@ config PWM_INTEL_LGM
 	  To compile this driver as a module, choose M here: the module
 	  will be called pwm-intel-lgm.
 
+config PWM_IPQ
+	tristate "IPQ PWM support"
+	depends on ARCH_QCOM || COMPILE_TEST
+	depends on HAVE_CLK && HAS_IOMEM
+	help
+	  Generic PWM framework driver for IPQ PWM block which supports
+	  4 pwm channels. Each of the these channels can be configured
+	  independent of each other.
+
+	  To compile this driver as a module, choose M here: the module
+	  will be called pwm-ipq.
+
 config PWM_IQS620A
 	tristate "Azoteq IQS620A PWM support"
 	depends on MFD_IQS62X || COMPILE_TEST
--- a/drivers/pwm/Makefile
+++ b/drivers/pwm/Makefile
@@ -28,6 +28,7 @@ obj-$(CONFIG_PWM_IMX1)		+= pwm-imx1.o
 obj-$(CONFIG_PWM_IMX27)		+= pwm-imx27.o
 obj-$(CONFIG_PWM_IMX_TPM)	+= pwm-imx-tpm.o
 obj-$(CONFIG_PWM_INTEL_LGM)	+= pwm-intel-lgm.o
+obj-$(CONFIG_PWM_IPQ)		+= pwm-ipq.o
 obj-$(CONFIG_PWM_IQS620A)	+= pwm-iqs620a.o
 obj-$(CONFIG_PWM_JZ4740)	+= pwm-jz4740.o
 obj-$(CONFIG_PWM_KEEMBAY)	+= pwm-keembay.o
--- /dev/null
+++ b/drivers/pwm/pwm-ipq.c
@@ -0,0 +1,239 @@
+// SPDX-License-Identifier: BSD-3-Clause OR GPL-2.0
+/*
+ * Copyright (c) 2016-2017, 2020 The Linux Foundation. All rights reserved.
+ *
+ * Hardware notes / Limitations:
+ * - The PWM controller has no publicly available datasheet.
+ * - Each of the four channels is programmed via two 32-bit registers
+ *   (REG0 and REG1 at 8-byte stride).
+ * - Period and duty-cycle reconfiguration is fully atomic: new divider,
+ *   pre-divider, and high-duration values are latched by setting the
+ *   UPDATE bit (bit 30 in REG1). The hardware applies the new settings
+ *   at the beginning of the next period without disabling the output,
+ *   so the currently running period is always completed.
+ * - On disable (clearing the ENABLE bit 31 in REG1), the hardware
+ *   finishes the current period before stopping the output. The pin
+ *   is then driven to the inactive (low) level.
+ * - Upon disabling, the hardware resets the pre-divider (PRE_DIV) and divider
+ *   fields (PWM_DIV) in REG0 and REG1 to 0x0000 and 0x0001 respectively.
+ * - Only normal polarity is supported.
+ */
+
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/pwm.h>
+#include <linux/clk.h>
+#include <linux/io.h>
+#include <linux/of.h>
+#include <linux/math64.h>
+#include <linux/of_device.h>
+#include <linux/bitfield.h>
+#include <linux/units.h>
+
+/* The frequency range supported is 1 Hz to clock rate */
+#define IPQ_PWM_MAX_PERIOD_NS	((u64)NSEC_PER_SEC)
+
+/*
+ * Two 32-bit registers for each PWM: REG0, and REG1.
+ * Base offset for PWM #i is at 8 * #i.
+ */
+#define IPQ_PWM_REG0			0
+#define IPQ_PWM_REG0_PWM_DIV		GENMASK(15, 0)
+#define IPQ_PWM_REG0_HI_DURATION	GENMASK(31, 16)
+
+#define IPQ_PWM_REG1			4
+#define IPQ_PWM_REG1_PRE_DIV		GENMASK(15, 0)
+
+/*
+ * The max value specified for each field is based on the number of bits
+ * in the pwm control register for that field (16-bit)
+ */
+#define IPQ_PWM_MAX_DIV			FIELD_MAX(IPQ_PWM_REG0_PWM_DIV)
+
+/*
+ * Enable bit is set to enable output toggling in pwm device.
+ * Update bit is set to trigger the change and is unset automatically
+ * to reflect the changed divider and high duration values in register.
+ */
+#define IPQ_PWM_REG1_UPDATE		BIT(30)
+#define IPQ_PWM_REG1_ENABLE		BIT(31)
+
+struct ipq_pwm_chip {
+	void __iomem *mem;
+	unsigned long clk_rate;
+};
+
+static struct ipq_pwm_chip *ipq_pwm_from_chip(struct pwm_chip *chip)
+{
+	return pwmchip_get_drvdata(chip);
+}
+
+static unsigned int ipq_pwm_reg_read(struct pwm_device *pwm, unsigned int reg)
+{
+	struct ipq_pwm_chip *ipq_chip = ipq_pwm_from_chip(pwm->chip);
+	unsigned int off = 8 * pwm->hwpwm + reg;
+
+	return readl(ipq_chip->mem + off);
+}
+
+static void ipq_pwm_reg_write(struct pwm_device *pwm, unsigned int reg,
+			      unsigned int val)
+{
+	struct ipq_pwm_chip *ipq_chip = ipq_pwm_from_chip(pwm->chip);
+	unsigned int off = 8 * pwm->hwpwm + reg;
+
+	writel(val, ipq_chip->mem + off);
+}
+
+static int ipq_pwm_apply(struct pwm_chip *chip, struct pwm_device *pwm,
+			 const struct pwm_state *state)
+{
+	struct ipq_pwm_chip *ipq_chip = ipq_pwm_from_chip(chip);
+	unsigned int pre_div, pwm_div;
+	u64 period_ns, duty_ns;
+	unsigned long val = 0;
+	unsigned long hi_dur;
+
+	if (state->polarity != PWM_POLARITY_NORMAL)
+		return -EINVAL;
+
+	if (!ipq_chip->clk_rate)
+		return -EINVAL;
+
+	if (state->period < DIV64_U64_ROUND_UP(NSEC_PER_SEC,
+					       ipq_chip->clk_rate))
+		return -ERANGE;
+
+	period_ns = min(state->period, IPQ_PWM_MAX_PERIOD_NS);
+	duty_ns = min(state->duty_cycle, period_ns);
+
+	pwm_div = IPQ_PWM_MAX_DIV - 1;
+	pre_div = mul_u64_u64_div_u64(period_ns, ipq_chip->clk_rate,
+				      (u64)NSEC_PER_SEC * (pwm_div + 1));
+	pre_div = (pre_div > 0) ? pre_div - 1 : 0;
+
+	if (pre_div > IPQ_PWM_MAX_DIV)
+		pre_div = IPQ_PWM_MAX_DIV;
+
+	/*
+	 * high duration = pwm duty * (pwm div + 1)
+	 * pwm duty = duty_ns / period_ns
+	 */
+	hi_dur = mul_u64_u64_div_u64(duty_ns, ipq_chip->clk_rate,
+				     (u64)(pre_div + 1) * NSEC_PER_SEC);
+
+	val = FIELD_PREP(IPQ_PWM_REG0_HI_DURATION, hi_dur) |
+		FIELD_PREP(IPQ_PWM_REG0_PWM_DIV, pwm_div);
+	ipq_pwm_reg_write(pwm, IPQ_PWM_REG0, val);
+
+	val = FIELD_PREP(IPQ_PWM_REG1_PRE_DIV, pre_div);
+	ipq_pwm_reg_write(pwm, IPQ_PWM_REG1, val);
+
+	/* PWM enable toggle needs a separate write to REG1 */
+	val |= IPQ_PWM_REG1_UPDATE;
+	if (state->enabled)
+		val |= IPQ_PWM_REG1_ENABLE;
+	ipq_pwm_reg_write(pwm, IPQ_PWM_REG1, val);
+
+	return 0;
+}
+
+static int ipq_pwm_get_state(struct pwm_chip *chip, struct pwm_device *pwm,
+			     struct pwm_state *state)
+{
+	struct ipq_pwm_chip *ipq_chip = ipq_pwm_from_chip(chip);
+	unsigned int pre_div, pwm_div, hi_dur;
+	u64 effective_div, hi_div;
+	u32 reg0, reg1;
+
+	reg1 = ipq_pwm_reg_read(pwm, IPQ_PWM_REG1);
+	state->enabled = reg1 & IPQ_PWM_REG1_ENABLE;
+
+	if (!state->enabled)
+		return 0;
+
+	reg0 = ipq_pwm_reg_read(pwm, IPQ_PWM_REG0);
+
+	state->polarity = PWM_POLARITY_NORMAL;
+
+	pwm_div = FIELD_GET(IPQ_PWM_REG0_PWM_DIV, reg0);
+	hi_dur = FIELD_GET(IPQ_PWM_REG0_HI_DURATION, reg0);
+	pre_div = FIELD_GET(IPQ_PWM_REG1_PRE_DIV, reg1);
+
+	effective_div = (u64)(pre_div + 1) * (pwm_div + 1);
+	state->period = DIV64_U64_ROUND_UP(effective_div * NSEC_PER_SEC,
+					   ipq_chip->clk_rate);
+
+	hi_div = hi_dur * (pre_div + 1);
+	state->duty_cycle = DIV64_U64_ROUND_UP(hi_div * NSEC_PER_SEC,
+					       ipq_chip->clk_rate);
+
+	/*
+	 * ensure a valid config is passed back to PWM core in case duty_cycle
+	 * is > period (>100%)
+	 */
+	state->duty_cycle = min(state->duty_cycle, state->period);
+
+	return 0;
+}
+
+static const struct pwm_ops ipq_pwm_ops = {
+	.apply = ipq_pwm_apply,
+	.get_state = ipq_pwm_get_state,
+};
+
+static int ipq_pwm_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct ipq_pwm_chip *pwm;
+	struct pwm_chip *chip;
+	struct clk *clk;
+	int ret;
+
+	chip = devm_pwmchip_alloc(dev, 4, sizeof(*pwm));
+	if (IS_ERR(chip))
+		return PTR_ERR(chip);
+	pwm = ipq_pwm_from_chip(chip);
+
+	pwm->mem = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(pwm->mem))
+		return dev_err_probe(dev, PTR_ERR(pwm->mem),
+				     "Failed to acquire resource\n");
+
+	clk = devm_clk_get_enabled(dev, NULL);
+	if (IS_ERR(clk))
+		return dev_err_probe(dev, PTR_ERR(clk),
+				     "Failed to get clock\n");
+
+	ret = devm_clk_rate_exclusive_get(dev, clk);
+	if (ret)
+		return dev_err_probe(dev, ret, "Failed to lock clock rate\n");
+
+	pwm->clk_rate = clk_get_rate(clk);
+
+	chip->ops = &ipq_pwm_ops;
+
+	ret = devm_pwmchip_add(dev, chip);
+	if (ret < 0)
+		return dev_err_probe(dev, ret, "Failed to add pwm chip\n");
+
+	return 0;
+}
+
+static const struct of_device_id pwm_ipq_dt_match[] = {
+	{ .compatible = "qcom,ipq6018-pwm", },
+	{}
+};
+MODULE_DEVICE_TABLE(of, pwm_ipq_dt_match);
+
+static struct platform_driver ipq_pwm_driver = {
+	.driver = {
+		.name = "ipq-pwm",
+		.of_match_table = pwm_ipq_dt_match,
+	},
+	.probe = ipq_pwm_probe,
+};
+
+module_platform_driver(ipq_pwm_driver);
+
+MODULE_LICENSE("GPL");
