From 4c711536c4d5489de846a7bd73a8cf3563722c76 Mon Sep 17 00:00:00 2001
From: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
Date: Sun, 26 Apr 2026 23:22:20 +0300
Subject: [PATCH 06/29] pinctrl: airoha: add pin controller and gpio driver for
 AN7581 SoC

This patch adds U-Boot pin controller and gpio driver for Airoha AN7581 SoC.

Signed-off-by: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
Reviewed-by: David Lechner <dlechner@baylibre.com>
---
 drivers/pinctrl/airoha/Kconfig          |    5 +
 drivers/pinctrl/airoha/Makefile         |    2 +
 drivers/pinctrl/airoha/pinctrl-an7581.c | 1484 +++++++++++++++++++++++
 3 files changed, 1491 insertions(+)
 create mode 100644 drivers/pinctrl/airoha/pinctrl-an7581.c

diff --git a/drivers/pinctrl/airoha/Kconfig b/drivers/pinctrl/airoha/Kconfig
index eb87afbb374..ae387f70b22 100644
--- a/drivers/pinctrl/airoha/Kconfig
+++ b/drivers/pinctrl/airoha/Kconfig
@@ -9,3 +9,8 @@ config PINCTRL_AIROHA
 	select REGMAP
 	select SYSCON
 	bool
+
+config PINCTRL_AIROHA_AN7581
+	bool "Airoha AN7581 pin controller and gpio driver"
+	depends on TARGET_AN7581
+	select PINCTRL_AIROHA
diff --git a/drivers/pinctrl/airoha/Makefile b/drivers/pinctrl/airoha/Makefile
index a25b744dd7a..909bd9a04d9 100644
--- a/drivers/pinctrl/airoha/Makefile
+++ b/drivers/pinctrl/airoha/Makefile
@@ -1,3 +1,5 @@
 # SPDX-License-Identifier: GPL-2.0
 
 obj-$(CONFIG_PINCTRL_AIROHA)		+= pinctrl-airoha.o
+
+obj-$(CONFIG_PINCTRL_AIROHA_AN7581)	+= pinctrl-an7581.o
diff --git a/drivers/pinctrl/airoha/pinctrl-an7581.c b/drivers/pinctrl/airoha/pinctrl-an7581.c
new file mode 100644
index 00000000000..4f7da74a1cf
--- /dev/null
+++ b/drivers/pinctrl/airoha/pinctrl-an7581.c
@@ -0,0 +1,1484 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * Author: Lorenzo Bianconi <lorenzo@kernel.org>
+ * Author: Benjamin Larsson <benjamin.larsson@genexis.eu>
+ * Author: Markus Gothe <markus.gothe@genexis.eu>
+ */
+
+#include "airoha-common.h"
+
+/* MUX */
+#define REG_GPIO_2ND_I2C_MODE			0x0214
+#define GPIO_MDC_IO_MASTER_MODE_MASK		BIT(14)
+#define GPIO_I2C_MASTER_MODE_MODE		BIT(13)
+#define GPIO_I2S_MODE_MASK			BIT(12)
+#define GPIO_I2C_SLAVE_MODE_MODE		BIT(11)
+#define GPIO_LAN3_LED1_MODE_MASK		BIT(10)
+#define GPIO_LAN3_LED0_MODE_MASK		BIT(9)
+#define GPIO_LAN2_LED1_MODE_MASK		BIT(8)
+#define GPIO_LAN2_LED0_MODE_MASK		BIT(7)
+#define GPIO_LAN1_LED1_MODE_MASK		BIT(6)
+#define GPIO_LAN1_LED0_MODE_MASK		BIT(5)
+#define GPIO_LAN0_LED1_MODE_MASK		BIT(4)
+#define GPIO_LAN0_LED0_MODE_MASK		BIT(3)
+#define PON_TOD_1PPS_MODE_MASK			BIT(2)
+#define GSW_TOD_1PPS_MODE_MASK			BIT(1)
+#define GPIO_2ND_I2C_MODE_MASK			BIT(0)
+
+#define REG_GPIO_SPI_CS1_MODE			0x0218
+#define GPIO_PCM_SPI_CS4_MODE_MASK		BIT(21)
+#define GPIO_PCM_SPI_CS3_MODE_MASK		BIT(20)
+#define GPIO_PCM_SPI_CS2_MODE_P156_MASK		BIT(19)
+#define GPIO_PCM_SPI_CS2_MODE_P128_MASK		BIT(18)
+#define GPIO_PCM_SPI_CS1_MODE_MASK		BIT(17)
+#define GPIO_PCM_SPI_MODE_MASK			BIT(16)
+#define GPIO_PCM2_MODE_MASK			BIT(13)
+#define GPIO_PCM1_MODE_MASK			BIT(12)
+#define GPIO_PCM_INT_MODE_MASK			BIT(9)
+#define GPIO_PCM_RESET_MODE_MASK		BIT(8)
+#define GPIO_SPI_QUAD_MODE_MASK			BIT(4)
+#define GPIO_SPI_CS4_MODE_MASK			BIT(3)
+#define GPIO_SPI_CS3_MODE_MASK			BIT(2)
+#define GPIO_SPI_CS2_MODE_MASK			BIT(1)
+#define GPIO_SPI_CS1_MODE_MASK			BIT(0)
+
+#define REG_GPIO_PON_MODE			0x021c
+#define GPIO_PARALLEL_NAND_MODE_MASK		BIT(14)
+#define GPIO_SGMII_MDIO_MODE_MASK		BIT(13)
+#define GPIO_PCIE_RESET2_MASK			BIT(12)
+#define SIPO_RCLK_MODE_MASK			BIT(11)
+#define GPIO_PCIE_RESET1_MASK			BIT(10)
+#define GPIO_PCIE_RESET0_MASK			BIT(9)
+#define GPIO_UART5_MODE_MASK			BIT(8)
+#define GPIO_UART4_MODE_MASK			BIT(7)
+#define GPIO_HSUART_CTS_RTS_MODE_MASK		BIT(6)
+#define GPIO_HSUART_MODE_MASK			BIT(5)
+#define GPIO_UART2_CTS_RTS_MODE_MASK		BIT(4)
+#define GPIO_UART2_MODE_MASK			BIT(3)
+#define GPIO_SIPO_MODE_MASK			BIT(2)
+#define GPIO_EMMC_MODE_MASK			BIT(1)
+#define GPIO_PON_MODE_MASK			BIT(0)
+
+#define REG_NPU_UART_EN				0x0224
+#define JTAG_UDI_EN_MASK			BIT(4)
+#define JTAG_DFD_EN_MASK			BIT(3)
+
+#define REG_FORCE_GPIO_EN			0x0228
+#define FORCE_GPIO_EN(n)			BIT(n)
+
+/* LED MAP */
+#define REG_LAN_LED0_MAPPING			0x027c
+#define REG_LAN_LED1_MAPPING			0x0280
+
+#define LAN4_LED_MAPPING_MASK			GENMASK(18, 16)
+#define LAN4_PHY_LED_MAP(_n)			FIELD_PREP_CONST(LAN4_LED_MAPPING_MASK, (_n))
+
+#define LAN3_LED_MAPPING_MASK			GENMASK(14, 12)
+#define LAN3_PHY_LED_MAP(_n)			FIELD_PREP_CONST(LAN3_LED_MAPPING_MASK, (_n))
+
+#define LAN2_LED_MAPPING_MASK			GENMASK(10, 8)
+#define LAN2_PHY_LED_MAP(_n)			FIELD_PREP_CONST(LAN2_LED_MAPPING_MASK, (_n))
+
+#define LAN1_LED_MAPPING_MASK			GENMASK(6, 4)
+#define LAN1_PHY_LED_MAP(_n)			FIELD_PREP_CONST(LAN1_LED_MAPPING_MASK, (_n))
+
+#define LAN0_LED_MAPPING_MASK			GENMASK(2, 0)
+#define LAN0_PHY_LED_MAP(_n)			FIELD_PREP_CONST(LAN0_LED_MAPPING_MASK, (_n))
+
+/* CONF */
+#define REG_I2C_SDA_E2				0x001c
+#define SPI_MISO_E2_MASK			BIT(14)
+#define SPI_MOSI_E2_MASK			BIT(13)
+#define SPI_CLK_E2_MASK				BIT(12)
+#define SPI_CS0_E2_MASK				BIT(11)
+#define PCIE2_RESET_E2_MASK			BIT(10)
+#define PCIE1_RESET_E2_MASK			BIT(9)
+#define PCIE0_RESET_E2_MASK			BIT(8)
+#define UART1_RXD_E2_MASK			BIT(3)
+#define UART1_TXD_E2_MASK			BIT(2)
+#define I2C_SCL_E2_MASK				BIT(1)
+#define I2C_SDA_E2_MASK				BIT(0)
+
+#define REG_I2C_SDA_E4				0x0020
+#define SPI_MISO_E4_MASK			BIT(14)
+#define SPI_MOSI_E4_MASK			BIT(13)
+#define SPI_CLK_E4_MASK				BIT(12)
+#define SPI_CS0_E4_MASK				BIT(11)
+#define PCIE2_RESET_E4_MASK			BIT(10)
+#define PCIE1_RESET_E4_MASK			BIT(9)
+#define PCIE0_RESET_E4_MASK			BIT(8)
+#define UART1_RXD_E4_MASK			BIT(3)
+#define UART1_TXD_E4_MASK			BIT(2)
+#define I2C_SCL_E4_MASK				BIT(1)
+#define I2C_SDA_E4_MASK				BIT(0)
+
+#define REG_GPIO_L_E2				0x0024
+#define REG_GPIO_L_E4				0x0028
+#define REG_GPIO_H_E2				0x002c
+#define REG_GPIO_H_E4				0x0030
+
+#define REG_I2C_SDA_PU				0x0044
+#define SPI_MISO_PU_MASK			BIT(14)
+#define SPI_MOSI_PU_MASK			BIT(13)
+#define SPI_CLK_PU_MASK				BIT(12)
+#define SPI_CS0_PU_MASK				BIT(11)
+#define PCIE2_RESET_PU_MASK			BIT(10)
+#define PCIE1_RESET_PU_MASK			BIT(9)
+#define PCIE0_RESET_PU_MASK			BIT(8)
+#define UART1_RXD_PU_MASK			BIT(3)
+#define UART1_TXD_PU_MASK			BIT(2)
+#define I2C_SCL_PU_MASK				BIT(1)
+#define I2C_SDA_PU_MASK				BIT(0)
+
+#define REG_I2C_SDA_PD				0x0048
+#define SPI_MISO_PD_MASK			BIT(14)
+#define SPI_MOSI_PD_MASK			BIT(13)
+#define SPI_CLK_PD_MASK				BIT(12)
+#define SPI_CS0_PD_MASK				BIT(11)
+#define PCIE2_RESET_PD_MASK			BIT(10)
+#define PCIE1_RESET_PD_MASK			BIT(9)
+#define PCIE0_RESET_PD_MASK			BIT(8)
+#define UART1_RXD_PD_MASK			BIT(3)
+#define UART1_TXD_PD_MASK			BIT(2)
+#define I2C_SCL_PD_MASK				BIT(1)
+#define I2C_SDA_PD_MASK				BIT(0)
+
+#define REG_GPIO_L_PU				0x004c
+#define REG_GPIO_L_PD				0x0050
+#define REG_GPIO_H_PU				0x0054
+#define REG_GPIO_H_PD				0x0058
+
+#define REG_PCIE_RESET_OD			0x018c
+#define PCIE2_RESET_OD_MASK			BIT(2)
+#define PCIE1_RESET_OD_MASK			BIT(1)
+#define PCIE0_RESET_OD_MASK			BIT(0)
+
+/* PWM MODE CONF */
+#define REG_GPIO_FLASH_MODE_CFG			0x0034
+#define GPIO15_FLASH_MODE_CFG			BIT(15)
+#define GPIO14_FLASH_MODE_CFG			BIT(14)
+#define GPIO13_FLASH_MODE_CFG			BIT(13)
+#define GPIO12_FLASH_MODE_CFG			BIT(12)
+#define GPIO11_FLASH_MODE_CFG			BIT(11)
+#define GPIO10_FLASH_MODE_CFG			BIT(10)
+#define GPIO9_FLASH_MODE_CFG			BIT(9)
+#define GPIO8_FLASH_MODE_CFG			BIT(8)
+#define GPIO7_FLASH_MODE_CFG			BIT(7)
+#define GPIO6_FLASH_MODE_CFG			BIT(6)
+#define GPIO5_FLASH_MODE_CFG			BIT(5)
+#define GPIO4_FLASH_MODE_CFG			BIT(4)
+#define GPIO3_FLASH_MODE_CFG			BIT(3)
+#define GPIO2_FLASH_MODE_CFG			BIT(2)
+#define GPIO1_FLASH_MODE_CFG			BIT(1)
+#define GPIO0_FLASH_MODE_CFG			BIT(0)
+
+/* PWM MODE CONF EXT */
+#define REG_GPIO_FLASH_MODE_CFG_EXT		0x0068
+#define GPIO51_FLASH_MODE_CFG			BIT(31)
+#define GPIO50_FLASH_MODE_CFG			BIT(30)
+#define GPIO49_FLASH_MODE_CFG			BIT(29)
+#define GPIO48_FLASH_MODE_CFG			BIT(28)
+#define GPIO47_FLASH_MODE_CFG			BIT(27)
+#define GPIO46_FLASH_MODE_CFG			BIT(26)
+#define GPIO45_FLASH_MODE_CFG			BIT(25)
+#define GPIO44_FLASH_MODE_CFG			BIT(24)
+#define GPIO43_FLASH_MODE_CFG			BIT(23)
+#define GPIO42_FLASH_MODE_CFG			BIT(22)
+#define GPIO41_FLASH_MODE_CFG			BIT(21)
+#define GPIO40_FLASH_MODE_CFG			BIT(20)
+#define GPIO39_FLASH_MODE_CFG			BIT(19)
+#define GPIO38_FLASH_MODE_CFG			BIT(18)
+#define GPIO37_FLASH_MODE_CFG			BIT(17)
+#define GPIO36_FLASH_MODE_CFG			BIT(16)
+#define GPIO31_FLASH_MODE_CFG			BIT(15)
+#define GPIO30_FLASH_MODE_CFG			BIT(14)
+#define GPIO29_FLASH_MODE_CFG			BIT(13)
+#define GPIO28_FLASH_MODE_CFG			BIT(12)
+#define GPIO27_FLASH_MODE_CFG			BIT(11)
+#define GPIO26_FLASH_MODE_CFG			BIT(10)
+#define GPIO25_FLASH_MODE_CFG			BIT(9)
+#define GPIO24_FLASH_MODE_CFG			BIT(8)
+#define GPIO23_FLASH_MODE_CFG			BIT(7)
+#define GPIO22_FLASH_MODE_CFG			BIT(6)
+#define GPIO21_FLASH_MODE_CFG			BIT(5)
+#define GPIO20_FLASH_MODE_CFG			BIT(4)
+#define GPIO19_FLASH_MODE_CFG			BIT(3)
+#define GPIO18_FLASH_MODE_CFG			BIT(2)
+#define GPIO17_FLASH_MODE_CFG			BIT(1)
+#define GPIO16_FLASH_MODE_CFG			BIT(0)
+
+#define AIROHA_PINCTRL_GPIO(gpio, mux_val)			\
+	{							\
+		.name = (gpio),					\
+		.regmap[0] = {					\
+			AIROHA_FUNC_MUX,			\
+			REG_GPIO_PON_MODE,			\
+			(mux_val),				\
+			(mux_val)				\
+		},						\
+		.regmap_size = 1,				\
+	}
+
+#define AIROHA_PINCTRL_GPIO_EXT(gpio, mux_val, smux_val)	\
+	{							\
+		.name = (gpio),					\
+		.regmap[0] = {					\
+			AIROHA_FUNC_PWM_EXT_MUX,		\
+			REG_GPIO_FLASH_MODE_CFG_EXT,		\
+			(mux_val),				\
+			0					\
+		},						\
+		.regmap[1] = {					\
+			AIROHA_FUNC_MUX,			\
+			REG_GPIO_PON_MODE,			\
+			(smux_val),				\
+			(smux_val)				\
+		},						\
+		.regmap_size = 2,				\
+	}
+
+/* PWM */
+#define AIROHA_PINCTRL_PWM(gpio, mux_val)			\
+	{							\
+		.name = (gpio),					\
+		.regmap[0] = {					\
+			AIROHA_FUNC_PWM_MUX,			\
+			REG_GPIO_FLASH_MODE_CFG,		\
+			(mux_val),				\
+			(mux_val)				\
+		},						\
+		.regmap_size = 1,				\
+	}
+
+#define AIROHA_PINCTRL_PWM_EXT(gpio, mux_val)			\
+	{							\
+		.name = (gpio),					\
+		.regmap[0] = {					\
+			AIROHA_FUNC_PWM_EXT_MUX,		\
+			REG_GPIO_FLASH_MODE_CFG_EXT,		\
+			(mux_val),				\
+			(mux_val)				\
+		},						\
+		.regmap_size = 1,				\
+	}
+
+#define AIROHA_PINCTRL_PWM_EXT_SEC(gpio, mux_val, smux_val)	\
+	{							\
+		.name = (gpio),					\
+		.regmap[0] = {					\
+			AIROHA_FUNC_PWM_EXT_MUX,		\
+			REG_GPIO_FLASH_MODE_CFG_EXT,		\
+			(mux_val),				\
+			(mux_val)				\
+		},						\
+		.regmap[1] = {					\
+			AIROHA_FUNC_MUX,			\
+			REG_GPIO_PON_MODE,			\
+			(smux_val),				\
+			(smux_val)				\
+		},						\
+		.regmap_size = 2,				\
+	}
+
+#define AIROHA_PINCTRL_PHY_LED0(gpio, mux_val, map_mask, map_val)	\
+	{								\
+		.name = (gpio),						\
+		.regmap[0] = {						\
+			AIROHA_FUNC_MUX,				\
+			REG_GPIO_2ND_I2C_MODE,				\
+			(mux_val),					\
+			(mux_val),					\
+		},							\
+		.regmap[1] = {						\
+			AIROHA_FUNC_MUX,				\
+			REG_LAN_LED0_MAPPING,				\
+			(map_mask),					\
+			(map_val),					\
+		},							\
+		.regmap_size = 2,					\
+	}
+
+#define AIROHA_PINCTRL_PHY_LED1(gpio, mux_val, map_mask, map_val)	\
+	{								\
+		.name = (gpio),						\
+		.regmap[0] = {						\
+			AIROHA_FUNC_MUX,				\
+			REG_GPIO_2ND_I2C_MODE,				\
+			(mux_val),					\
+			(mux_val),					\
+		},							\
+		.regmap[1] = {						\
+			AIROHA_FUNC_MUX,				\
+			REG_LAN_LED1_MAPPING,				\
+			(map_mask),					\
+			(map_val),					\
+		},							\
+		.regmap_size = 2,					\
+	}
+
+static struct pinctrl_pin_desc pinctrl_pins[] = {
+	PINCTRL_PIN(0, "uart1_txd"),
+	PINCTRL_PIN(1, "uart1_rxd"),
+	PINCTRL_PIN(2, "i2c_scl"),
+	PINCTRL_PIN(3, "i2c_sda"),
+	PINCTRL_PIN(4, "spi_cs0"),
+	PINCTRL_PIN(5, "spi_clk"),
+	PINCTRL_PIN(6, "spi_mosi"),
+	PINCTRL_PIN(7, "spi_miso"),
+	PINCTRL_PIN(13, "gpio0"),
+	PINCTRL_PIN(14, "gpio1"),
+	PINCTRL_PIN(15, "gpio2"),
+	PINCTRL_PIN(16, "gpio3"),
+	PINCTRL_PIN(17, "gpio4"),
+	PINCTRL_PIN(18, "gpio5"),
+	PINCTRL_PIN(19, "gpio6"),
+	PINCTRL_PIN(20, "gpio7"),
+	PINCTRL_PIN(21, "gpio8"),
+	PINCTRL_PIN(22, "gpio9"),
+	PINCTRL_PIN(23, "gpio10"),
+	PINCTRL_PIN(24, "gpio11"),
+	PINCTRL_PIN(25, "gpio12"),
+	PINCTRL_PIN(26, "gpio13"),
+	PINCTRL_PIN(27, "gpio14"),
+	PINCTRL_PIN(28, "gpio15"),
+	PINCTRL_PIN(29, "gpio16"),
+	PINCTRL_PIN(30, "gpio17"),
+	PINCTRL_PIN(31, "gpio18"),
+	PINCTRL_PIN(32, "gpio19"),
+	PINCTRL_PIN(33, "gpio20"),
+	PINCTRL_PIN(34, "gpio21"),
+	PINCTRL_PIN(35, "gpio22"),
+	PINCTRL_PIN(36, "gpio23"),
+	PINCTRL_PIN(37, "gpio24"),
+	PINCTRL_PIN(38, "gpio25"),
+	PINCTRL_PIN(39, "gpio26"),
+	PINCTRL_PIN(40, "gpio27"),
+	PINCTRL_PIN(41, "gpio28"),
+	PINCTRL_PIN(42, "gpio29"),
+	PINCTRL_PIN(43, "gpio30"),
+	PINCTRL_PIN(44, "gpio31"),
+	PINCTRL_PIN(45, "gpio32"),
+	PINCTRL_PIN(46, "gpio33"),
+	PINCTRL_PIN(47, "gpio34"),
+	PINCTRL_PIN(48, "gpio35"),
+	PINCTRL_PIN(49, "gpio36"),
+	PINCTRL_PIN(50, "gpio37"),
+	PINCTRL_PIN(51, "gpio38"),
+	PINCTRL_PIN(52, "gpio39"),
+	PINCTRL_PIN(53, "gpio40"),
+	PINCTRL_PIN(54, "gpio41"),
+	PINCTRL_PIN(55, "gpio42"),
+	PINCTRL_PIN(56, "gpio43"),
+	PINCTRL_PIN(57, "gpio44"),
+	PINCTRL_PIN(58, "gpio45"),
+	PINCTRL_PIN(59, "gpio46"),
+	PINCTRL_PIN(60, "pcie_reset0"),
+	PINCTRL_PIN(61, "pcie_reset1"),
+	PINCTRL_PIN(62, "pcie_reset2"),
+};
+
+static const int pon_pins[] = { 49, 50, 51, 52, 53, 54 };
+static const int pon_tod_1pps_pins[] = { 46 };
+static const int gsw_tod_1pps_pins[] = { 46 };
+static const int sipo_pins[] = { 16, 17 };
+static const int sipo_rclk_pins[] = { 16, 17, 43 };
+static const int mdio_pins[] = { 14, 15 };
+static const int uart2_pins[] = { 48, 55 };
+static const int uart2_cts_rts_pins[] = { 46, 47 };
+static const int hsuart_pins[] = { 28, 29 };
+static const int hsuart_cts_rts_pins[] = { 26, 27 };
+static const int uart4_pins[] = { 38, 39 };
+static const int uart5_pins[] = { 18, 19 };
+static const int i2c0_pins[] = { 2, 3 };
+static const int i2c1_pins[] = { 14, 15 };
+static const int jtag_udi_pins[] = { 16, 17, 18, 19, 20 };
+static const int jtag_dfd_pins[] = { 16, 17, 18, 19, 20 };
+static const int i2s_pins[] = { 26, 27, 28, 29 };
+static const int pcm1_pins[] = { 22, 23, 24, 25 };
+static const int pcm2_pins[] = { 18, 19, 20, 21 };
+static const int spi_quad_pins[] = { 32, 33 };
+static const int spi_pins[] = { 4, 5, 6, 7 };
+static const int spi_cs1_pins[] = { 34 };
+static const int pcm_spi_pins[] = { 18, 19, 20, 21, 22, 23, 24, 25 };
+static const int pcm_spi_int_pins[] = { 14 };
+static const int pcm_spi_rst_pins[] = { 15 };
+static const int pcm_spi_cs1_pins[] = { 43 };
+static const int pcm_spi_cs2_pins[] = { 40 };
+static const int pcm_spi_cs2_p128_pins[] = { 40 };
+static const int pcm_spi_cs2_p156_pins[] = { 40 };
+static const int pcm_spi_cs3_pins[] = { 41 };
+static const int pcm_spi_cs4_pins[] = { 42 };
+static const int emmc_pins[] = {
+	4, 5, 6, 30, 31, 32, 33, 34, 35, 36, 37
+};
+static const int pnand_pins[] = {
+	4, 5, 6, 7, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42
+};
+static const int gpio0_pins[] = { 13 };
+static const int gpio1_pins[] = { 14 };
+static const int gpio2_pins[] = { 15 };
+static const int gpio3_pins[] = { 16 };
+static const int gpio4_pins[] = { 17 };
+static const int gpio5_pins[] = { 18 };
+static const int gpio6_pins[] = { 19 };
+static const int gpio7_pins[] = { 20 };
+static const int gpio8_pins[] = { 21 };
+static const int gpio9_pins[] = { 22 };
+static const int gpio10_pins[] = { 23 };
+static const int gpio11_pins[] = { 24 };
+static const int gpio12_pins[] = { 25 };
+static const int gpio13_pins[] = { 26 };
+static const int gpio14_pins[] = { 27 };
+static const int gpio15_pins[] = { 28 };
+static const int gpio16_pins[] = { 29 };
+static const int gpio17_pins[] = { 30 };
+static const int gpio18_pins[] = { 31 };
+static const int gpio19_pins[] = { 32 };
+static const int gpio20_pins[] = { 33 };
+static const int gpio21_pins[] = { 34 };
+static const int gpio22_pins[] = { 35 };
+static const int gpio23_pins[] = { 36 };
+static const int gpio24_pins[] = { 37 };
+static const int gpio25_pins[] = { 38 };
+static const int gpio26_pins[] = { 39 };
+static const int gpio27_pins[] = { 40 };
+static const int gpio28_pins[] = { 41 };
+static const int gpio29_pins[] = { 42 };
+static const int gpio30_pins[] = { 43 };
+static const int gpio31_pins[] = { 44 };
+static const int gpio32_pins[] = { 45 };
+static const int gpio33_pins[] = { 46 };
+static const int gpio34_pins[] = { 47 };
+static const int gpio35_pins[] = { 48 };
+static const int gpio36_pins[] = { 49 };
+static const int gpio37_pins[] = { 50 };
+static const int gpio38_pins[] = { 51 };
+static const int gpio39_pins[] = { 52 };
+static const int gpio40_pins[] = { 53 };
+static const int gpio41_pins[] = { 54 };
+static const int gpio42_pins[] = { 55 };
+static const int gpio43_pins[] = { 56 };
+static const int gpio44_pins[] = { 57 };
+static const int gpio45_pins[] = { 58 };
+static const int gpio46_pins[] = { 59 };
+static const int gpio47_pins[] = { 60 };
+static const int gpio48_pins[] = { 61 };
+static const int gpio49_pins[] = { 62 };
+static const int pcie_reset0_pins[] = { 60 };
+static const int pcie_reset1_pins[] = { 61 };
+static const int pcie_reset2_pins[] = { 62 };
+
+static const struct pingroup pinctrl_groups[] = {
+	PINCTRL_PIN_GROUP("pon", pon),
+	PINCTRL_PIN_GROUP("pon_tod_1pps", pon_tod_1pps),
+	PINCTRL_PIN_GROUP("gsw_tod_1pps", gsw_tod_1pps),
+	PINCTRL_PIN_GROUP("sipo", sipo),
+	PINCTRL_PIN_GROUP("sipo_rclk", sipo_rclk),
+	PINCTRL_PIN_GROUP("mdio", mdio),
+	PINCTRL_PIN_GROUP("uart2", uart2),
+	PINCTRL_PIN_GROUP("uart2_cts_rts", uart2_cts_rts),
+	PINCTRL_PIN_GROUP("hsuart", hsuart),
+	PINCTRL_PIN_GROUP("hsuart_cts_rts", hsuart_cts_rts),
+	PINCTRL_PIN_GROUP("uart4", uart4),
+	PINCTRL_PIN_GROUP("uart5", uart5),
+	PINCTRL_PIN_GROUP("i2c0", i2c0),
+	PINCTRL_PIN_GROUP("i2c1", i2c1),
+	PINCTRL_PIN_GROUP("jtag_udi", jtag_udi),
+	PINCTRL_PIN_GROUP("jtag_dfd", jtag_dfd),
+	PINCTRL_PIN_GROUP("i2s", i2s),
+	PINCTRL_PIN_GROUP("pcm1", pcm1),
+	PINCTRL_PIN_GROUP("pcm2", pcm2),
+	PINCTRL_PIN_GROUP("spi", spi),
+	PINCTRL_PIN_GROUP("spi_quad", spi_quad),
+	PINCTRL_PIN_GROUP("spi_cs1", spi_cs1),
+	PINCTRL_PIN_GROUP("pcm_spi", pcm_spi),
+	PINCTRL_PIN_GROUP("pcm_spi_int", pcm_spi_int),
+	PINCTRL_PIN_GROUP("pcm_spi_rst", pcm_spi_rst),
+	PINCTRL_PIN_GROUP("pcm_spi_cs1", pcm_spi_cs1),
+	PINCTRL_PIN_GROUP("pcm_spi_cs2_p128", pcm_spi_cs2_p128),
+	PINCTRL_PIN_GROUP("pcm_spi_cs2_p156", pcm_spi_cs2_p156),
+	PINCTRL_PIN_GROUP("pcm_spi_cs2", pcm_spi_cs2),
+	PINCTRL_PIN_GROUP("pcm_spi_cs3", pcm_spi_cs3),
+	PINCTRL_PIN_GROUP("pcm_spi_cs4", pcm_spi_cs4),
+	PINCTRL_PIN_GROUP("emmc", emmc),
+	PINCTRL_PIN_GROUP("pnand", pnand),
+	PINCTRL_PIN_GROUP("gpio0", gpio0),
+	PINCTRL_PIN_GROUP("gpio1", gpio1),
+	PINCTRL_PIN_GROUP("gpio2", gpio2),
+	PINCTRL_PIN_GROUP("gpio3", gpio3),
+	PINCTRL_PIN_GROUP("gpio4", gpio4),
+	PINCTRL_PIN_GROUP("gpio5", gpio5),
+	PINCTRL_PIN_GROUP("gpio6", gpio6),
+	PINCTRL_PIN_GROUP("gpio7", gpio7),
+	PINCTRL_PIN_GROUP("gpio8", gpio8),
+	PINCTRL_PIN_GROUP("gpio9", gpio9),
+	PINCTRL_PIN_GROUP("gpio10", gpio10),
+	PINCTRL_PIN_GROUP("gpio11", gpio11),
+	PINCTRL_PIN_GROUP("gpio12", gpio12),
+	PINCTRL_PIN_GROUP("gpio13", gpio13),
+	PINCTRL_PIN_GROUP("gpio14", gpio14),
+	PINCTRL_PIN_GROUP("gpio15", gpio15),
+	PINCTRL_PIN_GROUP("gpio16", gpio16),
+	PINCTRL_PIN_GROUP("gpio17", gpio17),
+	PINCTRL_PIN_GROUP("gpio18", gpio18),
+	PINCTRL_PIN_GROUP("gpio19", gpio19),
+	PINCTRL_PIN_GROUP("gpio20", gpio20),
+	PINCTRL_PIN_GROUP("gpio21", gpio21),
+	PINCTRL_PIN_GROUP("gpio22", gpio22),
+	PINCTRL_PIN_GROUP("gpio23", gpio23),
+	PINCTRL_PIN_GROUP("gpio24", gpio24),
+	PINCTRL_PIN_GROUP("gpio25", gpio25),
+	PINCTRL_PIN_GROUP("gpio26", gpio26),
+	PINCTRL_PIN_GROUP("gpio27", gpio27),
+	PINCTRL_PIN_GROUP("gpio28", gpio28),
+	PINCTRL_PIN_GROUP("gpio29", gpio29),
+	PINCTRL_PIN_GROUP("gpio30", gpio30),
+	PINCTRL_PIN_GROUP("gpio31", gpio31),
+	PINCTRL_PIN_GROUP("gpio32", gpio32),
+	PINCTRL_PIN_GROUP("gpio33", gpio33),
+	PINCTRL_PIN_GROUP("gpio34", gpio34),
+	PINCTRL_PIN_GROUP("gpio35", gpio35),
+	PINCTRL_PIN_GROUP("gpio36", gpio36),
+	PINCTRL_PIN_GROUP("gpio37", gpio37),
+	PINCTRL_PIN_GROUP("gpio38", gpio38),
+	PINCTRL_PIN_GROUP("gpio39", gpio39),
+	PINCTRL_PIN_GROUP("gpio40", gpio40),
+	PINCTRL_PIN_GROUP("gpio41", gpio41),
+	PINCTRL_PIN_GROUP("gpio42", gpio42),
+	PINCTRL_PIN_GROUP("gpio43", gpio43),
+	PINCTRL_PIN_GROUP("gpio44", gpio44),
+	PINCTRL_PIN_GROUP("gpio45", gpio45),
+	PINCTRL_PIN_GROUP("gpio46", gpio46),
+	PINCTRL_PIN_GROUP("gpio47", gpio47),
+	PINCTRL_PIN_GROUP("gpio48", gpio48),
+	PINCTRL_PIN_GROUP("gpio49", gpio49),
+	PINCTRL_PIN_GROUP("pcie_reset0", pcie_reset0),
+	PINCTRL_PIN_GROUP("pcie_reset1", pcie_reset1),
+	PINCTRL_PIN_GROUP("pcie_reset2", pcie_reset2),
+};
+
+static const char *const pon_groups[] = { "pon" };
+static const char *const tod_1pps_groups[] = {
+	"pon_tod_1pps", "gsw_tod_1pps"
+};
+static const char *const sipo_groups[] = { "sipo", "sipo_rclk" };
+static const char *const mdio_groups[] = { "mdio" };
+static const char *const uart_groups[] = {
+	"uart2", "uart2_cts_rts", "hsuart", "hsuart_cts_rts",
+	"uart4", "uart5"
+};
+static const char *const i2c_groups[] = { "i2c1" };
+static const char *const jtag_groups[] = { "jtag_udi", "jtag_dfd" };
+static const char *const pcm_groups[] = { "pcm1", "pcm2" };
+static const char *const spi_groups[] = { "spi_quad", "spi_cs1" };
+static const char *const pcm_spi_groups[] = {
+	"pcm_spi", "pcm_spi_int", "pcm_spi_rst", "pcm_spi_cs1",
+	"pcm_spi_cs2_p156", "pcm_spi_cs2_p128", "pcm_spi_cs3",
+	"pcm_spi_cs4"
+};
+static const char *const i2s_groups[] = { "i2s" };
+static const char *const emmc_groups[] = { "emmc" };
+static const char *const pnand_groups[] = { "pnand" };
+static const char *const gpio_groups[] = { "gpio47", "gpio48", "gpio49" };
+static const char *const pcie_reset_groups[] = {
+	"pcie_reset0", "pcie_reset1", "pcie_reset2"
+};
+static const char *const pwm_groups[] = {
+	"gpio0",  "gpio1",  "gpio2",  "gpio3",  "gpio4",  "gpio5",
+	"gpio6",  "gpio7",  "gpio8",  "gpio9",  "gpio10", "gpio11",
+	"gpio12", "gpio13", "gpio14", "gpio15", "gpio16", "gpio17",
+	"gpio18", "gpio19", "gpio20", "gpio21", "gpio22", "gpio23",
+	"gpio24", "gpio25", "gpio26", "gpio27", "gpio28", "gpio29",
+	"gpio30", "gpio31", "gpio36", "gpio37", "gpio38", "gpio39",
+	"gpio40", "gpio41", "gpio42", "gpio43", "gpio44", "gpio45",
+	"gpio46", "gpio47", "gpio48", "gpio49"
+};
+static const char *const phy1_led0_groups[] = {
+	"gpio33", "gpio34", "gpio35", "gpio42"
+};
+static const char *const phy2_led0_groups[] = {
+	"gpio33", "gpio34", "gpio35", "gpio42"
+};
+static const char *const phy3_led0_groups[] = {
+	"gpio33", "gpio34", "gpio35", "gpio42"
+};
+static const char *const phy4_led0_groups[] = {
+	"gpio33", "gpio34", "gpio35", "gpio42"
+};
+static const char *const phy1_led1_groups[] = {
+	"gpio43", "gpio44", "gpio45", "gpio46"
+};
+static const char *const phy2_led1_groups[] = {
+	"gpio43", "gpio44", "gpio45", "gpio46"
+};
+static const char *const phy3_led1_groups[] = {
+	"gpio43", "gpio44", "gpio45", "gpio46"
+};
+static const char *const phy4_led1_groups[] = {
+	"gpio43", "gpio44", "gpio45", "gpio46"
+};
+
+static const struct airoha_pinctrl_func_group pon_func_group[] = {
+	{
+		.name = "pon",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_PON_MODE_MASK,
+			GPIO_PON_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group tod_1pps_func_group[] = {
+	{
+		.name = "pon_tod_1pps",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_2ND_I2C_MODE,
+			PON_TOD_1PPS_MODE_MASK,
+			PON_TOD_1PPS_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "gsw_tod_1pps",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_2ND_I2C_MODE,
+			GSW_TOD_1PPS_MODE_MASK,
+			GSW_TOD_1PPS_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group sipo_func_group[] = {
+	{
+		.name = "sipo",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_SIPO_MODE_MASK | SIPO_RCLK_MODE_MASK,
+			GPIO_SIPO_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "sipo_rclk",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_SIPO_MODE_MASK | SIPO_RCLK_MODE_MASK,
+			GPIO_SIPO_MODE_MASK | SIPO_RCLK_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group mdio_func_group[] = {
+	{
+		.name = "mdio",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_2ND_I2C_MODE,
+			GPIO_MDC_IO_MASTER_MODE_MASK,
+			GPIO_MDC_IO_MASTER_MODE_MASK
+		},
+		.regmap[1] = {
+			AIROHA_FUNC_MUX,
+			REG_FORCE_GPIO_EN,
+			FORCE_GPIO_EN(1) | FORCE_GPIO_EN(2),
+			FORCE_GPIO_EN(1) | FORCE_GPIO_EN(2)
+		},
+		.regmap_size = 2,
+	},
+};
+
+static const struct airoha_pinctrl_func_group uart_func_group[] = {
+	{
+		.name = "uart2",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_UART2_MODE_MASK,
+			GPIO_UART2_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "uart2_cts_rts",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_UART2_MODE_MASK | GPIO_UART2_CTS_RTS_MODE_MASK,
+			GPIO_UART2_MODE_MASK | GPIO_UART2_CTS_RTS_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "hsuart",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_HSUART_MODE_MASK | GPIO_HSUART_CTS_RTS_MODE_MASK,
+			GPIO_HSUART_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+	{
+		.name = "hsuart_cts_rts",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_HSUART_MODE_MASK | GPIO_HSUART_CTS_RTS_MODE_MASK,
+			GPIO_HSUART_MODE_MASK | GPIO_HSUART_CTS_RTS_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "uart4",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_UART4_MODE_MASK,
+			GPIO_UART4_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "uart5",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_UART5_MODE_MASK,
+			GPIO_UART5_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group i2c_func_group[] = {
+	{
+		.name = "i2c1",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_2ND_I2C_MODE,
+			GPIO_2ND_I2C_MODE_MASK,
+			GPIO_2ND_I2C_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group jtag_func_group[] = {
+	{
+		.name = "jtag_udi",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_NPU_UART_EN,
+			JTAG_UDI_EN_MASK,
+			JTAG_UDI_EN_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "jtag_dfd",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_NPU_UART_EN,
+			JTAG_DFD_EN_MASK,
+			JTAG_DFD_EN_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group pcm_func_group[] = {
+	{
+		.name = "pcm1",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM1_MODE_MASK,
+			GPIO_PCM1_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcm2",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM2_MODE_MASK,
+			GPIO_PCM2_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group spi_func_group[] = {
+	{
+		.name = "spi_quad",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_SPI_QUAD_MODE_MASK,
+			GPIO_SPI_QUAD_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "spi_cs1",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_SPI_CS1_MODE_MASK,
+			GPIO_SPI_CS1_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "spi_cs2",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_SPI_CS2_MODE_MASK,
+			GPIO_SPI_CS2_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "spi_cs3",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_SPI_CS3_MODE_MASK,
+			GPIO_SPI_CS3_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "spi_cs4",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_SPI_CS4_MODE_MASK,
+			GPIO_SPI_CS4_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group pcm_spi_func_group[] = {
+	{
+		.name = "pcm_spi",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM_SPI_MODE_MASK,
+			GPIO_PCM_SPI_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcm_spi_int",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM_INT_MODE_MASK,
+			GPIO_PCM_INT_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcm_spi_rst",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM_RESET_MODE_MASK,
+			GPIO_PCM_RESET_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcm_spi_cs1",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM_SPI_CS1_MODE_MASK,
+			GPIO_PCM_SPI_CS1_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcm_spi_cs2_p128",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM_SPI_CS2_MODE_P128_MASK,
+			GPIO_PCM_SPI_CS2_MODE_P128_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcm_spi_cs2_p156",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM_SPI_CS2_MODE_P156_MASK,
+			GPIO_PCM_SPI_CS2_MODE_P156_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcm_spi_cs3",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM_SPI_CS3_MODE_MASK,
+			GPIO_PCM_SPI_CS3_MODE_MASK
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcm_spi_cs4",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_SPI_CS1_MODE,
+			GPIO_PCM_SPI_CS4_MODE_MASK,
+			GPIO_PCM_SPI_CS4_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group i2s_func_group[] = {
+	{
+		.name = "i2s",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_2ND_I2C_MODE,
+			GPIO_I2S_MODE_MASK,
+			GPIO_I2S_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group emmc_func_group[] = {
+	{
+		.name = "emmc",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_EMMC_MODE_MASK,
+			GPIO_EMMC_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group pnand_func_group[] = {
+	{
+		.name = "pnand",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_PARALLEL_NAND_MODE_MASK,
+			GPIO_PARALLEL_NAND_MODE_MASK
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group gpio_func_group[] = {
+	AIROHA_PINCTRL_GPIO_EXT("gpio47", GPIO47_FLASH_MODE_CFG,
+				GPIO_PCIE_RESET0_MASK),
+	AIROHA_PINCTRL_GPIO_EXT("gpio48", GPIO48_FLASH_MODE_CFG,
+				GPIO_PCIE_RESET1_MASK),
+	AIROHA_PINCTRL_GPIO_EXT("gpio49", GPIO49_FLASH_MODE_CFG,
+				GPIO_PCIE_RESET2_MASK),
+};
+
+static const struct airoha_pinctrl_func_group pcie_reset_func_group[] = {
+	{
+		.name = "pcie_reset0",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_PCIE_RESET0_MASK,
+			0
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcie_reset1",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_PCIE_RESET1_MASK,
+			0
+		},
+		.regmap_size = 1,
+	}, {
+		.name = "pcie_reset2",
+		.regmap[0] = {
+			AIROHA_FUNC_MUX,
+			REG_GPIO_PON_MODE,
+			GPIO_PCIE_RESET2_MASK,
+			0
+		},
+		.regmap_size = 1,
+	},
+};
+
+static const struct airoha_pinctrl_func_group pwm_func_group[] = {
+	AIROHA_PINCTRL_PWM("gpio0", GPIO0_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio1", GPIO1_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio2", GPIO2_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio3", GPIO3_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio4", GPIO4_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio5", GPIO5_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio6", GPIO6_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio7", GPIO7_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio8", GPIO8_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio9", GPIO9_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio10", GPIO10_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio11", GPIO11_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio12", GPIO12_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio13", GPIO13_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio14", GPIO14_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM("gpio15", GPIO15_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio16", GPIO16_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio17", GPIO17_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio18", GPIO18_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio19", GPIO19_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio20", GPIO20_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio21", GPIO21_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio22", GPIO22_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio23", GPIO23_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio24", GPIO24_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio25", GPIO25_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio26", GPIO26_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio27", GPIO27_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio28", GPIO28_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio29", GPIO29_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio30", GPIO30_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio31", GPIO31_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio36", GPIO36_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio37", GPIO37_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio38", GPIO38_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio39", GPIO39_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio40", GPIO40_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio41", GPIO41_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio42", GPIO42_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio43", GPIO43_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio44", GPIO44_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio45", GPIO45_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT("gpio46", GPIO46_FLASH_MODE_CFG),
+	AIROHA_PINCTRL_PWM_EXT_SEC("gpio47", GPIO47_FLASH_MODE_CFG,
+				   GPIO_PCIE_RESET0_MASK),
+	AIROHA_PINCTRL_PWM_EXT_SEC("gpio48", GPIO48_FLASH_MODE_CFG,
+				   GPIO_PCIE_RESET1_MASK),
+	AIROHA_PINCTRL_PWM_EXT_SEC("gpio49", GPIO49_FLASH_MODE_CFG,
+				   GPIO_PCIE_RESET2_MASK),
+};
+
+static const struct airoha_pinctrl_func_group phy1_led0_func_group[] = {
+	AIROHA_PINCTRL_PHY_LED0("gpio33", GPIO_LAN0_LED0_MODE_MASK,
+				LAN0_LED_MAPPING_MASK, LAN0_PHY_LED_MAP(0)),
+	AIROHA_PINCTRL_PHY_LED0("gpio34", GPIO_LAN1_LED0_MODE_MASK,
+				LAN1_LED_MAPPING_MASK, LAN1_PHY_LED_MAP(0)),
+	AIROHA_PINCTRL_PHY_LED0("gpio35", GPIO_LAN2_LED0_MODE_MASK,
+				LAN2_LED_MAPPING_MASK, LAN2_PHY_LED_MAP(0)),
+	AIROHA_PINCTRL_PHY_LED0("gpio42", GPIO_LAN3_LED0_MODE_MASK,
+				LAN3_LED_MAPPING_MASK, LAN3_PHY_LED_MAP(0)),
+};
+
+static const struct airoha_pinctrl_func_group phy2_led0_func_group[] = {
+	AIROHA_PINCTRL_PHY_LED0("gpio33", GPIO_LAN0_LED0_MODE_MASK,
+				LAN0_LED_MAPPING_MASK, LAN0_PHY_LED_MAP(1)),
+	AIROHA_PINCTRL_PHY_LED0("gpio34", GPIO_LAN1_LED0_MODE_MASK,
+				LAN1_LED_MAPPING_MASK, LAN1_PHY_LED_MAP(1)),
+	AIROHA_PINCTRL_PHY_LED0("gpio35", GPIO_LAN2_LED0_MODE_MASK,
+				LAN2_LED_MAPPING_MASK, LAN2_PHY_LED_MAP(1)),
+	AIROHA_PINCTRL_PHY_LED0("gpio42", GPIO_LAN3_LED0_MODE_MASK,
+				LAN3_LED_MAPPING_MASK, LAN3_PHY_LED_MAP(1)),
+};
+
+static const struct airoha_pinctrl_func_group phy3_led0_func_group[] = {
+	AIROHA_PINCTRL_PHY_LED0("gpio33", GPIO_LAN0_LED0_MODE_MASK,
+				LAN0_LED_MAPPING_MASK, LAN0_PHY_LED_MAP(2)),
+	AIROHA_PINCTRL_PHY_LED0("gpio34", GPIO_LAN1_LED0_MODE_MASK,
+				LAN1_LED_MAPPING_MASK, LAN1_PHY_LED_MAP(2)),
+	AIROHA_PINCTRL_PHY_LED0("gpio35", GPIO_LAN2_LED0_MODE_MASK,
+				LAN2_LED_MAPPING_MASK, LAN2_PHY_LED_MAP(2)),
+	AIROHA_PINCTRL_PHY_LED0("gpio42", GPIO_LAN3_LED0_MODE_MASK,
+				LAN3_LED_MAPPING_MASK, LAN3_PHY_LED_MAP(2)),
+};
+
+static const struct airoha_pinctrl_func_group phy4_led0_func_group[] = {
+	AIROHA_PINCTRL_PHY_LED0("gpio33", GPIO_LAN0_LED0_MODE_MASK,
+				LAN0_LED_MAPPING_MASK, LAN0_PHY_LED_MAP(3)),
+	AIROHA_PINCTRL_PHY_LED0("gpio34", GPIO_LAN1_LED0_MODE_MASK,
+				LAN1_LED_MAPPING_MASK, LAN1_PHY_LED_MAP(3)),
+	AIROHA_PINCTRL_PHY_LED0("gpio35", GPIO_LAN2_LED0_MODE_MASK,
+				LAN2_LED_MAPPING_MASK, LAN2_PHY_LED_MAP(3)),
+	AIROHA_PINCTRL_PHY_LED0("gpio42", GPIO_LAN3_LED0_MODE_MASK,
+				LAN3_LED_MAPPING_MASK, LAN3_PHY_LED_MAP(3)),
+};
+
+static const struct airoha_pinctrl_func_group phy1_led1_func_group[] = {
+	AIROHA_PINCTRL_PHY_LED1("gpio43", GPIO_LAN0_LED1_MODE_MASK,
+				LAN0_LED_MAPPING_MASK, LAN0_PHY_LED_MAP(0)),
+	AIROHA_PINCTRL_PHY_LED1("gpio44", GPIO_LAN1_LED1_MODE_MASK,
+				LAN1_LED_MAPPING_MASK, LAN1_PHY_LED_MAP(0)),
+	AIROHA_PINCTRL_PHY_LED1("gpio45", GPIO_LAN2_LED1_MODE_MASK,
+				LAN2_LED_MAPPING_MASK, LAN2_PHY_LED_MAP(0)),
+	AIROHA_PINCTRL_PHY_LED1("gpio46", GPIO_LAN3_LED1_MODE_MASK,
+				LAN3_LED_MAPPING_MASK, LAN3_PHY_LED_MAP(0)),
+};
+
+static const struct airoha_pinctrl_func_group phy2_led1_func_group[] = {
+	AIROHA_PINCTRL_PHY_LED1("gpio43", GPIO_LAN0_LED1_MODE_MASK,
+				LAN0_LED_MAPPING_MASK, LAN0_PHY_LED_MAP(1)),
+	AIROHA_PINCTRL_PHY_LED1("gpio44", GPIO_LAN1_LED1_MODE_MASK,
+				LAN1_LED_MAPPING_MASK, LAN1_PHY_LED_MAP(1)),
+	AIROHA_PINCTRL_PHY_LED1("gpio45", GPIO_LAN2_LED1_MODE_MASK,
+				LAN2_LED_MAPPING_MASK, LAN2_PHY_LED_MAP(1)),
+	AIROHA_PINCTRL_PHY_LED1("gpio46", GPIO_LAN3_LED1_MODE_MASK,
+				LAN3_LED_MAPPING_MASK, LAN3_PHY_LED_MAP(1)),
+};
+
+static const struct airoha_pinctrl_func_group phy3_led1_func_group[] = {
+	AIROHA_PINCTRL_PHY_LED1("gpio43", GPIO_LAN0_LED1_MODE_MASK,
+				LAN0_LED_MAPPING_MASK, LAN0_PHY_LED_MAP(2)),
+	AIROHA_PINCTRL_PHY_LED1("gpio44", GPIO_LAN1_LED1_MODE_MASK,
+				LAN1_LED_MAPPING_MASK, LAN1_PHY_LED_MAP(2)),
+	AIROHA_PINCTRL_PHY_LED1("gpio45", GPIO_LAN2_LED1_MODE_MASK,
+				LAN2_LED_MAPPING_MASK, LAN2_PHY_LED_MAP(2)),
+	AIROHA_PINCTRL_PHY_LED1("gpio46", GPIO_LAN3_LED1_MODE_MASK,
+				LAN3_LED_MAPPING_MASK, LAN3_PHY_LED_MAP(2)),
+};
+
+static const struct airoha_pinctrl_func_group phy4_led1_func_group[] = {
+	AIROHA_PINCTRL_PHY_LED1("gpio43", GPIO_LAN0_LED1_MODE_MASK,
+				LAN0_LED_MAPPING_MASK, LAN0_PHY_LED_MAP(3)),
+	AIROHA_PINCTRL_PHY_LED1("gpio44", GPIO_LAN1_LED1_MODE_MASK,
+				LAN1_LED_MAPPING_MASK, LAN1_PHY_LED_MAP(3)),
+	AIROHA_PINCTRL_PHY_LED1("gpio45", GPIO_LAN2_LED1_MODE_MASK,
+				LAN2_LED_MAPPING_MASK, LAN2_PHY_LED_MAP(3)),
+	AIROHA_PINCTRL_PHY_LED1("gpio46", GPIO_LAN3_LED1_MODE_MASK,
+				LAN3_LED_MAPPING_MASK, LAN3_PHY_LED_MAP(3)),
+};
+
+static const struct airoha_pinctrl_func pinctrl_funcs[] = {
+	PINCTRL_FUNC_DESC("pon", pon),
+	PINCTRL_FUNC_DESC("tod_1pps", tod_1pps),
+	PINCTRL_FUNC_DESC("sipo", sipo),
+	PINCTRL_FUNC_DESC("mdio", mdio),
+	PINCTRL_FUNC_DESC("uart", uart),
+	PINCTRL_FUNC_DESC("i2c", i2c),
+	PINCTRL_FUNC_DESC("jtag", jtag),
+	PINCTRL_FUNC_DESC("pcm", pcm),
+	PINCTRL_FUNC_DESC("spi", spi),
+	PINCTRL_FUNC_DESC("pcm_spi", pcm_spi),
+	PINCTRL_FUNC_DESC("i2s", i2s),
+	PINCTRL_FUNC_DESC("emmc", emmc),
+	PINCTRL_FUNC_DESC("pnand", pnand),
+	PINCTRL_FUNC_DESC("gpio", gpio),
+	PINCTRL_FUNC_DESC("pcie_reset", pcie_reset),
+	PINCTRL_FUNC_DESC("pwm", pwm),
+	PINCTRL_FUNC_DESC("phy1_led0", phy1_led0),
+	PINCTRL_FUNC_DESC("phy2_led0", phy2_led0),
+	PINCTRL_FUNC_DESC("phy3_led0", phy3_led0),
+	PINCTRL_FUNC_DESC("phy4_led0", phy4_led0),
+	PINCTRL_FUNC_DESC("phy1_led1", phy1_led1),
+	PINCTRL_FUNC_DESC("phy2_led1", phy2_led1),
+	PINCTRL_FUNC_DESC("phy3_led1", phy3_led1),
+	PINCTRL_FUNC_DESC("phy4_led1", phy4_led1),
+};
+
+static const struct airoha_pinctrl_conf pinctrl_pullup_conf[] = {
+	PINCTRL_CONF_DESC(0, REG_I2C_SDA_PU, UART1_TXD_PU_MASK),
+	PINCTRL_CONF_DESC(1, REG_I2C_SDA_PU, UART1_RXD_PU_MASK),
+	PINCTRL_CONF_DESC(2, REG_I2C_SDA_PU, I2C_SDA_PU_MASK),
+	PINCTRL_CONF_DESC(3, REG_I2C_SDA_PU, I2C_SCL_PU_MASK),
+	PINCTRL_CONF_DESC(4, REG_I2C_SDA_PU, SPI_CS0_PU_MASK),
+	PINCTRL_CONF_DESC(5, REG_I2C_SDA_PU, SPI_CLK_PU_MASK),
+	PINCTRL_CONF_DESC(6, REG_I2C_SDA_PU, SPI_MOSI_PU_MASK),
+	PINCTRL_CONF_DESC(7, REG_I2C_SDA_PU, SPI_MISO_PU_MASK),
+	PINCTRL_CONF_DESC(13, REG_GPIO_L_PU, BIT(0)),
+	PINCTRL_CONF_DESC(14, REG_GPIO_L_PU, BIT(1)),
+	PINCTRL_CONF_DESC(15, REG_GPIO_L_PU, BIT(2)),
+	PINCTRL_CONF_DESC(16, REG_GPIO_L_PU, BIT(3)),
+	PINCTRL_CONF_DESC(17, REG_GPIO_L_PU, BIT(4)),
+	PINCTRL_CONF_DESC(18, REG_GPIO_L_PU, BIT(5)),
+	PINCTRL_CONF_DESC(19, REG_GPIO_L_PU, BIT(6)),
+	PINCTRL_CONF_DESC(20, REG_GPIO_L_PU, BIT(7)),
+	PINCTRL_CONF_DESC(21, REG_GPIO_L_PU, BIT(8)),
+	PINCTRL_CONF_DESC(22, REG_GPIO_L_PU, BIT(9)),
+	PINCTRL_CONF_DESC(23, REG_GPIO_L_PU, BIT(10)),
+	PINCTRL_CONF_DESC(24, REG_GPIO_L_PU, BIT(11)),
+	PINCTRL_CONF_DESC(25, REG_GPIO_L_PU, BIT(12)),
+	PINCTRL_CONF_DESC(26, REG_GPIO_L_PU, BIT(13)),
+	PINCTRL_CONF_DESC(27, REG_GPIO_L_PU, BIT(14)),
+	PINCTRL_CONF_DESC(28, REG_GPIO_L_PU, BIT(15)),
+	PINCTRL_CONF_DESC(29, REG_GPIO_L_PU, BIT(16)),
+	PINCTRL_CONF_DESC(30, REG_GPIO_L_PU, BIT(17)),
+	PINCTRL_CONF_DESC(31, REG_GPIO_L_PU, BIT(18)),
+	PINCTRL_CONF_DESC(32, REG_GPIO_L_PU, BIT(19)),
+	PINCTRL_CONF_DESC(33, REG_GPIO_L_PU, BIT(20)),
+	PINCTRL_CONF_DESC(34, REG_GPIO_L_PU, BIT(21)),
+	PINCTRL_CONF_DESC(35, REG_GPIO_L_PU, BIT(22)),
+	PINCTRL_CONF_DESC(36, REG_GPIO_L_PU, BIT(23)),
+	PINCTRL_CONF_DESC(37, REG_GPIO_L_PU, BIT(24)),
+	PINCTRL_CONF_DESC(38, REG_GPIO_L_PU, BIT(25)),
+	PINCTRL_CONF_DESC(39, REG_GPIO_L_PU, BIT(26)),
+	PINCTRL_CONF_DESC(40, REG_GPIO_L_PU, BIT(27)),
+	PINCTRL_CONF_DESC(41, REG_GPIO_L_PU, BIT(28)),
+	PINCTRL_CONF_DESC(42, REG_GPIO_L_PU, BIT(29)),
+	PINCTRL_CONF_DESC(43, REG_GPIO_L_PU, BIT(30)),
+	PINCTRL_CONF_DESC(44, REG_GPIO_L_PU, BIT(31)),
+	PINCTRL_CONF_DESC(45, REG_GPIO_H_PU, BIT(0)),
+	PINCTRL_CONF_DESC(46, REG_GPIO_H_PU, BIT(1)),
+	PINCTRL_CONF_DESC(47, REG_GPIO_H_PU, BIT(2)),
+	PINCTRL_CONF_DESC(48, REG_GPIO_H_PU, BIT(3)),
+	PINCTRL_CONF_DESC(49, REG_GPIO_H_PU, BIT(4)),
+	PINCTRL_CONF_DESC(50, REG_GPIO_H_PU, BIT(5)),
+	PINCTRL_CONF_DESC(51, REG_GPIO_H_PU, BIT(6)),
+	PINCTRL_CONF_DESC(52, REG_GPIO_H_PU, BIT(7)),
+	PINCTRL_CONF_DESC(53, REG_GPIO_H_PU, BIT(8)),
+	PINCTRL_CONF_DESC(54, REG_GPIO_H_PU, BIT(9)),
+	PINCTRL_CONF_DESC(55, REG_GPIO_H_PU, BIT(10)),
+	PINCTRL_CONF_DESC(56, REG_GPIO_H_PU, BIT(11)),
+	PINCTRL_CONF_DESC(57, REG_GPIO_H_PU, BIT(12)),
+	PINCTRL_CONF_DESC(58, REG_GPIO_H_PU, BIT(13)),
+	PINCTRL_CONF_DESC(59, REG_GPIO_H_PU, BIT(14)),
+	PINCTRL_CONF_DESC(60, REG_I2C_SDA_PU, PCIE0_RESET_PU_MASK),
+	PINCTRL_CONF_DESC(61, REG_I2C_SDA_PU, PCIE1_RESET_PU_MASK),
+	PINCTRL_CONF_DESC(62, REG_I2C_SDA_PU, PCIE2_RESET_PU_MASK),
+};
+
+static const struct airoha_pinctrl_conf pinctrl_pulldown_conf[] = {
+	PINCTRL_CONF_DESC(0, REG_I2C_SDA_PD, UART1_TXD_PD_MASK),
+	PINCTRL_CONF_DESC(1, REG_I2C_SDA_PD, UART1_RXD_PD_MASK),
+	PINCTRL_CONF_DESC(2, REG_I2C_SDA_PD, I2C_SDA_PD_MASK),
+	PINCTRL_CONF_DESC(3, REG_I2C_SDA_PD, I2C_SCL_PD_MASK),
+	PINCTRL_CONF_DESC(4, REG_I2C_SDA_PD, SPI_CS0_PD_MASK),
+	PINCTRL_CONF_DESC(5, REG_I2C_SDA_PD, SPI_CLK_PD_MASK),
+	PINCTRL_CONF_DESC(6, REG_I2C_SDA_PD, SPI_MOSI_PD_MASK),
+	PINCTRL_CONF_DESC(7, REG_I2C_SDA_PD, SPI_MISO_PD_MASK),
+	PINCTRL_CONF_DESC(13, REG_GPIO_L_PD, BIT(0)),
+	PINCTRL_CONF_DESC(14, REG_GPIO_L_PD, BIT(1)),
+	PINCTRL_CONF_DESC(15, REG_GPIO_L_PD, BIT(2)),
+	PINCTRL_CONF_DESC(16, REG_GPIO_L_PD, BIT(3)),
+	PINCTRL_CONF_DESC(17, REG_GPIO_L_PD, BIT(4)),
+	PINCTRL_CONF_DESC(18, REG_GPIO_L_PD, BIT(5)),
+	PINCTRL_CONF_DESC(19, REG_GPIO_L_PD, BIT(6)),
+	PINCTRL_CONF_DESC(20, REG_GPIO_L_PD, BIT(7)),
+	PINCTRL_CONF_DESC(21, REG_GPIO_L_PD, BIT(8)),
+	PINCTRL_CONF_DESC(22, REG_GPIO_L_PD, BIT(9)),
+	PINCTRL_CONF_DESC(23, REG_GPIO_L_PD, BIT(10)),
+	PINCTRL_CONF_DESC(24, REG_GPIO_L_PD, BIT(11)),
+	PINCTRL_CONF_DESC(25, REG_GPIO_L_PD, BIT(12)),
+	PINCTRL_CONF_DESC(26, REG_GPIO_L_PD, BIT(13)),
+	PINCTRL_CONF_DESC(27, REG_GPIO_L_PD, BIT(14)),
+	PINCTRL_CONF_DESC(28, REG_GPIO_L_PD, BIT(15)),
+	PINCTRL_CONF_DESC(29, REG_GPIO_L_PD, BIT(16)),
+	PINCTRL_CONF_DESC(30, REG_GPIO_L_PD, BIT(17)),
+	PINCTRL_CONF_DESC(31, REG_GPIO_L_PD, BIT(18)),
+	PINCTRL_CONF_DESC(32, REG_GPIO_L_PD, BIT(19)),
+	PINCTRL_CONF_DESC(33, REG_GPIO_L_PD, BIT(20)),
+	PINCTRL_CONF_DESC(34, REG_GPIO_L_PD, BIT(21)),
+	PINCTRL_CONF_DESC(35, REG_GPIO_L_PD, BIT(22)),
+	PINCTRL_CONF_DESC(36, REG_GPIO_L_PD, BIT(23)),
+	PINCTRL_CONF_DESC(37, REG_GPIO_L_PD, BIT(24)),
+	PINCTRL_CONF_DESC(38, REG_GPIO_L_PD, BIT(25)),
+	PINCTRL_CONF_DESC(39, REG_GPIO_L_PD, BIT(26)),
+	PINCTRL_CONF_DESC(40, REG_GPIO_L_PD, BIT(27)),
+	PINCTRL_CONF_DESC(41, REG_GPIO_L_PD, BIT(28)),
+	PINCTRL_CONF_DESC(42, REG_GPIO_L_PD, BIT(29)),
+	PINCTRL_CONF_DESC(43, REG_GPIO_L_PD, BIT(30)),
+	PINCTRL_CONF_DESC(44, REG_GPIO_L_PD, BIT(31)),
+	PINCTRL_CONF_DESC(45, REG_GPIO_H_PD, BIT(0)),
+	PINCTRL_CONF_DESC(46, REG_GPIO_H_PD, BIT(1)),
+	PINCTRL_CONF_DESC(47, REG_GPIO_H_PD, BIT(2)),
+	PINCTRL_CONF_DESC(48, REG_GPIO_H_PD, BIT(3)),
+	PINCTRL_CONF_DESC(49, REG_GPIO_H_PD, BIT(4)),
+	PINCTRL_CONF_DESC(50, REG_GPIO_H_PD, BIT(5)),
+	PINCTRL_CONF_DESC(51, REG_GPIO_H_PD, BIT(6)),
+	PINCTRL_CONF_DESC(52, REG_GPIO_H_PD, BIT(7)),
+	PINCTRL_CONF_DESC(53, REG_GPIO_H_PD, BIT(8)),
+	PINCTRL_CONF_DESC(54, REG_GPIO_H_PD, BIT(9)),
+	PINCTRL_CONF_DESC(55, REG_GPIO_H_PD, BIT(10)),
+	PINCTRL_CONF_DESC(56, REG_GPIO_H_PD, BIT(11)),
+	PINCTRL_CONF_DESC(57, REG_GPIO_H_PD, BIT(12)),
+	PINCTRL_CONF_DESC(58, REG_GPIO_H_PD, BIT(13)),
+	PINCTRL_CONF_DESC(59, REG_GPIO_H_PD, BIT(14)),
+	PINCTRL_CONF_DESC(60, REG_I2C_SDA_PD, PCIE0_RESET_PD_MASK),
+	PINCTRL_CONF_DESC(61, REG_I2C_SDA_PD, PCIE1_RESET_PD_MASK),
+	PINCTRL_CONF_DESC(62, REG_I2C_SDA_PD, PCIE2_RESET_PD_MASK),
+};
+
+static const struct airoha_pinctrl_conf pinctrl_drive_e2_conf[] = {
+	PINCTRL_CONF_DESC(0, REG_I2C_SDA_E2, UART1_TXD_E2_MASK),
+	PINCTRL_CONF_DESC(1, REG_I2C_SDA_E2, UART1_RXD_E2_MASK),
+	PINCTRL_CONF_DESC(2, REG_I2C_SDA_E2, I2C_SDA_E2_MASK),
+	PINCTRL_CONF_DESC(3, REG_I2C_SDA_E2, I2C_SCL_E2_MASK),
+	PINCTRL_CONF_DESC(4, REG_I2C_SDA_E2, SPI_CS0_E2_MASK),
+	PINCTRL_CONF_DESC(5, REG_I2C_SDA_E2, SPI_CLK_E2_MASK),
+	PINCTRL_CONF_DESC(6, REG_I2C_SDA_E2, SPI_MOSI_E2_MASK),
+	PINCTRL_CONF_DESC(7, REG_I2C_SDA_E2, SPI_MISO_E2_MASK),
+	PINCTRL_CONF_DESC(13, REG_GPIO_L_E2, BIT(0)),
+	PINCTRL_CONF_DESC(14, REG_GPIO_L_E2, BIT(1)),
+	PINCTRL_CONF_DESC(15, REG_GPIO_L_E2, BIT(2)),
+	PINCTRL_CONF_DESC(16, REG_GPIO_L_E2, BIT(3)),
+	PINCTRL_CONF_DESC(17, REG_GPIO_L_E2, BIT(4)),
+	PINCTRL_CONF_DESC(18, REG_GPIO_L_E2, BIT(5)),
+	PINCTRL_CONF_DESC(19, REG_GPIO_L_E2, BIT(6)),
+	PINCTRL_CONF_DESC(20, REG_GPIO_L_E2, BIT(7)),
+	PINCTRL_CONF_DESC(21, REG_GPIO_L_E2, BIT(8)),
+	PINCTRL_CONF_DESC(22, REG_GPIO_L_E2, BIT(9)),
+	PINCTRL_CONF_DESC(23, REG_GPIO_L_E2, BIT(10)),
+	PINCTRL_CONF_DESC(24, REG_GPIO_L_E2, BIT(11)),
+	PINCTRL_CONF_DESC(25, REG_GPIO_L_E2, BIT(12)),
+	PINCTRL_CONF_DESC(26, REG_GPIO_L_E2, BIT(13)),
+	PINCTRL_CONF_DESC(27, REG_GPIO_L_E2, BIT(14)),
+	PINCTRL_CONF_DESC(28, REG_GPIO_L_E2, BIT(15)),
+	PINCTRL_CONF_DESC(29, REG_GPIO_L_E2, BIT(16)),
+	PINCTRL_CONF_DESC(30, REG_GPIO_L_E2, BIT(17)),
+	PINCTRL_CONF_DESC(31, REG_GPIO_L_E2, BIT(18)),
+	PINCTRL_CONF_DESC(32, REG_GPIO_L_E2, BIT(19)),
+	PINCTRL_CONF_DESC(33, REG_GPIO_L_E2, BIT(20)),
+	PINCTRL_CONF_DESC(34, REG_GPIO_L_E2, BIT(21)),
+	PINCTRL_CONF_DESC(35, REG_GPIO_L_E2, BIT(22)),
+	PINCTRL_CONF_DESC(36, REG_GPIO_L_E2, BIT(23)),
+	PINCTRL_CONF_DESC(37, REG_GPIO_L_E2, BIT(24)),
+	PINCTRL_CONF_DESC(38, REG_GPIO_L_E2, BIT(25)),
+	PINCTRL_CONF_DESC(39, REG_GPIO_L_E2, BIT(26)),
+	PINCTRL_CONF_DESC(40, REG_GPIO_L_E2, BIT(27)),
+	PINCTRL_CONF_DESC(41, REG_GPIO_L_E2, BIT(28)),
+	PINCTRL_CONF_DESC(42, REG_GPIO_L_E2, BIT(29)),
+	PINCTRL_CONF_DESC(43, REG_GPIO_L_E2, BIT(30)),
+	PINCTRL_CONF_DESC(44, REG_GPIO_L_E2, BIT(31)),
+	PINCTRL_CONF_DESC(45, REG_GPIO_H_E2, BIT(0)),
+	PINCTRL_CONF_DESC(46, REG_GPIO_H_E2, BIT(1)),
+	PINCTRL_CONF_DESC(47, REG_GPIO_H_E2, BIT(2)),
+	PINCTRL_CONF_DESC(48, REG_GPIO_H_E2, BIT(3)),
+	PINCTRL_CONF_DESC(49, REG_GPIO_H_E2, BIT(4)),
+	PINCTRL_CONF_DESC(50, REG_GPIO_H_E2, BIT(5)),
+	PINCTRL_CONF_DESC(51, REG_GPIO_H_E2, BIT(6)),
+	PINCTRL_CONF_DESC(52, REG_GPIO_H_E2, BIT(7)),
+	PINCTRL_CONF_DESC(53, REG_GPIO_H_E2, BIT(8)),
+	PINCTRL_CONF_DESC(54, REG_GPIO_H_E2, BIT(9)),
+	PINCTRL_CONF_DESC(55, REG_GPIO_H_E2, BIT(10)),
+	PINCTRL_CONF_DESC(56, REG_GPIO_H_E2, BIT(11)),
+	PINCTRL_CONF_DESC(57, REG_GPIO_H_E2, BIT(12)),
+	PINCTRL_CONF_DESC(58, REG_GPIO_H_E2, BIT(13)),
+	PINCTRL_CONF_DESC(59, REG_GPIO_H_E2, BIT(14)),
+	PINCTRL_CONF_DESC(60, REG_I2C_SDA_E2, PCIE0_RESET_E2_MASK),
+	PINCTRL_CONF_DESC(61, REG_I2C_SDA_E2, PCIE1_RESET_E2_MASK),
+	PINCTRL_CONF_DESC(62, REG_I2C_SDA_E2, PCIE2_RESET_E2_MASK),
+};
+
+static const struct airoha_pinctrl_conf pinctrl_drive_e4_conf[] = {
+	PINCTRL_CONF_DESC(0, REG_I2C_SDA_E4, UART1_TXD_E4_MASK),
+	PINCTRL_CONF_DESC(1, REG_I2C_SDA_E4, UART1_RXD_E4_MASK),
+	PINCTRL_CONF_DESC(2, REG_I2C_SDA_E4, I2C_SDA_E4_MASK),
+	PINCTRL_CONF_DESC(3, REG_I2C_SDA_E4, I2C_SCL_E4_MASK),
+	PINCTRL_CONF_DESC(4, REG_I2C_SDA_E4, SPI_CS0_E4_MASK),
+	PINCTRL_CONF_DESC(5, REG_I2C_SDA_E4, SPI_CLK_E4_MASK),
+	PINCTRL_CONF_DESC(6, REG_I2C_SDA_E4, SPI_MOSI_E4_MASK),
+	PINCTRL_CONF_DESC(7, REG_I2C_SDA_E4, SPI_MISO_E4_MASK),
+	PINCTRL_CONF_DESC(13, REG_GPIO_L_E4, BIT(0)),
+	PINCTRL_CONF_DESC(14, REG_GPIO_L_E4, BIT(1)),
+	PINCTRL_CONF_DESC(15, REG_GPIO_L_E4, BIT(2)),
+	PINCTRL_CONF_DESC(16, REG_GPIO_L_E4, BIT(3)),
+	PINCTRL_CONF_DESC(17, REG_GPIO_L_E4, BIT(4)),
+	PINCTRL_CONF_DESC(18, REG_GPIO_L_E4, BIT(5)),
+	PINCTRL_CONF_DESC(19, REG_GPIO_L_E4, BIT(6)),
+	PINCTRL_CONF_DESC(20, REG_GPIO_L_E4, BIT(7)),
+	PINCTRL_CONF_DESC(21, REG_GPIO_L_E4, BIT(8)),
+	PINCTRL_CONF_DESC(22, REG_GPIO_L_E4, BIT(9)),
+	PINCTRL_CONF_DESC(23, REG_GPIO_L_E4, BIT(10)),
+	PINCTRL_CONF_DESC(24, REG_GPIO_L_E4, BIT(11)),
+	PINCTRL_CONF_DESC(25, REG_GPIO_L_E4, BIT(12)),
+	PINCTRL_CONF_DESC(26, REG_GPIO_L_E4, BIT(13)),
+	PINCTRL_CONF_DESC(27, REG_GPIO_L_E4, BIT(14)),
+	PINCTRL_CONF_DESC(28, REG_GPIO_L_E4, BIT(15)),
+	PINCTRL_CONF_DESC(29, REG_GPIO_L_E4, BIT(16)),
+	PINCTRL_CONF_DESC(30, REG_GPIO_L_E4, BIT(17)),
+	PINCTRL_CONF_DESC(31, REG_GPIO_L_E4, BIT(18)),
+	PINCTRL_CONF_DESC(32, REG_GPIO_L_E4, BIT(19)),
+	PINCTRL_CONF_DESC(33, REG_GPIO_L_E4, BIT(20)),
+	PINCTRL_CONF_DESC(34, REG_GPIO_L_E4, BIT(21)),
+	PINCTRL_CONF_DESC(35, REG_GPIO_L_E4, BIT(22)),
+	PINCTRL_CONF_DESC(36, REG_GPIO_L_E4, BIT(23)),
+	PINCTRL_CONF_DESC(37, REG_GPIO_L_E4, BIT(24)),
+	PINCTRL_CONF_DESC(38, REG_GPIO_L_E4, BIT(25)),
+	PINCTRL_CONF_DESC(39, REG_GPIO_L_E4, BIT(26)),
+	PINCTRL_CONF_DESC(40, REG_GPIO_L_E4, BIT(27)),
+	PINCTRL_CONF_DESC(41, REG_GPIO_L_E4, BIT(28)),
+	PINCTRL_CONF_DESC(42, REG_GPIO_L_E4, BIT(29)),
+	PINCTRL_CONF_DESC(43, REG_GPIO_L_E4, BIT(30)),
+	PINCTRL_CONF_DESC(44, REG_GPIO_L_E4, BIT(31)),
+	PINCTRL_CONF_DESC(45, REG_GPIO_H_E4, BIT(0)),
+	PINCTRL_CONF_DESC(46, REG_GPIO_H_E4, BIT(1)),
+	PINCTRL_CONF_DESC(47, REG_GPIO_H_E4, BIT(2)),
+	PINCTRL_CONF_DESC(48, REG_GPIO_H_E4, BIT(3)),
+	PINCTRL_CONF_DESC(49, REG_GPIO_H_E4, BIT(4)),
+	PINCTRL_CONF_DESC(50, REG_GPIO_H_E4, BIT(5)),
+	PINCTRL_CONF_DESC(51, REG_GPIO_H_E4, BIT(6)),
+	PINCTRL_CONF_DESC(52, REG_GPIO_H_E4, BIT(7)),
+	PINCTRL_CONF_DESC(53, REG_GPIO_H_E4, BIT(8)),
+	PINCTRL_CONF_DESC(54, REG_GPIO_H_E4, BIT(9)),
+	PINCTRL_CONF_DESC(55, REG_GPIO_H_E4, BIT(10)),
+	PINCTRL_CONF_DESC(56, REG_GPIO_H_E4, BIT(11)),
+	PINCTRL_CONF_DESC(57, REG_GPIO_H_E4, BIT(12)),
+	PINCTRL_CONF_DESC(58, REG_GPIO_H_E4, BIT(13)),
+	PINCTRL_CONF_DESC(59, REG_GPIO_H_E4, BIT(14)),
+	PINCTRL_CONF_DESC(60, REG_I2C_SDA_E4, PCIE0_RESET_E4_MASK),
+	PINCTRL_CONF_DESC(61, REG_I2C_SDA_E4, PCIE1_RESET_E4_MASK),
+	PINCTRL_CONF_DESC(62, REG_I2C_SDA_E4, PCIE2_RESET_E4_MASK),
+};
+
+static const struct airoha_pinctrl_conf pinctrl_pcie_rst_od_conf[] = {
+	PINCTRL_CONF_DESC(60, REG_PCIE_RESET_OD, PCIE0_RESET_OD_MASK),
+	PINCTRL_CONF_DESC(61, REG_PCIE_RESET_OD, PCIE1_RESET_OD_MASK),
+	PINCTRL_CONF_DESC(62, REG_PCIE_RESET_OD, PCIE2_RESET_OD_MASK),
+};
+
+static const struct airoha_pinctrl_match_data pinctrl_match_data = {
+	.gpio_offs = 13,
+	.gpio_pin_cnt = 50,
+	.chip_scu_compatible = "airoha,en7581-chip-scu",
+	.pins = pinctrl_pins,
+	.num_pins = ARRAY_SIZE(pinctrl_pins),
+	.grps = pinctrl_groups,
+	.num_grps = ARRAY_SIZE(pinctrl_groups),
+	.funcs = pinctrl_funcs,
+	.num_funcs = ARRAY_SIZE(pinctrl_funcs),
+	.confs_info = {
+		[AIROHA_PINCTRL_CONFS_PULLUP] = {
+			.confs = pinctrl_pullup_conf,
+			.num_confs = ARRAY_SIZE(pinctrl_pullup_conf),
+		},
+		[AIROHA_PINCTRL_CONFS_PULLDOWN] = {
+			.confs = pinctrl_pulldown_conf,
+			.num_confs = ARRAY_SIZE(pinctrl_pulldown_conf),
+		},
+		[AIROHA_PINCTRL_CONFS_DRIVE_E2] = {
+			.confs = pinctrl_drive_e2_conf,
+			.num_confs = ARRAY_SIZE(pinctrl_drive_e2_conf),
+		},
+		[AIROHA_PINCTRL_CONFS_DRIVE_E4] = {
+			.confs = pinctrl_drive_e4_conf,
+			.num_confs = ARRAY_SIZE(pinctrl_drive_e4_conf),
+		},
+		[AIROHA_PINCTRL_CONFS_PCIE_RST_OD] = {
+			.confs = pinctrl_pcie_rst_od_conf,
+			.num_confs = ARRAY_SIZE(pinctrl_pcie_rst_od_conf),
+		},
+	},
+};
+
+static const struct udevice_id pinctrl_of_match[] = {
+	{ .compatible = "airoha,en7581-pinctrl",
+	  .data = (uintptr_t)&pinctrl_match_data },
+	{ .compatible = "airoha,an7581-pinctrl",
+	  .data = (uintptr_t)&pinctrl_match_data },
+	{ /* sentinel */ }
+};
+
+U_BOOT_DRIVER(airoha_an7581_pinctrl) = {
+	.name = "airoha-an7581-pinctrl",
+	.id = UCLASS_PINCTRL,
+	.of_match = of_match_ptr(pinctrl_of_match),
+	.probe = airoha_pinctrl_probe,
+	.bind = airoha_pinctrl_bind,
+	.priv_auto = sizeof(struct airoha_pinctrl),
+	.ops = &airoha_pinctrl_ops,
+};
-- 
2.53.0

