From 2ff84ce933de37e91d132553a2555c4b4e9dedc8 Mon Sep 17 00:00:00 2001
From: Shiji Yang <yangshiji66@outlook.com>
Date: Tue, 24 Feb 2026 15:32:42 +0800
Subject: [PATCH 1/2] pwm: mediatek: set mt7628 pwm45_fixup flag to false

According to the programing guide, mt7628 has generic register layout
like most other hardware revisions. We should not set pwm45_fixup flag
for it.

Signed-off-by: Shiji Yang <yangshiji66@outlook.com>
---
 drivers/pwm/pwm-mediatek.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/pwm/pwm-mediatek.c
+++ b/drivers/pwm/pwm-mediatek.c
@@ -458,7 +458,7 @@ static const struct pwm_mediatek_of_data
 
 static const struct pwm_mediatek_of_data mt7628_pwm_data = {
 	.num_pwms = 4,
-	.pwm45_fixup = true,
+	.pwm45_fixup = false,
 	.chanreg_base = 0x10,
 	.chanreg_width = 0x40,
 };
