From bcc0886b4d25cc9d82e4aa0cfa78c1268c3fcb86 Mon Sep 17 00:00:00 2001
From: Jonas Karlman <jonas@kwiboo.se>
Date: Thu, 13 Mar 2025 22:48:27 +0000
Subject: [PATCH] arm64: dts: rockchip: Add TSADC controller for RK3528

Signed-off-by: Jonas Karlman <jonas@kwiboo.se>
---
 arch/arm64/boot/dts/rockchip/rk3528.dtsi | 78 ++++++++++++++++++++++++
 1 file changed, 78 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3528.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3528.dtsi
@@ -9,6 +9,7 @@
 #include <dt-bindings/interrupt-controller/irq.h>
 #include <dt-bindings/phy/phy.h>
 #include <dt-bindings/pinctrl/rockchip.h>
+#include <dt-bindings/thermal/thermal.h>
 #include <dt-bindings/clock/rockchip,rk3528-cru.h>
 #include <dt-bindings/power/rockchip,rk3528-power.h>
 #include <dt-bindings/reset/rockchip,rk3528-cru.h>
@@ -55,6 +56,7 @@
 			device_type = "cpu";
 			enable-method = "psci";
 			clocks = <&scmi_clk SCMI_CLK_CPU>;
+			#cooling-cells = <2>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
@@ -64,6 +66,7 @@
 			device_type = "cpu";
 			enable-method = "psci";
 			clocks = <&scmi_clk SCMI_CLK_CPU>;
+			#cooling-cells = <2>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
@@ -73,6 +76,7 @@
 			device_type = "cpu";
 			enable-method = "psci";
 			clocks = <&scmi_clk SCMI_CLK_CPU>;
+			#cooling-cells = <2>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 
@@ -82,6 +86,7 @@
 			device_type = "cpu";
 			enable-method = "psci";
 			clocks = <&scmi_clk SCMI_CLK_CPU>;
+			#cooling-cells = <2>;
 			operating-points-v2 = <&cpu_opp_table>;
 		};
 	};
@@ -255,6 +260,51 @@
 		};
 	};
 
+	thermal-zones {
+		soc_thermal: soc-thermal {
+			polling-delay-passive = <20>;
+			polling-delay = <1000>;
+			sustainable-power = <638>;
+			thermal-sensors = <&tsadc 0>;
+
+			trips {
+				threshold: trip-point-0 {
+					temperature = <70000>;
+					hysteresis = <2000>;
+					type = "passive";
+				};
+				target: trip-point-1 {
+					temperature = <85000>;
+					hysteresis = <2000>;
+					type = "passive";
+				};
+				soc_crit: soc-crit {
+					temperature = <95000>;
+					hysteresis = <2000>;
+					type = "critical";
+				};
+			};
+
+			cooling-maps {
+				map0 {
+					trip = <&target>;
+					cooling-device =
+						<&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+						<&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+						<&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+						<&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+					contribution = <2048>;
+				};
+				map1 {
+					trip = <&target>;
+					cooling-device =
+						<&gpu THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+					contribution = <1024>;
+				};
+			};
+		};
+	};
+
 	timer {
 		compatible = "arm,armv8-timer";
 		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
@@ -692,6 +742,7 @@
 			assigned-clock-rates = <297000000>, <300000000>;
 			clocks = <&cru ACLK_GPU_MALI>, <&scmi_clk SCMI_CLK_GPU>;
 			clock-names = "bus", "core";
+			#cooling-cells = <2>;
 			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>,
 				     <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>,
 				     <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>,
@@ -1034,6 +1085,33 @@
 			status = "disabled";
 		};
 
+		tsadc: tsadc@ffad0000 {
+			compatible = "rockchip,rk3528-tsadc";
+			reg = <0x0 0xffad0000 0x0 0x400>;
+			assigned-clocks = <&cru CLK_TSADC>, <&cru CLK_TSADC_TSEN>;
+			assigned-clock-rates = <1200000>, <12000000>;
+			clocks = <&cru CLK_TSADC>, <&cru PCLK_TSADC>,
+				 <&cru CLK_TSADC_TSEN>;
+			clock-names = "tsadc", "apb_pclk", "tsen";
+			interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
+			power-domains = <&power RK3528_PD_VPU>;
+			resets = <&cru SRST_P_TSADC>, <&cru SRST_TSADC>;
+			reset-names = "tsadc-apb", "tsadc";
+			rockchip,grf = <&vpu_grf>;
+			rockchip,hw-tshut-mode = <0>;
+			rockchip,hw-tshut-polarity = <0>;
+			rockchip,hw-tshut-temp = <100000>;
+			#thermal-sensor-cells = <1>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sensor@0 {
+				reg = <0>;
+				nvmem-cells = <&tsadc_trim>;
+				nvmem-cell-names = "trim";
+			};
+		};
+
 		saradc: adc@ffae0000 {
 			compatible = "rockchip,rk3528-saradc";
 			reg = <0x0 0xffae0000 0x0 0x10000>;
