From e941dae591d8cd24f6758ecded9cc9741082e76d Mon Sep 17 00:00:00 2001
From: Geert Uytterhoeven <geert@linux-m68k.org>
Date: Thu, 27 May 2021 20:13:43 +0200
Subject: [PATCH 1012/1021] dt-bindings: dma: dw-axi-dmac: Increase DMA channel
 limit to 16

The first DMAC instance in the StarFive JH7100 SoC supports 16 DMA
channels.

FIXME Given there are more changes to the driver than just increasing
      DMAC_MAX_CHANNELS, we probably need a new compatible value, too.

Signed-off-by: Geert Uytterhoeven <geert@linux-m68k.org>
---
 Documentation/devicetree/bindings/dma/snps,dw-axi-dmac.yaml | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/Documentation/devicetree/bindings/dma/snps,dw-axi-dmac.yaml
+++ b/Documentation/devicetree/bindings/dma/snps,dw-axi-dmac.yaml
@@ -57,7 +57,7 @@ properties:
 
   dma-channels:
     minimum: 1
-    maximum: 8
+    maximum: 16
 
   dma-noncoherent: true
 
@@ -83,14 +83,14 @@ properties:
       Channel priority specifier associated with the DMA channels.
     $ref: /schemas/types.yaml#/definitions/uint32-array
     minItems: 1
-    maxItems: 8
+    maxItems: 16
 
   snps,block-size:
     description: |
       Channel block size specifier associated with the DMA channels.
     $ref: /schemas/types.yaml#/definitions/uint32-array
     minItems: 1
-    maxItems: 8
+    maxItems: 16
 
   snps,axi-max-burst-len:
     description: |
