From ff161318a23b1af94eeb0b74e25daa17f9a8e18e Mon Sep 17 00:00:00 2001
From: Dom Cobley <popcornmix@gmail.com>
Date: Wed, 31 Jan 2024 19:47:39 +0000
Subject: [PATCH] Revert "ARM: dts: bcm2711: Add BCM2711 xHCI support"

This reverts commit 522c35e08b53f157ad3e51848caa861b258001e4.
---
 arch/arm/boot/dts/broadcom/bcm2711.dtsi | 15 ---------------
 1 file changed, 15 deletions(-)

--- a/arch/arm/boot/dts/broadcom/bcm2711.dtsi
+++ b/arch/arm/boot/dts/broadcom/bcm2711.dtsi
@@ -602,21 +602,6 @@
 			};
 		};
 
-		xhci: usb@7e9c0000 {
-			compatible = "brcm,bcm2711-xhci", "brcm,xhci-brcm-v2";
-			reg = <0x0 0x7e9c0000 0x100000>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			interrupts = <GIC_SPI 176 IRQ_TYPE_LEVEL_HIGH>;
-			power-domains = <&pm BCM2835_POWER_DOMAIN_USB>;
-			/* DWC2 and this IP block share the same USB PHY,
-			 * enabling both at the same time results in lockups.
-			 * So keep this node disabled and let the bootloader
-			 * decide which interface should be enabled.
-			 */
-			status = "disabled";
-		};
-
 		v3d: gpu@7ec00000 {
 			compatible = "brcm,2711-v3d";
 			reg = <0x0 0x7ec00000 0x4000>,
