// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9330.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	pinctrl-names = "default";
	pinctrl-0 = <&jtag_disable_pins>;

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
		label-mac-device = &wmac;
	};

	gpio_leds: leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&switch_led_disable_pins>;

		led_system: system {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 28 GPIO_ACTIVE_HIGH>;
			default-state = "on";
			panic-indicator;
		};
	};

	gpio_keys: keys {
		compatible = "gpio-keys";
	};
};

&usb {
	status = "okay";

	dr_mode = "host";
};

&usb_phy {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <50000000>;
		reg = <0>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x040000 0xfa0000>;
			};

			partition@fe0000 {
				label = "config";
				reg = <0xfe0000 0x10000>;
				read-only;
			};
			partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_art_0: macaddr@0 {
						reg = <0x0 0x6>;
					};

					macaddr_art_6: macaddr@6 {
						reg = <0x6 0x6>;
					};

					macaddr_art_1002: macaddr@1002 {
						reg = <0x1002 0x6>;
					};

					cal_art_1000: calibration@1000 {
						reg = <0x1000 0x440>;
					};
				};
			};
		};
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	status = "okay";

	nvmem-cells = <&macaddr_art_6>;
	nvmem-cell-names = "mac-address";

	gmac-config {
		device = <&gmac>;

		switch-phy-addr-swap = <0>;
		switch-phy-swap = <0>;
	};
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_art_1002>, <&cal_art_1000>;
	nvmem-cell-names = "mac-address", "calibration";
};
