// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/* Copyright (c) 2021, Dirk Buchwalder <buchwalder@posteo.de> */

/dts-v1/;

#include "ipq8074.dtsi"
#include "ipq8074-hk-cpu.dtsi"
#include "ipq8074-ess.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "QNAP 301w";
	compatible = "qnap,301w", "qcom,ipq8074";

	aliases {
		serial0 = &blsp1_uart5;
		/*
		 * Aliases as required by u-boot
		 * to patch MAC addresses
		 */
		led-boot = &led_system_red;
		led-failsafe = &led_system_red;
		led-running = &led_pwr_green;
		led-upgrade = &led_system_red;
		ethernet0 = &lan4;
		ethernet1 = &lan3;
		ethernet2 = &lan2;
		ethernet3 = &lan1;
		ethernet4 = &port_10g_1;
		ethernet5 = &port_10g_2;
		label-mac-device = &lan4;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		wps-button {
			label = "wps";
			gpios = <&tlmm 57 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset-button {
			label = "reset";
			gpios = <&tlmm 67 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&leds_pins>;
		pinctrl-names = "default";

		led_system_green: led-system-green {
			gpios = <&tlmm 1 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
		};

		led_system_red: led-system-red {
			gpios = <&tlmm 3 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
		};

		led_pwr_green: led-pwr-green {
			gpios = <&tlmm 4 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
		};

		led-wifi-green {
			gpios = <&tlmm 42 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
		};

		led-lan4-green {
			gpios = <&tlmm 6 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			function-enumerator = <4>;
		};

		led-lan4-amber {
			gpios = <&tlmm 7 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_LAN;
			function-enumerator = <4>;
		};

		led-lan3-green {
			gpios = <&tlmm 8 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			function-enumerator = <3>;
		};

		led-lan3-amber {
			gpios = <&tlmm 11 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_LAN;
			function-enumerator = <3>;
		};

		led-lan2-green {
			gpios = <&tlmm 12 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			function-enumerator = <2>;
		};

		led-lan2-amber {
			gpios = <&tlmm 13 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_LAN;
			function-enumerator = <2>;
		};

		led-lan1-green {
			gpios = <&tlmm 14 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			function-enumerator = <1>;
		};

		led-lan1-amber {
			gpios = <&tlmm 15 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_LAN;
			function-enumerator = <1>;
		};

		led-10g-1-green {
			gpios = <&tlmm 54 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = "10g";
			function-enumerator = <1>;
		};

		led-10g-1-amber {
			gpios = <&tlmm 56 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_AMBER>;
			function = "10g";
			function-enumerator = <1>;
		};

		led-10g-2-green {
			gpios = <&tlmm 51 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = "10g";
			function-enumerator = <2>;
		};

		led-10g-2-amber {
			gpios = <&tlmm 52 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_AMBER>;
			function = "10g";
			function-enumerator = <2>;
		};
	};
};

&tlmm {

	mdio_pins: mdio-state {
		mdc-pins {
			pins = "gpio68";
			function = "mdc";
			drive-strength = <8>;
			bias-pull-up;
		};

		mdio-pins {
			pins = "gpio69";
			function = "mdio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};

	button_pins: button-state {
		wps-pins {
			pins = "gpio57";
			function = "gpio";
			drive-strength = <8>;
			bias-pull-up;
		};

		rst-pins {
			pins = "gpio67";
			function = "gpio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};

	leds_pins: leds-state {
		pins = "gpio1", "gpio3", "gpio4", "gpio6", "gpio7", "gpio8",
		       "gpio11", "gpio12", "gpio13", "gpio14", "gpio15", "gpio42",
		       "gpio51", "gpio52", "gpio54", "gpio56";
		function = "gpio";
		drive-strength = <8>;
		bias-pull-down;
	};
};

&blsp1_uart5 {
	status = "okay";
};

&prng {
	status = "okay";
};

&ssphy_0 {
	status = "okay";
};

&qusb_phy_0 {
	status = "okay";
};

&ssphy_1 {
	status = "okay";
};

&qusb_phy_1 {
	status = "okay";
};

&usb_0 {
	status = "okay";
};

&usb_1 {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&crypto {
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&blsp1_spi1 { /* BLSP1 QUP1 */
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";

	flash@0 {
		reg = <0>;
		compatible = "jedec,spi-nor";
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "0:sbl1";
				reg = <0x0 0x50000>;
				read-only;
			};

			partition@50000 {
				label = "0:mibib";
				reg = <0x50000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "0:qsee";
				reg = <0x60000 0x180000>;
				read-only;
			};

			partition@1e0000 {
				label = "0:devcfg";
				reg = <0x1e0000 0x10000>;
				read-only;
			};

			partition@1f0000 {
				label = "0:apdp";
				reg = <0x1f0000 0x10000>;
				read-only;
			};

			partition@200000 {
				label = "0:rpm";
				reg = <0x200000 0x40000>;
				read-only;
			};

			partition@240000 {
				label = "0:cdt";
				reg = <0x240000 0x10000>;
				read-only;
			};

			partition@250000 {
				label = "0:appsblenv";
				reg = <0x250000 0x20000>;
			};

			partition@270000 {
				label = "0:appsbl";
				reg = <0x250000 0x100000>;
				read-only;
			};

			partition@370000 {
				label = "0:art";
				reg = <0x370000 0x40000>;
				read-only;
			};

			partition@3b0000 {
				label = "0:ethphyfw1";
				reg = <0x3b0000 0x80000>;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					aqr0_fw: firmware@0 {
						reg = <0x0 0x5fc02>;
					};
				};
			};

			partition@430000 {
				label = "0:ethphyfw2";
				reg = <0x430000 0x80000>;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					aqr1_fw: firmware@0 {
						reg = <0x0 0x5fc02>;
					};
				};
			};

			partition@4b0000 {
				label = "reserved";
				reg = <0x4b0000 0x350000>;
			};
		};
	};
};

&mdio {
	status = "okay";

	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
	reset-gpios = <&tlmm 37 GPIO_ACTIVE_LOW>;

	aqr113c_0: ethernet-phy@0 {
		compatible ="ethernet-phy-ieee802.3-c45";
		reg = <0>;
		reset-gpios = <&tlmm 44 GPIO_ACTIVE_LOW>;
		firmware-name = "marvell/AQR-G4_v5.4.C-AQR_CIG_WF-1945_0x0_ID44778_VER1630.cld";
		nvmem-cell-names = "firmware";
		nvmem-cells = <&aqr0_fw>;
	};

	aqr113c_8: ethernet-phy@8 {
		compatible ="ethernet-phy-ieee802.3-c45";
		reg = <8>;
		reset-gpios = <&tlmm 59 GPIO_ACTIVE_LOW>;
		firmware-name = "marvell/AQR-G4_v5.4.C-AQR_CIG_WF-1945_0x8_ID44776_VER1630.cld";
		nvmem-cell-names = "firmware";
		nvmem-cells = <&aqr1_fw>;
	};

	ethernet-phy-package@16 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "qcom,qca8075-package";
		reg = <16>;

		qcom,package-mode = "qsgmii";

		qca8075_16: ethernet-phy@16 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <16>;
		};

		qca8075_17: ethernet-phy@17 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <17>;
		};

		qca8075_18: ethernet-phy@18 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <18>;
		};

		qca8075_19: ethernet-phy@19 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <19>;
		};
	};
};

&sdhc_1 {
	status = "okay";

	/* According to the stock dts from the QNAP gpl drop
	 * the emmc has a problem with the hs400 > hs200 speed switch.
	 * Therefore remove the mmc-hs400-1_8v property
	*/
	/delete-property/ mmc-hs400-1_8v;
	mmc-hs200-1_8v;
	mmc-ddr-1_8v;
	vqmmc-supply = <&l11>;
};

&uniphy0 {
	status = "okay";
};

&uniphy1 {
	status = "okay";
};

&uniphy2 {
	status = "okay";
};

&switch {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			ethernet = <&edma>;
			phy-mode = "internal";

			fixed-link {
				speed = <1000>;
				full-duplex;
			};
		};

		lan4: port@1 {
			reg = <1>;
			label = "lan4";
			phy-handle = <&qca8075_16>;
			phy-mode = "qsgmii";
			pcs-handle = <&uniphy0 0>;
		};

		lan3: port@2 {
			reg = <2>;
			label = "lan3";
			phy-handle = <&qca8075_17>;
			phy-mode = "qsgmii";
			pcs-handle = <&uniphy0 1>;
		};

		lan2: port@3 {
			reg = <3>;
			label = "lan2";
			phy-handle = <&qca8075_18>;
			phy-mode = "qsgmii";
			pcs-handle = <&uniphy0 2>;
		};


		lan1: port@4 {
			reg = <4>;
			label = "lan1";
			phy-handle = <&qca8075_19>;
			phy-mode = "qsgmii";
			pcs-handle = <&uniphy0 3>;
		};

		port_10g_1: port@5 {
			reg = <5>;
			label = "10g-1";
			phy-handle = <&aqr113c_8>;
			phy-mode = "usxgmii";
			pcs-handle = <&uniphy1 0>;
		};

		port_10g_2: port@6 {
			reg = <6>;
			label = "10g-2";
			phy-handle = <&aqr113c_0>;
			phy-mode = "usxgmii";
			pcs-handle = <&uniphy2 0>;
		};
	};
};

&edma {
	status = "okay";
};

&wifi {
	status = "okay";

	qcom,ath11k-calibration-variant = "QNAP-301w";
};
