// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "ruijie,rg-ew1300g-v1", "mediatek,mt7621-soc";
	model = "Ruijie RG-EW1300G v1";

	aliases {
		led-boot = &led_status_red;
		led-failsafe = &led_status_green;
		led-running = &led_status_green;
		led-upgrade = &led_status_red;
	};

	chosen {
		bootargs = "console=ttyS0,57600n8";
	};

	leds {
		compatible = "gpio-leds";
		led_status_green: status_green {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		led_status_red: status_red {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led_mesh_green: mesh_green {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		button-mesh {
			label = "mesh";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		button-reset {
			label = "reset";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x50000>;
				read-only;
			};

			partition@50000 {
				label = "u-boot-env";
				reg = <0x50000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "factory";
				reg = <0x60000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_factory_0: eeprom@0 {
						reg = <0x0 0x4da8>;
					};
				};
			};

			partition@70000 {
				label = "product_info";
				reg = <0x70000 0x10000>;
				read-only;
			};

			partition@80000 {
				label = "kdump";
				reg = <0x80000 0x10000>;
				read-only;
			};

			partition@90000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x90000 0xf70000>;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>;
		nvmem-cell-names = "eeprom";
	};
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "wan";
		};

		port@1 {
			status = "okay";
			label = "lan3";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan1";
		};
	};
};
