// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "rtl838x.dtsi"
#include "rtl83xx_hpe_1920.dtsi"

/ {
	i2c0: i2c-gpio-0 {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio1 23 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio1 24 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	sfp0: sfp-0 {
		compatible = "sff,sfp";
		i2c-bus = <&i2c0>;
		los-gpio = <&gpio1 26 GPIO_ACTIVE_HIGH>;
		mod-def0-gpio = <&gpio1 25 GPIO_ACTIVE_LOW>;
		// tx-fault and tx-disable unconnected
	};

	i2c1: i2c-gpio-1 {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio1 13 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio1 14 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	sfp1: sfp-1 {
		compatible = "sff,sfp";
		i2c-bus = <&i2c1>;
		los-gpio = <&gpio1 22 GPIO_ACTIVE_HIGH>;
		mod-def0-gpio = <&gpio1 21 GPIO_ACTIVE_LOW>;
		// tx-fault and tx-disable unconnected
	};
};

&mdio_aux {
	status = "okay";

	gpio1: expander@0 {
		compatible = "realtek,rtl8231";
		reg = <0>;

		gpio-controller;
		#gpio-cells = <2>;
		gpio-ranges = <&gpio1 0 0 37>;

		led-controller {
			compatible = "realtek,rtl8231-leds";
			status = "disabled";
		};
	};
};

&mdio_bus0 {
	PHY_C22(8, 8)
	PHY_C22(9, 9)
	PHY_C22(10, 10)
	PHY_C22(11, 11)
	PHY_C22(12, 12)
	PHY_C22(13, 13)
	PHY_C22(14, 14)
	PHY_C22(15, 15)
};

&switch0 {
	ethernet-ports {
		#address-cells = <1>;
		#size-cells = <0>;

		SWITCH_PORT(8, 1, internal)
		SWITCH_PORT(9, 2, internal)
		SWITCH_PORT(10, 3, internal)
		SWITCH_PORT(11, 4, internal)
		SWITCH_PORT(12, 5, internal)
		SWITCH_PORT(13, 6, internal)
		SWITCH_PORT(14, 7, internal)
		SWITCH_PORT(15, 8, internal)

		port@24 {
			reg = <24>;
			label = "lan9";
			pcs-handle = <&serdes4 0>;
			phy-mode = "1000base-x";
			managed = "in-band-status";
			sfp = <&sfp0>;

			nvmem-cells = <&macaddr_factory 10>;
			nvmem-cell-names = "mac-address";
		};

		port@26 {
			reg = <26>;
			label = "lan10";
			pcs-handle = <&serdes5 0>;
			phy-mode = "1000base-x";
			managed = "in-band-status";
			sfp = <&sfp1>;

			nvmem-cells = <&macaddr_factory 11>;
			nvmem-cell-names = "mac-address";
		};

		port@28 {
			ethernet = <&ethernet0>;
			reg = <28>;
			phy-mode = "internal";
			fixed-link {
				speed = <1000>;
				full-duplex;
			};
		};
	};
};

&port8 {
	nvmem-cells = <&macaddr_factory 2>;
	nvmem-cell-names = "mac-address";
};

&port9 {
	nvmem-cells = <&macaddr_factory 3>;
	nvmem-cell-names = "mac-address";
};

&port10 {
	nvmem-cells = <&macaddr_factory 4>;
	nvmem-cell-names = "mac-address";
};

&port11 {
	nvmem-cells = <&macaddr_factory 5>;
	nvmem-cell-names = "mac-address";
};

&port12 {
	nvmem-cells = <&macaddr_factory 6>;
	nvmem-cell-names = "mac-address";
};

&port13 {
	nvmem-cells = <&macaddr_factory 7>;
	nvmem-cell-names = "mac-address";
};

&port14 {
	nvmem-cells = <&macaddr_factory 8>;
	nvmem-cell-names = "mac-address";
};

&port15 {
	nvmem-cells = <&macaddr_factory 9>;
	nvmem-cell-names = "mac-address";
};
