From: Felix Fietkau <nbd@nbd.name>
Date: Thu, 22 Aug 2024 18:02:17 +0200
Subject: [PATCH] net: bridge: fix switchdev host mdb entry updates

When a mdb entry is removed, the bridge switchdev code can issue a
switchdev_port_obj_del call for a port that was not offloaded.

This leads to an imbalance in switchdev_port_obj_add/del calls, since
br_switchdev_mdb_replay has not been called for the port before.

This can lead to potential multicast forwarding issues and messages such as:
mt7915e 0000:01:00.0 wl1-ap0: Failed to del Host Multicast Database entry
	(object id=3) with error: -ENOENT (-2).

Fix this issue by checking the port offload status when iterating over
lower devs.

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/net/bridge/br_switchdev.c
+++ b/net/bridge/br_switchdev.c
@@ -575,10 +575,18 @@ static void br_switchdev_host_mdb(struct
 				  struct net_bridge_mdb_entry *mp, int type)
 {
 	struct net_device *lower_dev;
+	struct net_bridge_port *port;
 	struct list_head *iter;
 
-	netdev_for_each_lower_dev(dev, lower_dev, iter)
+	rcu_read_lock();
+	netdev_for_each_lower_dev(dev, lower_dev, iter) {
+		port = br_port_get_rcu(lower_dev);
+		if (!port || !port->offload_count)
+			continue;
+
 		br_switchdev_host_mdb_one(dev, lower_dev, mp, type);
+	}
+	rcu_read_unlock();
 }
 
 static int
