// SPDX-License-Identifier: GPL-2.0-only OR MIT

#include "qcom-ipq4019.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "Sony NCP-HG100/Cellular";
	compatible = "sony,ncp-hg100-cellular";

	aliases {
		// TODO: Verify if the ethernet0 alias is needed
		ethernet0 = &gmac;
		led-boot = &led_cloud_green;
		led-failsafe = &led_cloud_red;
		led-running = &led_cloud_green;
		led-upgrade = &led_cloud_green;
		label-mac-device = &gmac;
	};

	chosen {
		bootargs = "console=ttyMSM0,115200n8 root=/dev/mmcblk0p15 rootfstype=squashfs,ext4";
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x20000000>;
	};

	soc {
		tcsr@1949000 {
			status = "okay";
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			status = "okay";
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
		};

		ess_tcsr@1953000 {
			status = "okay";
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			status = "okay";
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};

	keys-repeat {
		compatible = "gpio-keys";
		pinctrl-0 = <&keys_pins>;
		pinctrl-names = "default";
		autorepeat;

		key-volup {
			label = "volume up";
			linux,code = <KEY_VOLUMEUP>;
			gpios = <&tlmm 39 GPIO_ACTIVE_HIGH>;
			linux,input-type = <EV_KEY>;
		};

		key-voldown {
			label = "volume down";
			linux,code = <KEY_VOLUMEDOWN>;
			gpios = <&tlmm 40 GPIO_ACTIVE_HIGH>;
			linux,input-type = <EV_KEY>;
		};

		key-alexatrigger {
			label = "alexa trigger";
			linux,code = <BTN_0>;
			gpios = <&tlmm 42 GPIO_ACTIVE_HIGH>;
			linux,input-type = <EV_KEY>;
		};

		key-mute {
			label = "mic mute";
			linux,code = <BTN_1>;
			gpios = <&tlmm 47 GPIO_ACTIVE_LOW>;
			linux,input-type = <EV_SW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		key-reset {
			label = "reset";
			gpios = <&tlmm 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		key-wps {
			label = "setup";
			gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};
};

&tlmm {
	pinctrl-0 = <&bt_pins>, <&aud_pins>, <&mcu_pins>;
	pinctrl-names = "default";

	/*
	 * uart0 is shared for debug console and Z-Wave,
	 * use only for debug console in OpenWrt.
	 *
	 * 1: debug console
	 * 0: Z-Wave
	 */
	uart0_ctrl_pins: uart0_ctrl_pinmux {
		mux {
			pins = "gpio15";
			function = "gpio";
			output-high;
		};
	};

	serial_pins: serial_pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	/*
	 * reset pin for Z-Wave
	 * active-low, >= 20ns
	 */
	zwave_pins: zwave_pinmux {
		mux {
			pins = "gpio59";
			function = "gpio";
			output-high;
		};
	};

	serial_1_pins: serial1_pinmux {
		mux {
			pins = "gpio8", "gpio9",
				"gpio10", "gpio11";
			function = "blsp_uart1";
			bias-disable;
		};
	};

	bt_pins: bt_pinmux {
		mux_reset {
			pins = "gpio66";
			function = "gpio";
			output-high;
		};

		mux_pwr {
			pins = "gpio68";
			function = "gpio";
			output-high;
		};
	};

	mdio_pins: mdio_pinmux {
		mux_1 {
			pins = "gpio6";
			function = "mdio";
			bias-pull-up;
		};

		mux_2 {
			pins = "gpio7";
			function = "mdc";
			bias-pull-up;
		};
	};

	i2c_1_pins: i2c_1_pinmux {
		mux {
			pins = "gpio12", "gpio13";
			function = "blsp_i2c1";
			bias-disable;
		};
	};

	keys_pins: keys_pinmux {
		mux_1 {
			pins = "gpio39", "gpio40", "gpio42", "gpio47";
			function = "gpio";
			bias-disable;
		};

		mux_2 {
			pins = "gpio2";
			function = "gpio";
			input;
		};
	};

	sd_pins: sd_pins {
		mux {
			function = "sdio";
			pins = "gpio23", "gpio24", "gpio25", "gpio26",
				"gpio28", "gpio29", "gpio30", "gpio31";
			drive-strength = <4>;
		};

		mux_sd_clk {
			function = "sdio";
			pins = "gpio27";
			drive-strength = <16>;
		};

		mux_sd7 {
			function = "sdio";
			pins = "gpio32";
			drive-strength = <4>;
			bias-disable;
		};
	};

	aud_pins: aud_pinmux {
		mux {
			pins = "gpio48", "gpio49", "gpio50", "gpio51";
			function = "aud_pin";
		};
	};

	alc1304_pins: alc1304_pinmux {
		mux_1 {
			pins = "gpio44";
			function = "gpio";
			bias-disable;
		};

		mux_2 {
			pins = "gpio45";
			function = "gpio";
			bias-disable;
		};
	};

	cx2902x_reset: cx2902x_pinmux {
		mux_1 {
			pins = "gpio64";
			function = "gpio";
			bias-disable;
		};

		mux_2 {
			pins = "gpio65";
			function = "gpio";
			bias-disable;
		};
	};

	lte_pins: lte_pinmux {
		mux_en {
			pins = "gpio20";
			function = "gpio";
			output-high;
		};

		mux_reset {
			pins = "gpio35";
			function = "gpio";
			input;
		};
	};

	usb3_pins: usb3_pinmux {
		mux_en {
			pins = "gpio36";
			function = "gpio";
			output-high;
		};

		mux_flt {
			pins = "gpio4";
			function = "gpio";
			input;
		};
	};

	mcu_pins: mcu_pinmux {
		mux_boot {
			pins = "gpio38";
			function = "gpio";
			output-low;
		};

		mux_reset {
			pins = "gpio5";
			function = "gpio";
			output-high;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&blsp1_i2c4 {
	/*
	 * There is no driver for the following devices:
	 * - CY8C4014LQI@14	: Touch-Sensor for buttons on top
	 * - MINI54FDE@15	: MCU for Fan/RGB LED/Thermal control
	 * - ALC5629@18		: I2S/PCM Audio DAC
	 * - CX20924@41		: Voice Input Processor
	 */
	pinctrl-0 = <&i2c_1_pins>;
	pinctrl-names = "default";
	status = "okay";

	led-controller@32 {
		compatible = "ti,lp55231";
		reg = <0x32>;
		clock-mode = /bits/ 8 <0>;
		enable-gpios = <&tlmm 1 GPIO_ACTIVE_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;

		led@0 {
			chan-name = "green:wan";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x0>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN;
		};

		led@1 {
			chan-name = "blue:wan";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x1>;
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WAN;
		};

		led@2 {
			chan-name = "green:lan";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x2>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
		};

		led@3 {
			chan-name = "blue:lan";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x3>;
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_LAN;
		};

		led@4 {
			chan-name = "green:wlan-2";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x4>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <2>;
			linux,default-trigger = "phy0tpt";
		};

		led@5 {
			chan-name = "blue:wlan-2";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x5>;
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <2>;
		};

		led@6 {
			chan-name = "red:wan";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x6>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WAN;
		};

		led@7 {
			chan-name = "red:lan";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x7>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_LAN;
		};

		led@8 {
			chan-name = "red:wlan-2";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x8>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <2>;
		};
	};

	led-controller@33 {
		compatible = "ti,lp55231";
		reg = <0x33>;
		clock-mode = /bits/ 8 <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		led@0 {
			chan-name = "green:wlan-5";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x0>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			linux,default-trigger = "phy1tpt";
			function-enumerator = <5>;
		};

		led@1 {
			chan-name = "blue:wlan-5";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x1>;
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <5>;
		};

		led@2 {
			chan-name = "green:wan-4";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x2>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN; /* WWAN/LTE/4G */
			function-enumerator = <4>; /* WWAN/LTE/4G */
		};

		led@3 {
			chan-name = "blue:wan-4";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x3>;
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WAN; /* WWAN/LTE/4G */
			function-enumerator = <4>; /* WWAN/LTE/4G */
		};

		led_cloud_green: led@4 {
			chan-name = "green:power";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x4>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
		};

		led@5 {
			chan-name = "blue:power";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x5>;
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_POWER;
		};

		led@6 {
			chan-name = "red:wlan-5";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x6>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <5>;
		};

		led@7 {
			chan-name = "red:wan-4";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x7>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WAN; /* WWAN/LTE/4G */
			function-enumerator = <4>; /* WWAN/LTE/4G */
		};

		led_cloud_red: led@8 {
			chan-name = "red:power";
			led-cur = /bits/ 8 <50>;
			max-cur = /bits/ 8 <100>;
			reg = <0x8>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_POWER;
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>, <&uart0_ctrl_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&blsp1_uart2 {
	pinctrl-0 = <&serial_1_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&crypto {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&mdio {
	status = "okay";
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
	reset-gpios = <&tlmm 41 GPIO_ACTIVE_LOW>;
};

&prng {
	status = "okay";
};

&vqmmc {
	status = "okay";
};

&sdhci {
	status = "okay";
	pinctrl-0 = <&sd_pins>;
	pinctrl-names = "default";
	vqmmc-supply = <&vqmmc>;
	non-removable;
	#address-cells = <1>;
	#size-cells = <0>;

	emmc@0 {
		compatible = "mmc-card";
		reg = <0>;

		block {
			compatible = "block-device";
			partitions {
				block-partition-art {
					partname = "ART";

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						precal_art_1000: pre-calibration@1000 {
							reg = <0x1000 0x2f20>;
						};

						precal_art_5000: pre-calibration@5000 {
							reg = <0x5000 0x2f20>;
						};
					};
				};
			};
		};
	};
};

&usb2 {
	status = "okay";
};

&usb2_hs_phy {
	status = "okay";
};

&usb3 {
	status = "okay";

	pinctrl-0 = <&usb3_pins>, <&lte_pins>;
	pinctrl-names = "default";
};

&usb3_dwc {
	#address-cells = <1>;
	#size-cells = <0>;

	device@1 {
		compatible = "usb1bc7,1900";
		reg = <1>;
	};
};

&usb3_hs_phy {
	status = "okay";
};

&usb3_ss_phy {
	status = "okay";
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport4 {
	status = "okay";
	label = "lan";
};

&swport5 {
	status = "okay";
	label = "wan";
};

&wifi0 {
	status = "okay";
	qcom,ath10k-calibration-variant = "Sony-NCP-HG100-Cellular";
	nvmem-cells = <&precal_art_1000>;
	nvmem-cell-names = "pre-calibration";
};

&wifi1 {
	status = "okay";
	qcom,ath10k-calibration-variant = "Sony-NCP-HG100-Cellular";
	nvmem-cells = <&precal_art_5000>;
	nvmem-cell-names = "pre-calibration";
};

&watchdog {
	status = "okay";
};
