From 19e00bdfbb1b5f7a2d1f3c1c38b3da25e17ea486 Mon Sep 17 00:00:00 2001
From: George Moussalem <george.moussalem@outlook.com>
Date: Mon, 8 Jun 2026 09:09:16 +0400
Subject: [PATCH] dt-bindings: net: ethernet-phy: increase max clock count to
 two

The clocks property has a restriction to maximum one.
Yet, some PHYs may require more than 1 clock such as the IPQ5018 PHY
which requires two clocks for RX and TX. As such, increase maxItems to
two.

Reviewed-by: Rob Herring (Arm) <robh@kernel.org>
Signed-off-by: George Moussalem <george.moussalem@outlook.com>
Link: https://patch.msgid.link/20260608-ipq5018-gephy-clocks-v4-1-fb2ccd56894b@outlook.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 Documentation/devicetree/bindings/net/ethernet-phy.yaml | 9 ++++++---
 1 file changed, 6 insertions(+), 3 deletions(-)

--- a/Documentation/devicetree/bindings/net/ethernet-phy.yaml
+++ b/Documentation/devicetree/bindings/net/ethernet-phy.yaml
@@ -102,10 +102,13 @@ properties:
       by software.
 
   clocks:
-    maxItems: 1
+    minItems: 1
+    maxItems: 2
     description:
-      External clock connected to the PHY. If not specified it is assumed
-      that the PHY uses a fixed crystal or an internal oscillator.
+      External clock connected to the PHY or RX and TX clocks that the PHY
+      requires to enable explicitly. If not specified it is assumed
+      that the PHY uses a fixed crystal or an internal oscillator or that the
+      RX/TX clocks are hardware enabled by default.
 
   enet-phy-lane-swap:
     $ref: /schemas/types.yaml#/definitions/flag
