From dca5896703826d0d5fadcc11ee755b83db705571 Mon Sep 17 00:00:00 2001
From: Chukun Pan <amadeus@jmu.edu.cn>
Date: Mon,  1 Dec 2025 18:00:06 +0800
Subject: [PATCH] arm64: dts: rockchip: Add HINLINK H28K

The HINLINK H28K is a development board with the
Rockchip RK3528 SoC. It has the following features:

- 1x USB 2.0
- 8/32GB eMMC
- 1/2/4GB LPDDR4
- MicroSD card slot
- 1x 1GbE RTL8111H Ethernet
- 1x 1GbE RTL8211F Ethernet

Signed-off-by: Chukun Pan <amadeus@jmu.edu.cn>
---
 arch/arm64/boot/dts/rockchip/Makefile         |   1 +
 .../boot/dts/rockchip/rk3528-hinlink-h28k.dts | 301 ++++++++++++++++++
 2 files changed, 302 insertions(+)
 create mode 100644 arch/arm64/boot/dts/rockchip/rk3528-hinlink-h28k.dts

--- a/arch/arm64/boot/dts/rockchip/Makefile
+++ b/arch/arm64/boot/dts/rockchip/Makefile
@@ -90,6 +90,7 @@ dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-sa
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-sapphire-excavator.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399pro-rock-pi-n10.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3528-armsom-sige1.dtb
+dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3528-hinlink-h28k.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3528-nanopi-zero2.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3528-radxa-e20c.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3528-rock-2a.dtb
--- /dev/null
+++ b/arch/arm64/boot/dts/rockchip/rk3528-hinlink-h28k.dts
@@ -0,0 +1,318 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+
+/dts-v1/;
+
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/leds/common.h>
+#include <dt-bindings/pwm/pwm.h>
+#include "rk3528.dtsi"
+
+/ {
+	model = "HINLINK H28K";
+	compatible = "hinlink,h28k", "rockchip,rk3528";
+
+	aliases {
+		ethernet0 = &gmac1;
+		mmc0 = &sdhci;
+		mmc1 = &sdmmc;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:1500000n8";
+	};
+
+	keys {
+		compatible = "adc-keys";
+		io-channels = <&saradc 0>;
+		io-channel-names = "buttons";
+		keyup-threshold-microvolt = <1800000>;
+		poll-interval = <100>;
+
+		button-boot {
+			label = "BOOT";
+			linux,code = <KEY_SETUP>;
+			press-threshold-microvolt = <0>;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&lan_led>, <&wan_led>, <&work_led>;
+
+		led-0 {
+			color = <LED_COLOR_ID_AMBER>;
+			function = LED_FUNCTION_LAN;
+			gpios = <&gpio4 RK_PC1 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "netdev";
+		};
+
+		led-1 {
+			color = <LED_COLOR_ID_BLUE>;
+			function = LED_FUNCTION_WAN;
+			gpios = <&gpio4 RK_PC0 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "netdev";
+		};
+
+		led-2 {
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_STATUS;
+			gpios = <&gpio4 RK_PB7 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-on";
+		};
+	};
+
+	vdd_0v9: regulator-0v9-vdd {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd_0v9";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <900000>;
+		regulator-max-microvolt = <900000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
+	vcc_ddr: regulator-1v1-vcc-ddr {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_ddr";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1100000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
+	vcc_1v8: regulator-1v8-vcc {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_1v8";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		vin-supply = <&vcc_3v3>;
+	};
+
+	vcc_3v3: regulator-3v3-vcc {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_3v3";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
+	vcc3v3_sd: regulator-3v3-vcc-sd {
+		compatible = "regulator-fixed";
+		gpios = <&gpio4 RK_PA1 GPIO_ACTIVE_LOW>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&sdmmc_pwren_l>;
+		regulator-name = "vcc3v3_sd";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc_3v3>;
+	};
+
+	vcc5v0_sys: regulator-5v0-vcc-sys {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc5v0_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+	};
+
+	vccio_sd: regulator-vccio-sd {
+		compatible = "regulator-gpio";
+		gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&sdmmc_vol_ctrl_h>;
+		regulator-name = "vccio_sd";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <3300000>;
+		states = <1800000 0x0>, <3300000 0x1>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
+	vdd_arm: regulator-vdd-arm {
+		compatible = "pwm-regulator";
+		pwms = <&pwm1 0 5000 PWM_POLARITY_INVERTED>;
+		pwm-supply = <&vcc5v0_sys>;
+		regulator-name = "vdd_arm";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <746000>;
+		regulator-max-microvolt = <1201000>;
+		regulator-settling-time-up-us = <250>;
+	};
+
+	vdd_logic: regulator-vdd-logic {
+		compatible = "pwm-regulator";
+		pwms = <&pwm2 0 5000 PWM_POLARITY_INVERTED>;
+		pwm-supply = <&vcc5v0_sys>;
+		regulator-name = "vdd_logic";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <705000>;
+		regulator-max-microvolt = <1006000>;
+		regulator-settling-time-up-us = <250>;
+	};
+};
+
+&combphy {
+	status = "okay";
+};
+
+&cpu0 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu1 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu2 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu3 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&gmac1 {
+	clock_in_out = "output";
+	phy-handle = <&rgmii_phy>;
+	phy-mode = "rgmii-id";
+	phy-supply = <&vcc_3v3>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmii_miim>,
+		    <&rgmii_tx_bus2>,
+		    <&rgmii_rx_bus2>,
+		    <&rgmii_rgmii_clk>,
+		    <&rgmii_rgmii_bus>;
+	status = "okay";
+};
+
+&gpu {
+	mali-supply = <&vdd_logic>;
+	status = "okay";
+};
+
+&mdio1 {
+	rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <0x1>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&gmac1_rstn_l>;
+		reset-assert-us = <20000>;
+		reset-deassert-us = <100000>;
+		reset-gpios = <&gpio4 RK_PC2 GPIO_ACTIVE_LOW>;
+	};
+};
+
+&pcie {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rtl8111hs_isolateb_l>;
+	reset-gpios = <&gpio4 RK_PA3 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc_3v3>;
+	status = "okay";
+};
+
+&pinctrl {
+	gmac {
+		gmac1_rstn_l: gmac1-rstn-l {
+			rockchip,pins = <4 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	leds {
+		lan_led: lan-led {
+			rockchip,pins = <4 RK_PC1 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		wan_led: wan-led {
+			rockchip,pins = <4 RK_PC0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		work_led: work-led {
+			rockchip,pins = <4 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	pcie {
+		rtl8111hs_isolateb_l: rtl8111hs-isolateb-l {
+			rockchip,pins = <4 RK_PA6 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	sdmmc {
+		sdmmc_pwren_l: sdmmc-pwren-l {
+			rockchip,pins = <4 RK_PA1 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		sdmmc_vol_ctrl_h: sdmmc-vol-ctrl-h {
+			rockchip,pins = <4 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+};
+
+&pwm1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pwm1m0_pins>;
+	status = "okay";
+};
+
+&pwm2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pwm2m0_pins>;
+	status = "okay";
+};
+
+&saradc {
+	vref-supply = <&vcc_1v8>;
+	status = "okay";
+};
+
+&sdhci {
+	bus-width = <8>;
+	cap-mmc-highspeed;
+	mmc-hs200-1_8v;
+	non-removable;
+	vmmc-supply = <&vcc_3v3>;
+	vqmmc-supply = <&vcc_1v8>;
+	status = "okay";
+};
+
+&sdmmc {
+	bus-width = <4>;
+	cap-sd-highspeed;
+	disable-wp;
+	sd-uhs-sdr104;
+	vmmc-supply = <&vcc3v3_sd>;
+	vqmmc-supply = <&vccio_sd>;
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0m0_xfer>;
+	status = "okay";
+};
+
+&usb2phy {
+	status = "okay";
+};
+
+&usb2phy_host {
+	phy-supply = <&vcc5v0_sys>;
+	status = "okay";
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
