From 5dd98e0389545b302b0c46cef2264b5b09c01677 Mon Sep 17 00:00:00 2001
From: Aleksander Jan Bajkowski <olek2@wp.pl>
Date: Sun, 24 May 2026 14:44:53 +0200
Subject: [PATCH] arm64: dts: marvell: armada-37xx: mark EIP97 as dma-coherent

Armada 37xx has coherent bus, similar to Armada 7k/8k. Cache
synchronization consumes a lot of CPU cycles. Enabling coherent DMA
increases IOPS performance up to 4 times. Some numbers:
					Data length
Algo		MB	   16	  64	 128	 256	1024	1424	4096
DES-ECB		1	+21 %	+5 %	+5 %	+7 %	+7 %	+3 %	+20 %
AES-ECB-128	1	+21 %	+6 %	+6 %	+6 %	+9 %	+8 %	+22 %
AES-CBC-128	1	+21 %	+5 %	+5 %	+5 %	+6 %	+7 %	+23 %
AES-CBC-256	1	+23 %	+7 %	+8 %	+6 %	+11 %	+13 %	+20 %

					Data length
Algo		MB	    16	    64	   256	  512	  1024	 1420	 4096	 8192
AES-GCM-128	1	 +44 %	 +42 %	 +31 %	 +32 %	 +27 %	+30 %	+32 %	+30 %
AES-GCM-128	8	+319 %	+326 %	+163 %	+148 %	 +75 %	+72 %	+74 %	+41 %
AES-GCM-128	4096	+123 %	+128 %	 +90 %	 +83 %	+116 %	+59 %	+38 %	+28 %

					Data length
Algo		MB	   16	   64	  256	 1024	 2048	 4096	 8192
MD5		1	+21 %	+15 %	+29 %	+25 %	+50 %	+16 %	+20 %
SHA1		1	+24 %	+22 %	+27 %	+22 %	+18 %	+20 %	+20 %
SHA256		1	+30 %	+24 %	+25 %	+26 %	+21 %	+41 %	+19 %
SHA512		1	 +4 %	 +3 %	 +8 %	+10 %	+24 %	+10 %	+11 %

Tested on Armada 3720. Platform passes testmgr selftests.

Signed-off-by: Aleksander Jan Bajkowski <olek2@wp.pl>
Signed-off-by: Gregory CLEMENT <gregory.clement@bootlin.com>
---
 arch/arm64/boot/dts/marvell/armada-37xx.dtsi | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm64/boot/dts/marvell/armada-37xx.dtsi
+++ b/arch/arm64/boot/dts/marvell/armada-37xx.dtsi
@@ -438,6 +438,7 @@
 				interrupt-names = "ring0", "ring1", "ring2",
 						  "ring3", "eip", "mem";
 				clocks = <&nb_periph_clk 15>;
+				dma-coherent;
 			};
 
 			rwtm: mailbox@b0000 {
