From c06a2f2903f6fba0a3088ad05fc5cf61a66e5d89 Mon Sep 17 00:00:00 2001
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Tue, 28 Apr 2026 07:23:38 +0200
Subject: [PATCH] net: airoha: Rename get_src_port_id callback in get_sport

For code consistency, rename get_src_port_id callback in get_sport.
Please note this patch does not introduce any logical change and it is
just a cosmetic patch.

Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Link: https://patch.msgid.link/20260428-airoha-get_src_port_id-callback-v1-1-3f765c91c1e8@kernel.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/airoha/airoha_eth.c | 10 +++++-----
 drivers/net/ethernet/airoha/airoha_eth.h |  2 +-
 2 files changed, 6 insertions(+), 6 deletions(-)

--- a/drivers/net/ethernet/airoha/airoha_eth.c
+++ b/drivers/net/ethernet/airoha/airoha_eth.c
@@ -1825,7 +1825,7 @@ static int airoha_set_gdm2_loopback(stru
 	airoha_fe_clear(eth, REG_FE_VIP_PORT_EN, BIT(AIROHA_GDM2_IDX));
 	airoha_fe_clear(eth, REG_FE_IFC_PORT_EN, BIT(AIROHA_GDM2_IDX));
 
-	src_port = eth->soc->ops.get_src_port_id(port, port->nbq);
+	src_port = eth->soc->ops.get_sport(port, port->nbq);
 	if (src_port < 0)
 		return src_port;
 
@@ -3199,7 +3199,7 @@ static const char * const en7581_xsi_rst
 	"xfp-mac",
 };
 
-static int airoha_en7581_get_src_port_id(struct airoha_gdm_port *port, int nbq)
+static int airoha_en7581_get_sport(struct airoha_gdm_port *port, int nbq)
 {
 	switch (port->id) {
 	case AIROHA_GDM3_IDX:
@@ -3252,7 +3252,7 @@ static const char * const an7583_xsi_rst
 	"xfp-mac",
 };
 
-static int airoha_an7583_get_src_port_id(struct airoha_gdm_port *port, int nbq)
+static int airoha_an7583_get_sport(struct airoha_gdm_port *port, int nbq)
 {
 	switch (port->id) {
 	case AIROHA_GDM3_IDX:
@@ -3300,7 +3300,7 @@ static const struct airoha_eth_soc_data
 	.num_xsi_rsts = ARRAY_SIZE(en7581_xsi_rsts_names),
 	.num_ppe = 2,
 	.ops = {
-		.get_src_port_id = airoha_en7581_get_src_port_id,
+		.get_sport = airoha_en7581_get_sport,
 		.get_vip_port = airoha_en7581_get_vip_port,
 	},
 };
@@ -3311,7 +3311,7 @@ static const struct airoha_eth_soc_data
 	.num_xsi_rsts = ARRAY_SIZE(an7583_xsi_rsts_names),
 	.num_ppe = 1,
 	.ops = {
-		.get_src_port_id = airoha_an7583_get_src_port_id,
+		.get_sport = airoha_an7583_get_sport,
 		.get_vip_port = airoha_an7583_get_vip_port,
 	},
 };
--- a/drivers/net/ethernet/airoha/airoha_eth.h
+++ b/drivers/net/ethernet/airoha/airoha_eth.h
@@ -578,7 +578,7 @@ struct airoha_eth_soc_data {
 	int num_xsi_rsts;
 	int num_ppe;
 	struct {
-		int (*get_src_port_id)(struct airoha_gdm_port *port, int nbq);
+		int (*get_sport)(struct airoha_gdm_port *port, int nbq);
 		u32 (*get_vip_port)(struct airoha_gdm_port *port, int nbq);
 	} ops;
 };
