From b38140838f1f6b4e1f89130ab18d10ad404caf54 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Thu, 28 Mar 2024 16:16:37 +0000
Subject: [PATCH] Revert "usb: phy: generic: Get the vbus supply"

This reverts commit 03e607cbb2931374db1825f371e9c7f28526d3f4.
---
 drivers/usb/phy/phy-generic.c | 7 -------
 1 file changed, 7 deletions(-)

--- a/drivers/usb/phy/phy-generic.c
+++ b/drivers/usb/phy/phy-generic.c
@@ -256,13 +256,6 @@ int usb_phy_gen_create_phy(struct device
 		return dev_err_probe(dev, PTR_ERR(nop->vcc),
 				     "could not get vcc regulator\n");
 
-	nop->vbus_draw = devm_regulator_get_exclusive(dev, "vbus");
-	if (PTR_ERR(nop->vbus_draw) == -ENODEV)
-		nop->vbus_draw = NULL;
-	if (IS_ERR(nop->vbus_draw))
-		return dev_err_probe(dev, PTR_ERR(nop->vbus_draw),
-				     "could not get vbus regulator\n");
-
 	nop->dev		= dev;
 	nop->phy.dev		= nop->dev;
 	nop->phy.label		= "nop-xceiv";
