From 124ef4a79d8054f84c22a60d79ccd82646b6402a Mon Sep 17 00:00:00 2001
From: Weijie Gao <weijie.gao@mediatek.com>
Date: Fri, 29 Jul 2022 17:04:12 +0800
Subject: [PATCH 17/30] board: mt7981: add reference board using new spi-nand
 driver

Add a new reference board using new spi-nand driver for SPI-NAND flash on
SNFI interface

Signed-off-by: Weijie Gao <weijie.gao@mediatek.com>
---
 arch/arm/dts/Makefile                  |   1 +
 arch/arm/dts/mt7981-snfi-nand-rfb.dts  | 132 +++++++++++++++++++++++++
 configs/mt7981_snfi_nand_rfb_defconfig |  57 +++++++++++
 3 files changed, 190 insertions(+)
 create mode 100644 arch/arm/dts/mt7981-snfi-nand-rfb.dts
 create mode 100644 configs/mt7981_snfi_nand_rfb_defconfig

--- a/arch/arm/dts/Makefile
+++ b/arch/arm/dts/Makefile
@@ -1099,6 +1099,7 @@ dtb-$(CONFIG_ARCH_MEDIATEK) += \
 	mt7622-bananapi-bpi-r64.dtb \
 	mt7623n-bananapi-bpi-r2.dtb \
 	mt7981-rfb.dtb \
+	mt7981-snfi-nand-rfb.dtb \
 	mt7981-emmc-rfb.dtb \
 	mt7981-sd-rfb.dtb \
 	mt7986a-bpi-r3-sd.dtb \
--- /dev/null
+++ b/arch/arm/dts/mt7981-snfi-nand-rfb.dts
@@ -0,0 +1,132 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (c) 2021 MediaTek Inc.
+ * Author: Sam Shih <sam.shih@mediatek.com>
+ */
+
+/dts-v1/;
+#include "mt7981.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	#address-cells = <1>;
+	#size-cells = <1>;
+	model = "mt7981-rfb";
+	compatible = "mediatek,mt7981", "mediatek,mt7981-rfb";
+	chosen {
+		stdout-path = &uart0;
+		tick-timer = &timer0;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>;
+	status = "disabled";
+};
+
+&eth {
+	status = "okay";
+	mediatek,gmac-id = <0>;
+	phy-mode = "sgmii";
+	mediatek,switch = "mt7531";
+	reset-gpios = <&pio 39 GPIO_ACTIVE_HIGH>;
+
+	fixed-link {
+		speed = <1000>;
+		full-duplex;
+	};
+};
+
+&pio {
+	snfi_pins: snfi-pins-func-1 {
+		mux {
+			function = "flash";
+			groups = "snfi";
+		};
+
+		clk {
+			pins = "SPI0_CLK";
+			drive-strength = <MTK_DRIVE_8mA>;
+			bias-pull-down = <MTK_PUPD_SET_R1R0_00>;
+		};
+
+		conf-pu {
+			pins = "SPI0_CS", "SPI0_HOLD", "SPI0_WP";
+			drive-strength = <MTK_DRIVE_6mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_00>;
+		};
+
+		conf-pd {
+			pins = "SPI0_MOSI", "SPI0_MISO";
+			drive-strength = <MTK_DRIVE_6mA>;
+			bias-pull-down = <MTK_PUPD_SET_R1R0_00>;
+		};
+	};
+
+	spic_pins: spi1-pins-func-1 {
+		mux {
+			function = "spi";
+			groups = "spi1_1";
+		};
+	};
+
+	uart1_pins: spi1-pins-func-3 {
+		mux {
+			function = "uart";
+			groups = "uart1_2";
+		};
+	};
+
+	/* pin15 as pwm0 */
+	one_pwm_pins: one-pwm-pins {
+		mux {
+			function = "pwm";
+			groups = "pwm0_1";
+		};
+	};
+
+	/* pin15 as pwm0 and pin14 as pwm1 */
+	two_pwm_pins: two-pwm-pins {
+		mux {
+			function = "pwm";
+			groups = "pwm0_1", "pwm1_0";
+		};
+	};
+
+	/* pin15 as pwm0, pin14 as pwm1, pin7 as pwm2 */
+	three_pwm_pins: three-pwm-pins {
+		mux {
+			function = "pwm";
+			groups = "pwm0_1", "pwm1_0", "pwm2";
+		};
+	};
+
+	mmc0_pins_default: mmc0default {
+                mux {
+                       function = "flash";
+                       groups =  "emmc_45";
+                 };
+         };
+};
+
+&snand {
+	pinctrl-names = "default";
+	pinctrl-0 = <&snfi_pins>;
+	status = "okay";
+	quad-spi;
+};
+
+&pwm {
+	pinctrl-names = "default";
+	pinctrl-0 = <&two_pwm_pins>;
+	status = "okay";
+};
+
+&watchdog {
+	status = "disabled";
+};
--- /dev/null
+++ b/configs/mt7981_snfi_nand_rfb_defconfig
@@ -0,0 +1,58 @@
+CONFIG_ARM=y
+CONFIG_SYS_HAS_NONCACHED_MEMORY=y
+CONFIG_POSITION_INDEPENDENT=y
+CONFIG_ARCH_MEDIATEK=y
+CONFIG_TEXT_BASE=0x41e00000
+CONFIG_SYS_MALLOC_F_LEN=0x4000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_ENV_SIZE=0x20000
+CONFIG_DEFAULT_DEVICE_TREE="mt7981-snfi-nand-rfb"
+# CONFIG_BOARD_INIT is not set
+CONFIG_SYS_PROMPT="MT7981> "
+CONFIG_TARGET_MT7981=y
+CONFIG_DEBUG_UART_BASE=0x11002000
+CONFIG_DEBUG_UART_CLOCK=40000000
+CONFIG_SYS_LOAD_ADDR=0x46000000
+CONFIG_DEBUG_UART=y
+# CONFIG_AUTOBOOT is not set
+CONFIG_DEFAULT_FDT_FILE="mt7981-snfi-nand-rfb"
+CONFIG_LOGLEVEL=7
+CONFIG_LOG=y
+CONFIG_SYS_CBSIZE=512
+CONFIG_SYS_PBSIZE=1049
+# CONFIG_BOOTM_NETBSD is not set
+# CONFIG_BOOTM_PLAN9 is not set
+# CONFIG_BOOTM_RTEMS is not set
+# CONFIG_BOOTM_VXWORKS is not set
+# CONFIG_CMD_ELF is not set
+# CONFIG_CMD_UNLZ4 is not set
+# CONFIG_CMD_UNZIP is not set
+CONFIG_CMD_GPIO=y
+CONFIG_CMD_MTD=y
+CONFIG_CMD_PING=y
+CONFIG_CMD_SMC=y
+CONFIG_MTDIDS_DEFAULT="spi-nand0=spi-nand0"
+CONFIG_MTDPARTS_DEFAULT="spi-nand0:1024k(bl2),512k(u-boot-env),2048k(factory),2048k(fip),65536k(ubi)"
+CONFIG_CMD_UBI=y
+CONFIG_CMD_UBI_RENAME=y
+CONFIG_ENV_OVERWRITE=y
+CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
+CONFIG_NET_RANDOM_ETHADDR=y
+CONFIG_REGMAP=y
+CONFIG_SYSCON=y
+CONFIG_CLK=y
+# CONFIG_MMC is not set
+CONFIG_MTD=y
+CONFIG_DM_MTD=y
+CONFIG_MTK_SPI_NAND=y
+CONFIG_MTK_SPI_NAND_MTD=y
+CONFIG_PHY_FIXED=y
+CONFIG_MEDIATEK_ETH=y
+CONFIG_PINCTRL=y
+CONFIG_PINCONF=y
+CONFIG_PINCTRL_MT7981=y
+CONFIG_POWER_DOMAIN=y
+CONFIG_MTK_POWER_DOMAIN=y
+CONFIG_DM_SERIAL=y
+CONFIG_MTK_SERIAL=y
+CONFIG_HEXDUMP=y
