From 3e5127469a8d41153fb30031a271788f52dd17ec Mon Sep 17 00:00:00 2001
From: Nitheesh Sekar <quic_nsekar@quicinc.com>
Date: Wed, 26 Mar 2025 12:10:58 +0400
Subject: [PATCH] PCI: qcom: Add support for IPQ5018

Add IPQ5018 platform with is based on Qcom IP rev. 2.9.0 and Synopsys IP
rev. 5.00a.

The platform itself has two PCIe Gen2 controllers: one single-lane and
one dual-lane. So add the IPQ5018 compatible and re-use 2_9_0 ops.

Signed-off-by: Nitheesh Sekar <quic_nsekar@quicinc.com>
Signed-off-by: Sricharan R <quic_srichara@quicinc.com>
Signed-off-by: George Moussalem <george.moussalem@outlook.com>
Signed-off-by: Manivannan Sadhasivam <manivannan.sadhasivam@linaro.org>
Reviewed-by: Manivannan Sadhasivam <manivannan.sadhasivam@linaro.org>
Link: https://patch.msgid.link/20250326-ipq5018-pcie-v7-4-e1828fef06c9@outlook.com
---
 drivers/pci/controller/dwc/pcie-qcom.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/pci/controller/dwc/pcie-qcom.c
+++ b/drivers/pci/controller/dwc/pcie-qcom.c
@@ -1832,6 +1832,7 @@ static const struct of_device_id qcom_pc
 	{ .compatible = "qcom,pcie-apq8064", .data = &cfg_2_1_0 },
 	{ .compatible = "qcom,pcie-apq8084", .data = &cfg_1_0_0 },
 	{ .compatible = "qcom,pcie-ipq4019", .data = &cfg_2_4_0 },
+	{ .compatible = "qcom,pcie-ipq5018", .data = &cfg_2_9_0 },
 	{ .compatible = "qcom,pcie-ipq6018", .data = &cfg_2_9_0 },
 	{ .compatible = "qcom,pcie-ipq8064", .data = &cfg_2_1_0 },
 	{ .compatible = "qcom,pcie-ipq8064-v2", .data = &cfg_2_1_0 },
