// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6368.dtsi"

/ {
	model = "Netgear EVG2000";
	compatible = "netgear,evg2000", "brcm,bcm6369", "brcm,bcm6368";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 25 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led-2 {
			label = "green:voip2";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		led-4 {
			label = "red:internet";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		led-5 {
			label = "green:internet";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		led-14 {
			label = "green:voip1";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		led-15 {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led_power_green: led-22 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		led_power_red: led-23 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			panic-indicator;
		};

		led-24 {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 24 GPIO_ACTIVE_LOW>;
		};

		led-27 {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 27 GPIO_ACTIVE_LOW>;
		};
	};

	bcm4322-sprom {
		compatible = "brcm,ssb-sprom";

		pci-bus = <0>;
		pci-dev = <1>;

		nvmem-cells = <&macaddr_cfe_6a0 1>;
		nvmem-cell-names = "mac-address";

		brcm,sprom = "brcm/bcm4322-sprom.bin";
		brcm,sprom-fixups = <219 0xec08>;
	};
};

&ehci {
	status = "okay";
};

&ethernet {
	status = "okay";

	nvmem-cells = <&macaddr_cfe_6a0 0>;
	nvmem-cell-names = "mac-address";
};

&mdio_ext {
	switch@1e {
		compatible = "brcm,bcm53115";
		reg = <30>;

		dsa,member = <1 0>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "wan";
			};

			port@1 {
				reg = <1>;
				label = "lan1";
			};

			port@2 {
				reg = <2>;
				label = "lan2";
			};

			port@3 {
				reg = <3>;
				label = "lan3";
			};

			port@4 {
				reg = <4>;
				label = "lan4";
			};

			port@8 {
				reg = <8>;

				phy-mode = "rgmii-id";
				ethernet = <&switch0port5>;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};
	};
};

&switch0 {
	dsa,member = <0 0>;

	ports {
		switch0port5: port@5 {
			reg = <5>;
			label = "extsw";

			phy-mode = "rgmii-id";

			fixed-link {
				speed = <1000>;
				full-duplex;
			};
		};
	};
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "CFE";
			reg = <0x000000 0x020000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_cfe_6a0: macaddr@6a0 {
					compatible = "mac-base";
					reg = <0x6a0 0x6>;
					#nvmem-cell-cells = <1>;
				};
			};
		};

		partition@20000 {
			label = "firmware";
			reg = <0x020000 0xf40000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		partition@f60000 {
			label = "board_data";
			reg = <0xf60000 0x080000>;
			read-only;
		};

		partition@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&ohci {
	status = "okay";
};

&pci {
	status = "okay";
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};
