From: Christian Marangi <ansuelsmth@gmail.com>
To: Christian Marangi <ansuelsmth@gmail.com>,
	Lee Jones <lee@kernel.org>, Rob Herring <robh@kernel.org>,
	Krzysztof Kozlowski <krzk+dt@kernel.org>,
	Conor Dooley <conor+dt@kernel.org>,
	Andrew Lunn <andrew+netdev@lunn.ch>,
	"David S. Miller" <davem@davemloft.net>,
	Eric Dumazet <edumazet@google.com>,
	Jakub Kicinski <kuba@kernel.org>, Paolo Abeni <pabeni@redhat.com>,
	Vladimir Oltean <olteanv@gmail.com>,
	Srinivas Kandagatla <srinivas.kandagatla@linaro.org>,
	Heiner Kallweit <hkallweit1@gmail.com>,
	Russell King <linux@armlinux.org.uk>,
	Matthias Brugger <matthias.bgg@gmail.com>,
	AngeloGioacchino Del Regno
	<angelogioacchino.delregno@collabora.com>,
	linux-arm-kernel@lists.infradead.org,
	linux-mediatek@lists.infradead.org, netdev@vger.kernel.org,
	devicetree@vger.kernel.org, linux-kernel@vger.kernel.org,
	upstream@airoha.com
Subject: [net-next PATCH v11 0/9] net: dsa: Add Airoha AN8855 support
Date: Mon,  9 Dec 2024 14:44:17 +0100	[thread overview]
Message-ID: <20241209134459.27110-1-ansuelsmth@gmail.com> (raw)

This small series add the initial support for the Airoha AN8855 Switch.

It's a 5 port Gigabit Switch with SGMII/HSGMII upstream port.

This is starting to get in the wild and there are already some router
having this switch chip.

It's conceptually similar to mediatek switch but register and bits
are different. And there is that massive Hell that is the PCS
configuration.
Saddly for that part we have absolutely NO documentation currently.

There is this special thing where PHY needs to be calibrated with values
from the switch efuse. (the thing have a whole cpu timer and MCU)

---
 .../bindings/mfd/airoha,an8855-mfd.yaml       |  178 ++
 .../bindings/net/airoha,an8855-mdio.yaml      |   56 +
 .../net/dsa/airoha,an8855-switch.yaml         |  105 +
 .../bindings/nvmem/airoha,an8855-efuse.yaml   |  123 +
 MAINTAINERS                                   |   17 +
 drivers/mfd/Kconfig                           |   10 +
 drivers/mfd/Makefile                          |    1 +
 drivers/mfd/airoha-an8855.c                   |  278 ++
 drivers/net/dsa/Kconfig                       |    9 +
 drivers/net/dsa/Makefile                      |    1 +
 drivers/net/dsa/an8855.c                      | 2310 +++++++++++++++++
 drivers/net/dsa/an8855.h                      |  783 ++++++
 drivers/net/mdio/Kconfig                      |    9 +
 drivers/net/mdio/Makefile                     |    1 +
 drivers/net/mdio/mdio-an8855.c                |  113 +
 drivers/net/phy/Kconfig                       |    5 +
 drivers/net/phy/Makefile                      |    1 +
 drivers/net/phy/air_an8855.c                  |  267 ++
 drivers/nvmem/Kconfig                         |   11 +
 drivers/nvmem/Makefile                        |    2 +
 drivers/nvmem/an8855-efuse.c                  |   63 +
 include/linux/mfd/airoha-an8855-mfd.h         |   41 +
 22 files changed, 4384 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/mfd/airoha,an8855-mfd.yaml
 create mode 100644 Documentation/devicetree/bindings/net/airoha,an8855-mdio.yaml
 create mode 100644 Documentation/devicetree/bindings/net/dsa/airoha,an8855-switch.yaml
 create mode 100644 Documentation/devicetree/bindings/nvmem/airoha,an8855-efuse.yaml
 create mode 100644 drivers/mfd/airoha-an8855.c
 create mode 100644 drivers/net/dsa/an8855.c
 create mode 100644 drivers/net/dsa/an8855.h
 create mode 100644 drivers/net/mdio/mdio-an8855.c
 create mode 100644 drivers/net/phy/air_an8855.c
 create mode 100644 drivers/nvmem/an8855-efuse.c
 create mode 100644 include/linux/mfd/airoha-an8855-mfd.h

--- a/drivers/mfd/Kconfig
+++ b/drivers/mfd/Kconfig
@@ -53,6 +53,16 @@ config MFD_ALTERA_SYSMGR
 	  using regmap_mmio accesses for ARM32 parts and SMC calls to
 	  EL3 for ARM64 parts.
 
+config MFD_AIROHA_AN8855
+	tristate "Airoha AN8855 Switch MFD"
+	select MFD_CORE
+	select MDIO_DEVICE
+	depends on NETDEVICES && OF
+	help
+	  Support for the Airoha AN8855 Switch MFD. This is a SoC Switch
+	  that provides various peripherals. Currently it provides a
+	  DSA switch and a NVMEM provider.
+
 config MFD_ACT8945A
 	tristate "Active-semi ACT8945A"
 	select MFD_CORE
--- a/drivers/mfd/Makefile
+++ b/drivers/mfd/Makefile
@@ -9,6 +9,7 @@ obj-$(CONFIG_MFD_88PM800)	+= 88pm800.o 8
 obj-$(CONFIG_MFD_88PM805)	+= 88pm805.o 88pm80x.o
 obj-$(CONFIG_MFD_88PM886_PMIC)	+= 88pm886.o
 obj-$(CONFIG_MFD_ACT8945A)	+= act8945a.o
+obj-$(CONFIG_MFD_AIROHA_AN8855)	+= airoha-an8855.o
 obj-$(CONFIG_MFD_SM501)		+= sm501.o
 obj-$(CONFIG_ARCH_BCM2835)	+= bcm2835-pm.o
 obj-$(CONFIG_MFD_BCM590XX)	+= bcm590xx.o
--- a/drivers/net/dsa/Kconfig
+++ b/drivers/net/dsa/Kconfig
@@ -24,6 +24,15 @@ config NET_DSA_LOOP
 	  This enables support for a fake mock-up switch chip which
 	  exercises the DSA APIs.
 
+config NET_DSA_AN8855
+	tristate "Airoha AN8855 Ethernet switch support"
+	depends on MFD_AIROHA_AN8855
+	depends on NET_DSA
+	select NET_DSA_TAG_MTK
+	help
+	  This enables support for the Airoha AN8855 Ethernet switch
+	  chip.
+
 source "drivers/net/dsa/hirschmann/Kconfig"
 
 source "drivers/net/dsa/lantiq/Kconfig"
--- a/drivers/net/dsa/Makefile
+++ b/drivers/net/dsa/Makefile
@@ -1,4 +1,5 @@
 # SPDX-License-Identifier: GPL-2.0
+obj-$(CONFIG_NET_DSA_AN8855)	+= an8855.o
 obj-$(CONFIG_NET_DSA_BCM_SF2)	+= bcm-sf2.o
 bcm-sf2-objs			:= bcm_sf2.o bcm_sf2_cfp.o
 obj-$(CONFIG_NET_DSA_LOOP)	+= dsa_loop.o
--- a/drivers/net/mdio/Kconfig
+++ b/drivers/net/mdio/Kconfig
@@ -44,6 +44,15 @@ config MDIO_XGENE
 	  This module provides a driver for the MDIO busses found in the
 	  APM X-Gene SoC's.
 
+config MDIO_AN8855
+	tristate "Airoha AN8855 Switch MDIO bus controller"
+	depends on MFD_AIROHA_AN8855
+	depends on OF_MDIO
+	help
+	  This module provides a driver for the Airoha AN8855 Switch
+	  that requires a MDIO passtrough as switch address is shared
+	  with the internal PHYs and requires additional page handling.
+
 config MDIO_ASPEED
 	tristate "ASPEED MDIO bus controller"
 	depends on ARCH_ASPEED || COMPILE_TEST
--- a/drivers/net/mdio/Makefile
+++ b/drivers/net/mdio/Makefile
@@ -6,6 +6,7 @@ obj-$(CONFIG_FWNODE_MDIO)	+= fwnode_mdio
 obj-$(CONFIG_OF_MDIO)		+= of_mdio.o
 
 obj-$(CONFIG_MDIO_AIROHA)		+= mdio-airoha.o
+obj-$(CONFIG_MDIO_AN8855)		+= mdio-an8855.o
 obj-$(CONFIG_MDIO_ASPEED)		+= mdio-aspeed.o
 obj-$(CONFIG_MDIO_BCM_IPROC)		+= mdio-bcm-iproc.o
 obj-$(CONFIG_MDIO_BCM_UNIMAC)		+= mdio-bcm-unimac.o
--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -175,6 +175,11 @@ config AIROHA_EN8801SC_PHY
 	help
 	  Currently supports the Airoha EN8801SC PHY.
 
+config AIR_AN8855_PHY
+	tristate "Airoha AN8855 Internal Gigabit PHY"
+	help
+	  Currently supports the internal Airoha AN8855 Switch PHY.
+
 config AIR_EN8811H_PHY
 	tristate "Airoha EN8811H 2.5 Gigabit PHY"
 	select PHY_COMMON_PROPS
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -45,6 +45,7 @@ obj-y				+= $(sfp-obj-y) $(sfp-obj-m)
 obj-$(CONFIG_ADIN_PHY)		+= adin.o
 obj-$(CONFIG_ADIN1100_PHY)	+= adin1100.o
 obj-$(CONFIG_AIROHA_EN8801SC_PHY)   += en8801sc.o
+obj-$(CONFIG_AIR_AN8855_PHY)		+= air_an8855.o
 obj-$(CONFIG_AIR_EN8811H_PHY)   += air_en8811h.o
 obj-$(CONFIG_AMD_PHY)		+= amd.o
 obj-$(CONFIG_AMCC_QT2025_PHY)	+= qt2025.o
--- a/drivers/nvmem/Kconfig
+++ b/drivers/nvmem/Kconfig
@@ -31,7 +31,7 @@ source "drivers/nvmem/layouts/Kconfig"
 
 config NVMEM_AN8855_EFUSE
 	tristate "Airoha AN8855 eFuse support"
-	depends on COMPILE_TEST
+	depends on MFD_AIROHA_AN8855 || COMPILE_TEST
 	help
 	  Say y here to enable support for reading eFuses on Airoha AN8855
 	  Switch. These are e.g. used to store factory programmed
