From 109a9c8409f85d777f8ffa3fe145498a1fec0f1e Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Thu, 8 May 2025 04:03:58 +0100
Subject: [PATCH] arm64: dts: mt7988a: add serial1 and serial2 aliases

Add aliases serial1 and serial2, so boards can make use of the
auxilary UARTs of the MediaTek MT7988 SoC.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 arch/arm64/boot/dts/mediatek/mt7988a.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/mediatek/mt7988a.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt7988a.dtsi
@@ -296,7 +296,7 @@
 			status = "disabled";
 		};
 
-		serial@11000100 {
+		serial1: serial@11000100 {
 			compatible = "mediatek,mt7988-uart", "mediatek,mt6577-uart";
 			reg = <0 0x11000100 0 0x100>;
 			interrupts = <GIC_SPI 124 IRQ_TYPE_LEVEL_HIGH>;
@@ -307,7 +307,7 @@
 			status = "disabled";
 		};
 
-		serial@11000200 {
+		serial2: serial@11000200 {
 			compatible = "mediatek,mt7988-uart", "mediatek,mt6577-uart";
 			reg = <0 0x11000200 0 0x100>;
 			interrupts = <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>;
