From edc7cb910433e05eac61b13d94163f1e07fa6af4 Mon Sep 17 00:00:00 2001
From: Dim Fish <dimfish@gmail.com>
Date: Thu, 3 Jul 2025 18:06:18 +0300
Subject: [PATCH] mediatek: spinand: force update_cache_variants to use reset for Foresee NAND

Force update_cache_variantsvariants to use reset for Foresee NAND with bad blocks.

Tested on Xiaomi AX3000T + F35SQA001G with bad blocks and without bad blocks

Signed-off-by: Dim Fish <dimfish@gmail.com>
Link: https://github.com/openwrt/openwrt/pull/17963
Signed-off-by: Chuanhong Guo <gch981213@gmail.com>
---
Force update_cache_variants to use reset for Foresee NAND with bad blocks

Tested on Xiaomi AX3000T + F35SQA001G with bad blocks and without bad blocks

Signed-off-by: Dim Fish <dimfish@gmail.com>

--- a/drivers/mtd/nand/spi/foresee.c
+++ b/drivers/mtd/nand/spi/foresee.c
@@ -22,8 +22,8 @@ static SPINAND_OP_VARIANTS(write_cache_v
 		SPINAND_PROG_LOAD_1S_1S_1S_OP(true, 0, NULL, 0));
 
 static SPINAND_OP_VARIANTS(update_cache_variants,
-		SPINAND_PROG_LOAD_1S_1S_4S_OP(false, 0, NULL, 0),
-		SPINAND_PROG_LOAD_1S_1S_1S_OP(false, 0, NULL, 0));
+		SPINAND_PROG_LOAD_1S_1S_4S_OP(true, 0, NULL, 0),
+		SPINAND_PROG_LOAD_1S_1S_1S_OP(true, 0, NULL, 0));
 
 static int f35sqa002g_ooblayout_ecc(struct mtd_info *mtd, int section,
 				    struct mtd_oob_region *region)
