// SPDX-License-Identifier: GPL-2.0-only OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "Aruba AP-303H";
	compatible = "aruba,ap-303h";

	aliases {
		led-boot = &led_system_green;
		led-failsafe = &led_system_red;
		led-running = &led_system_green;
		led-upgrade = &led_system_amber;
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x10000000>;
	};

	soc {
		counter@4a1000 {
			compatible = "qcom,qca-gcnt";
			reg = <0x4a1000 0x4>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};

	leds {
		compatible = "gpio-leds";

		wifi_green {
			label = "green:wifi";
			gpios = <&tlmm 27 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};

		wifi_amber {
			label = "amber:wifi";
			gpios = <&tlmm 28 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1tpt";
		};

		pse {
			label = "green:pse";
			gpios = <&tlmm 42 GPIO_ACTIVE_HIGH>;
		};

		led_system_red: system_red {
			label = "red:system";
			gpios = <&tlmm 25 GPIO_ACTIVE_HIGH>;
		};

		led_system_green: system_green {
			label = "green:system";
			gpios = <&tlmm 24 GPIO_ACTIVE_HIGH>;
		};

		led_system_amber: system_amber {
			label = "amber:system";
			gpios = <&tlmm 26 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&watchdog {
	status = "okay";
};

&prng {
	status = "okay";
};

&crypto {
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_0_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&blsp1_uart2 {
	/* Texas Instruments CC2540T BLE radio */
	pinctrl-0 = <&serial_1_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&tlmm {
	/*
	 * In addition to the Pins listed below,
	 * the following GPIOs have "features":
	 * 39 - out - active low to force HW reset
	 * 32 - out - active low to reset TPM
	 * 43 - out - active low to reset BLE radio
	 * 41 - out - pulse to set warm reset status
	 * 34 - out - active low to enable PSE port
	 * 22 - in  - active low when 802.3at powered
	 * 29 - in  - active high when DC powered
	 * 40 - in  - active low when reset due to cold HW reset
	 * 30 - in  - active low when USB overcurrent detected
	 * 35 - in  - interrupt line for power monitor chip
	 * 31 - in  - active low when PSE port active
	 */
	mdio_pins: mdio_pinmux {
		mux_1 {
			pins = "gpio6";
			function = "mdio";
			bias-pull-up;
		};
		mux_2 {
			pins = "gpio7";
			function = "mdc";
			bias-pull-up;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pin {
			function = "blsp_spi0";
			pins = "gpio13", "gpio14", "gpio15";
			drive-strength = <12>;
			bias-disable;
		};
		pin_cs {
			function = "gpio";
			pins = "gpio12", "gpio59";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};

	i2c_0_pins: i2c_0_pinmux {
		mux {
			pins = "gpio20", "gpio21";
			function = "blsp_i2c0";
			drive-strength = <4>;
			bias-pull-up;
		};
	};

	serial_0_pins: serial_0_pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	serial_1_pins: serial_1_pinmux {
		mux {
			pins = "gpio8", "gpio9";
			function = "blsp_uart1";
			bias-disable;
		};
	};

	usb-power {
		line-name = "USB-power";
		gpios = <23 GPIO_ACTIVE_HIGH>;
		gpio-hog;
		output-high;
	};
};

&blsp1_i2c3 {
	pinctrl-0 = <&i2c_0_pins>;
	pinctrl-names = "default";
	status = "okay";
	clock-frequency = <400000>;

	tpm@29 {
		/* No Driver */
		compatible = "atmel,at97sc3203";
		reg = <0x29>;
		read-only;
	};

	power-monitor@40 {
		/* No driver */
		/* Device also replies on address 0x3f, see   */
		/* ISL28022 datasheet, "Broadcast Addressing" */
		compatible = "isl,isl28022";
		reg = <0x40>;
	};
};

&blsp1_spi1 {
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";
	cs-gpios = <&tlmm 12 GPIO_ACTIVE_LOW>, <&tlmm 59 GPIO_ACTIVE_LOW>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			/*
			 * There is no partition map for the NOR flash
			 * in the stock firmware.
			 *
			 * All partitions here are based on offsets
			 * found in the U-Boot GPL code and information
			 * from smem.
			 */

			partition@0 {
				label = "sbl1";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "mibib";
				reg = <0x40000 0x20000>;
				read-only;
			};

			partition@60000 {
				label = "qsee";
				reg = <0x60000 0x60000>;
				read-only;
			};

			partition@c0000 {
				label = "cdt";
				reg = <0xc0000 0x10000>;
				read-only;
			};

			partition@d0000 {
				label = "ddrparams";
				reg = <0xd0000 0x10000>;
				read-only;
			};

			partition@e0000 {
				label = "appsblenv";
				reg = <0xe0000 0x10000>;
				read-only;
			};

			partition@f0000 {
				label = "appsbl";
				reg = <0xf0000 0x100000>;
				read-only;
			};

			partition@1e0000 {
				label = "ART";
				reg = <0x1f0000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_art_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_art_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};

			partition@1f0000 {
				label = "osss";
				reg = <0x200000 0x170000>;
				read-only;
			};

			partition@200000 {
				label = "pds";
				reg = <0x370000 0x10000>;
				read-only;
			};

			partition@380000 {
				label = "apcd";
				reg = <0x380000 0x10000>;
				read-only;
			};

			partition@390000 {
				label = "mfginfo";
				reg = <0x390000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_mfginfo_1d: macaddr@1d {
						compatible = "mac-base";
						reg = <0x1d 0x6>;
						#nvmem-cell-cells = <1>;
					};

					macaddr_mfginfo_45: macaddr@45 {
						compatible = "mac-base";
						reg = <0x45 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@3a0000 {
				label = "fcache";
				reg = <0x3a0000 0x10000>;
				read-only;
			};

			partition@3b0000 {
				/* Called osss1 in smem */
				label = "u-boot-env-bak";
				reg = <0x3b0000 0x10000>;
				read-only;
			};

			partition@3f0000 {
				label = "u-boot-env";
				reg = <0x3c0000 0x40000>;
				read-only;
			};
		};
	};

	flash@1 {
		status = "okay";

		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				/* 'aos0' in Aruba firmware */
				label = "aos0";
				reg = <0x0 0x2000000>;
				read-only;
			};

			partition@2000000 {
				/* 'aos1' in Aruba firmware */
				label = "ubi";
				reg = <0x2000000 0x2000000>;
			};

			partition@4000000 {
				label = "aruba-ubifs";
				reg = <0x4000000 0x4000000>;
				read-only;
			};
		};
	};
};

&usb3 {
	status = "okay";
};

&usb3_dwc {
	phys = <&usb3_hs_phy>;
	phy-names = "usb2-phy";
};

&usb3_hs_phy {
	status = "okay";
};

&mdio {
	status = "okay";
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";

	reset-gpios = <&tlmm 19 GPIO_ACTIVE_LOW>;
	reset-delay-us = <2000>;
};

&gmac {
	status = "okay";

	nvmem-cell-names = "mac-address";
	nvmem-cells = <&macaddr_mfginfo_1d 1>;
};

&switch {
	status = "okay";
};

&swport2 {
	status = "okay";

	label = "lan1";
};

&swport3 {
	status = "okay";

	label = "lan2";
};

&swport4 {
	status = "okay";

	label = "lan3";
};

&swport5 {
	status = "okay";

	label = "wan";
	nvmem-cell-names = "mac-address";
	nvmem-cells = <&macaddr_mfginfo_1d 0>;
};

&wifi0 {
	status = "okay";
	nvmem-cell-names = "pre-calibration", "mac-address";
	nvmem-cells = <&precal_art_1000>, <&macaddr_mfginfo_45 0>;
	qcom,ath10k-calibration-variant = "Aruba-AP-303";
};

&wifi1 {
	status = "okay";
	nvmem-cell-names = "pre-calibration", "mac-address";
	nvmem-cells = <&precal_art_5000>, <&macaddr_mfginfo_45 1>;
	qcom,ath10k-calibration-variant = "Aruba-AP-303";
};
