// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x_senao_loader.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "araknis,an-500-ap-i-ac", "qca,qca9557";
	model = "Araknis AN-500-AP-I-AC";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			default-state = "off";
		};

		wifi5g {
			label = "blue:wifi5g";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wps {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
	};
};

&partitions {
	partition@ff0000 {
		label = "art";
		reg = <0xff0000 0x010000>;
		read-only;

		nvmem-layout {
			compatible = "fixed-layout";
			#address-cells = <1>;
			#size-cells = <1>;

			macaddr_art_0: macaddr@0 {
				compatible = "mac-base";
				reg = <0x0 0x6>;
				#nvmem-cell-cells = <1>;
			};

			cal_art_1000: calibration@1000 {
				reg = <0x1000 0x440>;
			};

			cal_art_5000: calibration@5000 {
				reg = <0x5000 0x844>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy5: ethernet-phy@5 {
		reg = <5>;
		eee-broken-100tx;
		eee-broken-1000t;
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0 0>;
	nvmem-cell-names = "mac-address";

	phy-handle = <&phy5>;
	phy-mode = "rgmii-id";

	pll-data = <0x82000000 0x80000101 0x80001313>;
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_art_0 1>, <&cal_art_1000>;
	nvmem-cell-names = "mac-address", "calibration";

	led {
		led-sources = <13>;
		led-active-low;
	};
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&cal_art_5000>, <&macaddr_art_0 2>;
		nvmem-cell-names = "calibration", "mac-address";
	};
};
