From 28702a215c96917d85558ad6309a57ab224808c0 Mon Sep 17 00:00:00 2001
From: Mieczyslaw Nalewaj <namiltd@yahoo.com>
Date: Sat, 9 May 2026 14:10:29 +0200
Subject: net: dsa: realtek: rtl8365mb: add support for RTL8367SB

Add chip info entry for the Realtek RTL8367SB switch. This device has
chip ID 0x6367 and version 0x0010. It exposes two external interfaces:
port 6 supports MII, TMII, RMII, RGMII, SGMII and HSGMII, while port 7
supports MII, TMII, RMII and RGMII. Use the existing 8365MB-VC jam table
for initialization.

Reviewed-by: Luiz Angelo Daros de Luca <luizluca@gmail.com>
Signed-off-by: Mieczyslaw Nalewaj <namiltd@yahoo.com>
Link: https://patch.msgid.link/3c6d822b-0e85-4173-86ba-2badb140bbf1@yahoo.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/realtek/rtl8365mb.c | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

--- a/drivers/net/dsa/realtek/rtl8365mb.c
+++ b/drivers/net/dsa/realtek/rtl8365mb.c
@@ -545,6 +545,20 @@ static const struct rtl8365mb_chip_info
 		.jam_size = ARRAY_SIZE(rtl8365mb_init_jam_8365mb_vc),
 	},
 	{
+		.name = "RTL8367SB",
+		.chip_id = 0x6367,
+		.chip_ver = 0x0010,
+		.extints = {
+			{ 6, 1, PHY_INTF(MII) | PHY_INTF(TMII) |
+				PHY_INTF(RMII) | PHY_INTF(RGMII) |
+				PHY_INTF(SGMII) | PHY_INTF(HSGMII) },
+			{ 7, 2, PHY_INTF(MII) | PHY_INTF(TMII) |
+				PHY_INTF(RMII) | PHY_INTF(RGMII) },
+		},
+		.jam_table = rtl8365mb_init_jam_8365mb_vc,
+		.jam_size = ARRAY_SIZE(rtl8365mb_init_jam_8365mb_vc),
+	},
+	{
 		.name = "RTL8367RB-VB",
 		.chip_id = 0x6367,
 		.chip_ver = 0x0020,
