From: Chuanhong Guo <gch981213@gmail.com>
Date: Tue, 20 Aug 2024 08:33:43 +0800
Subject: [PATCH 06/20] reset: add support for sf19a2890

Signed-off-by: Chuanhong Guo <gch981213@gmail.com>
---
 drivers/reset/Kconfig  | 8 ++++++++
 drivers/reset/Makefile | 1 +
 2 files changed, 9 insertions(+)

--- a/drivers/reset/Kconfig
+++ b/drivers/reset/Kconfig
@@ -242,6 +242,14 @@ config RESET_SCMI
 	  This driver uses SCMI Message Protocol to interact with the
 	  firmware controlling all the reset signals.
 
+config RESET_SF19A2890_PERIPH
+	bool "Siflower SF19A2890 Peripheral Reset Controller Driver"
+	default MACH_SIFLOWER_MIPS
+	depends on HAS_IOMEM
+	help
+	  This enables reset controller driver for peripheral reset blocks
+	  found on Siflower SF19A2890 SoC.
+
 config RESET_SIMPLE
 	bool "Simple Reset Controller Driver" if COMPILE_TEST || EXPERT
 	default ARCH_ASPEED || ARCH_BCMBCA || ARCH_BITMAIN || ARCH_REALTEK || ARCH_SOPHGO || ARCH_STM32 || (ARCH_INTEL_SOCFPGA && ARM64) || ARCH_SUNXI || ARC
--- a/drivers/reset/Makefile
+++ b/drivers/reset/Makefile
@@ -32,6 +32,7 @@ obj-$(CONFIG_RESET_QCOM_PDC) += reset-qc
 obj-$(CONFIG_RESET_RASPBERRYPI) += reset-raspberrypi.o
 obj-$(CONFIG_RESET_RZG2L_USBPHY_CTRL) += reset-rzg2l-usbphy-ctrl.o
 obj-$(CONFIG_RESET_SCMI) += reset-scmi.o
+obj-$(CONFIG_RESET_SF19A2890_PERIPH) += reset-sf19a2890-periph.o
 obj-$(CONFIG_RESET_SIMPLE) += reset-simple.o
 obj-$(CONFIG_RESET_SOCFPGA) += reset-socfpga.o
 obj-$(CONFIG_RESET_SUNPLUS) += reset-sunplus.o
