--- a/arch/arm64/boot/dts/rockchip/rk3568-rock-3b.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-rock-3b.dts
@@ -18,6 +18,10 @@
 		mmc0 = &sdhci;
 		mmc1 = &sdmmc0;
 		mmc2 = &sdmmc2;
+		led-boot = &led_green;
+		led-failsafe = &led_green;
+		led-running = &led_green;
+		led-upgrade = &led_green;
 	};
 
 	chosen {
@@ -47,12 +51,11 @@
 		pinctrl-names = "default";
 		pinctrl-0 = <&led>;
 
-		led-0 {
+		led_green: led-0 {
 			color = <LED_COLOR_ID_GREEN>;
 			default-state = "on";
 			function = LED_FUNCTION_HEARTBEAT;
 			gpios = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "heartbeat";
 		};
 	};
 
