// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "zyxel,nr7101", "mediatek,mt7621-soc";
	model = "Zyxel NR7101";

	aliases {
		led-boot = &led_system_green;
		led-failsafe = &led_system_green;
		led-running = &led_system_green;
		led-upgrade = &led_system_green;
		label-mac-device = &gmac0;
	};

	leds {
		compatible = "gpio-leds";

		system_yellow {
			label = "yellow:system";
			gpios = <&gpio 13 GPIO_ACTIVE_HIGH>;
		};

		led_system_green: system_green {
			label = "green:system";
			gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		};

		system_red {
			label = "red:system";
			gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wlan";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WLAN>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&gpio {
	lte_pwrkey {
		gpio-hog;
		gpios = <4 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "lte-pwrkey";
	};

	lte_power {
		gpio-hog;
		gpios = <18 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "lte-power";
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "Bootloader";
			reg = <0x0 0x80000>;
			read-only;
		};

		partition@80000 {
			label = "Config";
			reg = <0x80000 0x80000>;
		};

		partition@100000 {
			label = "Factory";
			reg = <0x100000 0x40000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				eeprom_factory_0: eeprom@0 {
					reg = <0x0 0x400>;
				};

				macaddr_factory_e000: macaddr@e000 {
					reg = <0xe000 0x6>;
				};
			};
		};

		partition@140000 {
			label = "Kernel";
			reg = <0x140000 0x1ec0000>;
		};

		partition@540000 {
			label = "ubi";
			reg = <0x540000 0x1ac0000>;
		};

		partition@2140000 {
			label = "Kernel2";
			reg = <0x2140000 0x1ec0000>;
		};

		partition@4000000 {
			label = "wwan";
			reg = <0x4000000 0x100000>;
		};

		partition@4100000 {
			label = "data";
			reg = <0x4100000 0x1000000>;
		};

		partition@5100000 {
			label = "rom-d";
			reg = <0x5100000 0x100000>;
			read-only;
		};

		partition@5200000 {
			label = "reserve";
			reg = <0x5200000 0x80000>;
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>;
		nvmem-cell-names = "eeprom";
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_e000>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	ports {
		port@2 {
			status = "okay";
			label = "lan";
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "uart3", "jtag", "wdt";
		function = "gpio";
	};
};
