From 39e4189d9d63a0b6fc15458ce0136e99ecdfb1b8 Mon Sep 17 00:00:00 2001
From: Frieder Schrempf <frieder.schrempf@kontron.de>
Date: Wed, 18 Dec 2024 16:27:32 +0100
Subject: arm64: dts: imx8mp-kontron: Add support for reading SD_VSEL signal

This fixes the LDO5 regulator handling of the pca9450 driver by
taking the status of the SD_VSEL into account to determine which
configuration register is used for the voltage setting.

Even without this change there is no functional issue, as the code
for switching the voltage in sdhci.c currently switches both, the
VSELECT/SD_VSEL signal and the regulator voltage at the same time
and doesn't run into an invalid corner case.

We should still make sure, that we always use the correct register
when controlling the regulator. At least in U-Boot this fixes an
actual bug where the wrong IO voltage is used and it makes sure
that the correct voltage can be read from sysfs.

Signed-off-by: Frieder Schrempf <frieder.schrempf@kontron.de>
Signed-off-by: Shawn Guo <shawnguo@kernel.org>
---
 arch/arm64/boot/dts/freescale/imx8mp-kontron-osm-s.dtsi | 7 ++++---
 1 file changed, 4 insertions(+), 3 deletions(-)

--- a/arch/arm64/boot/dts/freescale/imx8mp-kontron-osm-s.dtsi
+++ b/arch/arm64/boot/dts/freescale/imx8mp-kontron-osm-s.dtsi
@@ -311,6 +311,7 @@
 				regulator-name = "NVCC_SD (LDO5)";
 				regulator-min-microvolt = <1800000>;
 				regulator-max-microvolt = <3300000>;
+				sd-vsel-gpios = <&gpio1 4 GPIO_ACTIVE_HIGH>;
 			};
 		};
 	};
@@ -808,7 +809,7 @@
 			MX8MP_IOMUXC_SD2_DATA1__USDHC2_DATA1		0x1d0 /* SDIO_A_D1 */
 			MX8MP_IOMUXC_SD2_DATA2__USDHC2_DATA2		0x1d0 /* SDIO_A_D2 */
 			MX8MP_IOMUXC_SD2_DATA3__USDHC2_DATA3		0x1d0 /* SDIO_A_D3 */
-			MX8MP_IOMUXC_GPIO1_IO04__USDHC2_VSELECT		0x1d0
+			MX8MP_IOMUXC_GPIO1_IO04__USDHC2_VSELECT		0x400001d0
 		>;
 	};
 
@@ -820,7 +821,7 @@
 			MX8MP_IOMUXC_SD2_DATA1__USDHC2_DATA1		0x1d4 /* SDIO_A_D1 */
 			MX8MP_IOMUXC_SD2_DATA2__USDHC2_DATA2		0x1d4 /* SDIO_A_D2 */
 			MX8MP_IOMUXC_SD2_DATA3__USDHC2_DATA3		0x1d4 /* SDIO_A_D3 */
-			MX8MP_IOMUXC_GPIO1_IO04__USDHC2_VSELECT		0x1d0
+			MX8MP_IOMUXC_GPIO1_IO04__USDHC2_VSELECT		0x400001d0
 		>;
 	};
 
@@ -832,7 +833,7 @@
 			MX8MP_IOMUXC_SD2_DATA1__USDHC2_DATA1		0x1d6 /* SDIO_A_D1 */
 			MX8MP_IOMUXC_SD2_DATA2__USDHC2_DATA2		0x1d6 /* SDIO_A_D2 */
 			MX8MP_IOMUXC_SD2_DATA3__USDHC2_DATA3		0x1d6 /* SDIO_A_D3 */
-			MX8MP_IOMUXC_GPIO1_IO04__USDHC2_VSELECT		0x1d0
+			MX8MP_IOMUXC_GPIO1_IO04__USDHC2_VSELECT		0x400001d0
 		>;
 	};
 
