// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6358.dtsi"

/ {
	model = "Huawei EchoLife HG553";
	compatible = "huawei,hg553", "brcm,bcm6358";

	aliases {
		led-boot = &led_power_blue;
		led-failsafe = &led_power_red;
		led-running = &led_power_blue;
		led-upgrade = &led_power_blue;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		rfkill {
			label = "rfkill";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_blue: led-4 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		led_power_red: led-5 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		led-12 {
			label = "red:hspa";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		led-13 {
			label = "blue:hspa";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led-22 {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		led-23 {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		led-25 {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 25 GPIO_ACTIVE_LOW>;
		};

		led-34 {
			label = "red:dsl";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
		};

		led-35 {
			label = "blue:dsl";
			gpios = <&gpio 35 GPIO_ACTIVE_LOW>;
		};
	};

	bcm4318-sprom {
		compatible = "brcm,ssb-sprom";

		pci-bus = <0>;
		pci-dev = <1>;

		nvmem-cells = <&macaddr_cfe_6a0 1>;
		nvmem-cell-names = "mac-address";

		brcm,sprom = "brcm/bcm4318-sprom.bin";
	};
};

&ehci {
	status = "okay";
};

&ethernet1 {
	status = "okay";

	nvmem-cells = <&macaddr_cfe_6a0 0>;
	nvmem-cell-names = "mac-address";

	phy-mode = "mii";

	fixed-link {
		speed = <100>;
		full-duplex;
	};
};

&iudma {
	status = "okay";
};

&mdio1 {
	switch@1e {
		compatible = "brcm,bcm5325";
		reg = <30>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "lan1";

				phy-mode = "mii";
			};

			port@1 {
				reg = <1>;
				label = "lan2";

				phy-mode = "mii";
			};

			port@2 {
				reg = <2>;
				label = "lan3";

				phy-mode = "mii";
			};

			port@3 {
				reg = <3>;
				label = "lan4";

				phy-mode = "mii";
			};

			port@5 {
				reg = <5>;
				label = "cpu";

				phy-mode = "internal";
				ethernet = <&ethernet1>;

				fixed-link {
					speed = <100>;
					full-duplex;
				};
			};
		};
	};
};

&ohci {
	status = "okay";
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "cfe";
			reg = <0x000000 0x020000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_cfe_6a0: macaddr@6a0 {
					compatible = "mac-base";
					reg = <0x6a0 0x6>;
					#nvmem-cell-cells = <1>;
				};
			};
		};

		partition@20000 {
			label = "firmware";
			reg = <0x020000 0xfc0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		partition@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};
