// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/leds/common.h>

#include "qca955x_senao_router-dual.dtsi"

/ {
	compatible = "engenius,esr1750", "qca,qca9558";
	model = "EnGenius ESR1750";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g {
			label = "blue:wlan2g";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "blue:wlan5g";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wps_amber {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		wps_blue {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
	};
};

&phy0 {
	qca,mib-poll-interval = <500>;

	qca,ar8327-initvals = <
		0x04 0x87680000 /* PORT0 PAD MODE CTRL */
		0x10 0x40000000 /* POWER_ON_STRAP */
		0x50 0xcf35cf35 /* LED_CTRL0 */
		0x54 0xcf35cf35 /* LED_CTRL1 */
		0x58 0xcf35cf35 /* LED_CTRL2 */
		0x5c 0x03ffff00 /* LED_CTRL3 */
		0x7c 0x0000007e /* PORT0_STATUS */
	>;
};

&usb_phy1 {
	status = "okay";
};

&usb1 {
	status = "okay";
};

&nvmem {
	calibration_art_5000: calibration@5000 {
		reg = <0x5000 0x844>;
	};
};

&wmac {
	nvmem-cells = <&calibration_art_1000>, <&macaddr_uboot_eth 1>;
	nvmem-cell-names = "calibration", "mac-address";
};

&wifi0 {
	compatible = "qcom,ath10k";

	nvmem-cells = <&calibration_art_5000>, <&macaddr_uboot_eth 0>;
	nvmem-cell-names = "calibration", "mac-address";
};
