// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "tplink,tl-wa1201-v2", "qca,qca9563";
	model = "TP-Link TL-WA1201 v2";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		mdio-gpio0 = &mdio2;
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g {
			label = "green:wlan2g";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "green:wlan5g";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		lan {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	mdio2: mdio {
		compatible = "virtual,mdio-gpio";

		#address-cells = <1>;
		#size-cells = <0>;

		gpios = <&gpio 3 GPIO_ACTIVE_HIGH>, /* MDC */
			<&gpio 4 GPIO_ACTIVE_HIGH>; /* MDIO */

		phy4: ethernet-phy@4 {
			reg = <4>;

			eee-broken-100tx;
			eee-broken-1000t;
		};
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&precal_art_5000>, <&macaddr_info_8 (-1)>;
		nvmem-cell-names = "pre-calibration", "mac-address";
		qcom,ath10k-calibration-variant = "TP-Link-TL-WA1201-v2";
	};
};

&eth0 {
	status = "okay";

	phy-mode = "sgmii";
	phy-handle = <&phy4>;

	nvmem-cells = <&macaddr_info_8 0>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_info_8 0>, <&cal_art_1000>;
	nvmem-cell-names = "mac-address", "calibration";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "info";
				reg = <0x020000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_info_8: macaddr@8 {
						compatible = "mac-base";
						reg = <0x8 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@30000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x030000 0xce0000>;
			};

			partition@d10000 {
				label = "tplink";
				reg = <0xd10000 0x2e0000>;
				read-only;
			};

			partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					cal_art_1000: calibration@1000 {
						reg = <0x1000 0x440>;
					};

					precal_art_5000: pre-calibration@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};
		};
	};
};
