From 8faac4ef6206a1c771e1c016e205dcee8164d618 Mon Sep 17 00:00:00 2001
From: Jianwei Zheng <jianwei.zheng@rock-chips.com>
Date: Wed, 23 Jul 2025 12:23:03 +0000
Subject: [PATCH] phy: rockchip: inno-usb2: Add support for RK3528

The RK3528 has a single USB2PHY with a otg and host port.

Add support for the RK3528 variant of USB2PHY.

PHY tuning for RK3528:

- Turn off differential receiver in suspend mode to save power
  consumption.

- Set HS eye-height to 400mV instead of default 450mV.

- Choose the Tx fs/ls data as linestate from TX driver for otg port
  which uses dwc3 controller to improve fs/ls devices compatibility with
  long cables.

This is based on vendor kernel linux-stan-6.1-rkr5 tag.

Signed-off-by: Jianwei Zheng <jianwei.zheng@rock-chips.com>
Signed-off-by: Jonas Karlman <jonas@kwiboo.se>
---
 drivers/phy/rockchip/phy-rockchip-inno-usb2.c | 74 +++++++++++++++++++
 1 file changed, 74 insertions(+)

--- a/drivers/phy/rockchip/phy-rockchip-inno-usb2.c
+++ b/drivers/phy/rockchip/phy-rockchip-inno-usb2.c
@@ -1612,6 +1612,28 @@ static int rk3128_usb2phy_tuning(struct
 				BIT(2) << BIT_WRITEABLE_SHIFT | 0);
 }
 
+static int rk3528_usb2phy_tuning(struct rockchip_usb2phy *rphy)
+{
+	int ret = 0;
+
+	/* Turn off otg port differential receiver in suspend mode */
+	ret |= regmap_write(rphy->phy_base, 0x30, BIT(18) | 0x0000);
+
+	/* Turn off host port differential receiver in suspend mode */
+	ret |= regmap_write(rphy->phy_base, 0x430, BIT(18) | 0x0000);
+
+	/* Set otg port HS eye height to 400mv (default is 450mv) */
+	ret |= regmap_write(rphy->phy_base, 0x30, GENMASK(22, 20) | 0x0000);
+
+	/* Set host port HS eye height to 400mv (default is 450mv) */
+	ret |= regmap_write(rphy->phy_base, 0x430, GENMASK(22, 20) | 0x0000);
+
+	/* Choose the Tx fs/ls data as linestate from TX driver for otg port */
+	ret |= regmap_write(rphy->phy_base, 0x94, GENMASK(22, 19) | 0x0018);
+
+	return ret;
+}
+
 static int rk3576_usb2phy_tuning(struct rockchip_usb2phy *rphy)
 {
 	int ret;
@@ -1994,6 +2016,57 @@ static const struct rockchip_usb2phy_cfg
 	{ /* sentinel */ }
 };
 
+static const struct rockchip_usb2phy_cfg rk3528_phy_cfgs[] = {
+	{
+		.reg = 0xffdf0000,
+		.num_ports	= 2,
+		.phy_tuning	= rk3528_usb2phy_tuning,
+		.clkout_ctl_phy	= { 0x041c, 7, 2, 0, 0x27 },
+		.port_cfgs	= {
+			[USB2PHY_PORT_OTG] = {
+				.phy_sus	= { 0x004c, 8, 0, 0, 0x1d1 },
+				.bvalid_det_en	= { 0x0074, 3, 2, 0, 3 },
+				.bvalid_det_st	= { 0x0078, 3, 2, 0, 3 },
+				.bvalid_det_clr	= { 0x007c, 3, 2, 0, 3 },
+				.idfall_det_en	= { 0x0074, 5, 5, 0, 1 },
+				.idfall_det_st	= { 0x0078, 5, 5, 0, 1 },
+				.idfall_det_clr	= { 0x007c, 5, 5, 0, 1 },
+				.idrise_det_en	= { 0x0074, 4, 4, 0, 1 },
+				.idrise_det_st	= { 0x0078, 4, 4, 0, 1 },
+				.idrise_det_clr	= { 0x007c, 4, 4, 0, 1 },
+				.ls_det_en	= { 0x0074, 0, 0, 0, 1 },
+				.ls_det_st	= { 0x0078, 0, 0, 0, 1 },
+				.ls_det_clr	= { 0x007c, 0, 0, 0, 1 },
+				.utmi_avalid	= { 0x006c, 1, 1, 0, 1 },
+				.utmi_bvalid	= { 0x006c, 0, 0, 0, 1 },
+				.utmi_id	= { 0x006c, 6, 6, 0, 1 },
+				.utmi_ls	= { 0x006c, 5, 4, 0, 1 },
+			},
+			[USB2PHY_PORT_HOST] = {
+				.phy_sus	= { 0x005c, 8, 0, 0x1d2, 0x1d1 },
+				.ls_det_en	= { 0x0090, 0, 0, 0, 1 },
+				.ls_det_st	= { 0x0094, 0, 0, 0, 1 },
+				.ls_det_clr	= { 0x0098, 0, 0, 0, 1 },
+				.utmi_ls	= { 0x006c, 13, 12, 0, 1 },
+				.utmi_hstdet	= { 0x006c, 15, 15, 0, 1 },
+			}
+		},
+		.chg_det = {
+			.opmode		= { 0x004c, 3, 0, 5, 1 },
+			.cp_det		= { 0x006c, 19, 19, 0, 1 },
+			.dcp_det	= { 0x006c, 18, 18, 0, 1 },
+			.dp_det		= { 0x006c, 20, 20, 0, 1 },
+			.idm_sink_en	= { 0x0058, 1, 1, 0, 1 },
+			.idp_sink_en	= { 0x0058, 0, 0, 0, 1 },
+			.idp_src_en	= { 0x0058, 2, 2, 0, 1 },
+			.rdm_pdwn_en	= { 0x0058, 3, 3, 0, 1 },
+			.vdm_src_en	= { 0x0058, 5, 5, 0, 1 },
+			.vdp_src_en	= { 0x0058, 4, 4, 0, 1 },
+		},
+	},
+	{ /* sentinel */ }
+};
+
 static const struct rockchip_usb2phy_cfg rk3568_phy_cfgs[] = {
 	{
 		.reg = 0xfe8a0000,
@@ -2316,6 +2389,7 @@ static const struct of_device_id rockchi
 	{ .compatible = "rockchip,rk3328-usb2phy", .data = &rk3328_phy_cfgs },
 	{ .compatible = "rockchip,rk3366-usb2phy", .data = &rk3366_phy_cfgs },
 	{ .compatible = "rockchip,rk3399-usb2phy", .data = &rk3399_phy_cfgs },
+	{ .compatible = "rockchip,rk3528-usb2phy", .data = &rk3528_phy_cfgs },
 	{ .compatible = "rockchip,rk3568-usb2phy", .data = &rk3568_phy_cfgs },
 	{ .compatible = "rockchip,rk3576-usb2phy", .data = &rk3576_phy_cfgs },
 	{ .compatible = "rockchip,rk3588-usb2phy", .data = &rk3588_phy_cfgs },
